## ASxxxx Cross Assembler Updates

    New Release:

            ASxxxx Cross Assemblers, Version 2.20, July 1999

            Header files now include function prototypes.

    Addition of options:

               The  -o/-v  options  allow the simple creation of loadable or
            overlay modules.  Loadable and overlay modules normally need  to
            be  linked  with  a  main module(s) to resolve external symbols.
            The -o/-v options can be used to enable object  output  for  the
            loadable  or overlay module(s) and suppress the object code from
            the linked main module(s).  The -o/-v  options  can  be  applied
            repeatedly  to specify a single linked file, groups of files, or
            libraries for object code inclusion or suppression.

    Previous Releases:

            ASxxxx Cross Assemblers, Version 2.10, April 1999

    Supported Microprocessors:

            6800(6802/6808)         68HC11
            6801(hd6803)            68HC16
            6804                    8051
            6805                    8085(8080)
            68HC08                  Z80(hd64180)
            6809                    H8/3xx
            68HC12                  6500 family

    New Features:

            All ASlink commands may now be entered on the
    	command line.  (Useful for makefiles ...)

            Directory Path fixes for ASxxxx and ASlink.

    	Many changes for increased portability to
    	GCC compilers in Linux and DJGPP.

    	Fix for Divide by 0 and Modulus by 0 errors.

            Long Names (79 significant characters)

            Assembler and Linker are Case Insensitive by default.
            Case Sensitivity option enabled with the -z switch.

            Assembler long name SYMBOL TABLE format with -w switch.
    	Linker long name MAP format with -w switch.

... Home Page