## AS6812 Assembler

####

    68HC12 REGISTER SET

    The following is a list of the 68HC12 registers used by AS6812:

            a,b     -       8-bit accumulators
            d       -       16-bit accumulator <a:b>
            x,y     -       index registers
            sp,s    -       stack pointer
            pc      -       program counter
            ccr,cc  -       condition code register

    68HC12 INSTRUCTION SET

       The  following tables list all 68HC12 mnemonics recognized by
    the AS6812 assembler.  The designation [] refers to  a  required
    addressing  mode  argument.   The  following  list specifies the
    format for each addressing mode supported by AS6812:

            #data           immediate data
                            byte or word data

            ext             extended addressing

            pg              memory page number

            *dir            direct page addressing
                            (see .setdp directive)
                            0 <= dir <= 255

            label           branch label

            r,r1,r2         registers
                            ccr,a,b,d,x,y,sp,pc

            -x      x-      register indexed, pre or
            ,-x     ,x-     post autodecrement by 1

            n,-x    n,x-    register indexed, pre or
                            post autodecrement by 1 - 8

            +x      x+      register indexed, pre or
            ,+x     ,x+     post autoincrement by 1

            n,+x    n,x+    register indexed, pre or
                            post autoincrement by 1 - 8

            offset,x        register indexed addressing
                               -16 <= offset <= 15    ---  5-bit
                              -256 <= offset <= -17   ---  9-bit
                                16 <= offset <= 255   ---  9-bit
                            -32768 <= offset <= -257  --- 16-bit
                               256 <= offset <= 32767 --- 16-bit
                            (external definition of offset
                             uses 16-bit mode)

            [offset,x]      register indexed indirect addressing
                            -32768 <= offset <= 32767 --- 16-bit

            [,x]            register indexed indirect addressing
                            zero offset

            a,x             accumulator offset indexed addressing

            [d,x]           d accumulator offset indexed
                            indirect addressing

    The  terms  data, dir, label, offset, and ext may all be expres-
    sions.

       Note  that  not all addressing modes are valid with every in-
    struction, refer to the 68HC12 technical data for valid modes.

    Inherent Instructions

            aba             bgnd            cba
            daa             dex             dey
            ediv            edivs           emul
            emuls           fdiv            idiv
            idivs           inx             iny
            mem             mul             nop
            psha            pshb            pshc
            pshd            pshx            pshy
            pula            pulb            pulc
            puld            pulx            puly
            rev             revw            rtc
            rti             rts             sba
            stop            swi             tab
            tba             wai             wav
            wavr

    Short Branch Instructions

            bcc     label           bcs     label
            beq     label           bge     label
            bgt     label           bhi     label
            bhis    label           bhs     label
            ble     label           blo     label
            blos    label           bls     label
            blt     label           bmi     label
            bne     label           bpl     label
            bra     label           brn     label
            bvc     label           bvs     label
            bsr     label

    Long Branch Instructions

            lbcc    label           lbcs    label
            lbeq    label           lbge    label
            lbgt    label           lbhi    label
            lbhis   label           lbhs    label
            lble    label           lblo    label
            lblos   label           lbls    label
            lblt    label           lbmi    label
            lbne    label           lbpl    label
            lbra    label           lbrn    label
            lbvc    label           lbvs    label

    Branch on Decrement, Test, or Increment

            dbeq    r,label         dbne    r,label
            ibeq    r,label         ibne    r,label
            tbeq    r,label         tbne    r,label

    Bit Clear and Set Instructions

            bclr    [],#data
            bset    [],#data

    Branch on Bit Clear or Set

            brclr   [],#data,label
            brset   [],#data,label

    Single Operand Instructions

            asla            aslb
            asl     []

            asra            asrb
            asr     []

            clra            clrb
            clr     []

            coma            comb
            com     []

            deca            decb
            dec     []

            inca            incb
            inc     []

            lsla            lslb
            lsl     []

            lsra            lsrb
            lsr     []

            nega            negb
            neg     []

            rola            rolb
            rol     []

            rora            rorb
            ror     []

            tsta            tstb
            tst     []

    Double Operand Instructions

            adca    []              adcb    []

            adda    []              addb    []

            anda    []              andb    []

            bita    []              bitb    []

            cmpa    []              cmpb    []

            eora    []              eorb    []

            ldaa    []      <=>     lda     []

            ldab    []      <=>     ldb     []

            oraa    []      <=>     ora     []

            orab    []      <=>     orb     []

            sbca    []              sbcb    []

            staa    []      <=>     sta     []

            stab    []      <=>     stb     []

            suba    []              subb    []

    Move Instructions

            movb    [],[]           movw    [],[]

    D-register Instructions

            addd    []              subd    []
            cpd     []      <=>     cmpd    []
            ldd     []              std     []

    Index/Stack Register Instructions

            cps     []      <=>     cmps    []
            cpx     []      <=>     cmpx    []
            cpy     []      <=>     cmpy    []

            lds     []
            ldx     []              ldy     []

            leas    []
            leax    []              leay    []

            sts     []
            stx     []              sty     []

    Jump and Jump/Call to Subroutine Instructions

            call    [],pg
            jmp     []              jsr     []

    Other Special Instructions

            emacs   []
            emaxd   []              emaxm   []
            emind   []              eminm   []
            etbl    []
            maxa    []              maxm    []
            mina    []              minm    []
            tbl     []              trap    #data

    H.2.14  Register - Register Instructions

            exg     r1,r2           sex     r1,r2
            tfr     r1,r2

    Condition Code Register Instructions

            andcc   #data           orcc    #data

    M68HC11 Compatibility Mode Instructions

            abx             aby             clc
            cli             clv             des
            ins             sec             sei
            sev             tap             tpa
            tsx             tsy             txs
            tys             xgdx            xgdy

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page