## Assembly and Linking Example

####

      This section describes the assembly and linking of a moderately
    complex program.  (The project is a multi-channel high voltage
    control system for the stabilization of nuclear radiation detection
    equipment.)  The files may be found in the '/project/phs_4' directory.

      The project includes an 'optional' module that can be downloaded
    by the main project.  The 'optional' module is assembled from an
    independent file but must be linked with the main project files
    to resolve references external to the 'optional' module.

####

        ... Assembly
        ... Linking

        ... Go to Documentation Index

### ... Assembly

####

      the project files included twelve .asm modules and
    four .def include files:

            phs.asm                 system.def
            acia.asm                area.def
            acq.asm                 define.def
            hvctrl.asm              data.def
            termio.asm
            select.asm
            status.asm
            histos.asm
            help.asm
            aiconv.asm
            phsmon.asm
            phsopt.asm

      Each of the modules was assembled individually.  This was done
    by creating a command file containing the assembly command lines:

            as6809 -gloaxsff phs
            as6809 -gloaxsff acia
            as6809 -gloaxsff acq
            as6809 -gloaxsff hvctrl
            as6809 -gloaxsff termio
            as6809 -gloaxsff select
            as6809 -gloaxsff status
            as6809 -gloaxsff histos
            as6809 -gloaxsff help
            as6809 -gloaxsff aiconv
            as6809 -gloaxsff phsmon
            as6809 -gloaxsff phsopt

    the assembly process produced an object (.rel) file (-s), a listing
    (.lst) file (-l), and a symbol (.sym) file (-s) for each individual
    .asm file.  the assembly process made all undefined labels
    global (-g), all internal labels global (-a), the output in HEX
    format (-x), and the listing files to have relocations flagged (-ff).

##### => Section Index

### ... Linking

####

      The main program was linked using a file (PHS.LNK) containing the
    following command lines:

            -mxsu                          ; linker options
            phs                            ; output file name
            phs                            ; input file
            acia                           ; .
            acq                            ; .
            hvctrl                         ; .
            termio                         ; .
            select                         ; .
            status                         ; .
            histos                         ; .
            help                           ; .
            aiconv                         ; .
            phsmon                         ; input file
            -b WORKPG = 0x0F00             ; value definition
            -b BUFSAV = bufsav             ; .
            -b PGMSAV = pgmsav             ; .
            -b IRQVEC = irqvec             ; value definition
            -e                             ; end of file

    and was invoked by the command line:

            aslink -f phs

    The linking process produced a map (.map) file (-m) in HEX format (-x)
    and a Motorola (.s19) loader file (-s).  The -b options specify the
    memory addresses for certain program sections as defined in the
    assembled modules.  The file input was terminated by the -e option.

      The 'optional' loadable program was linked using a file (PHSOPT.LNK)
    containing the following command lines:

            -mxsu                          ; linker options
            phsopt                         ; output file name
            -v                             ; suppress linker output
            phs                            ; input file
            acia                           ; .
            acq                            ; .
            hvctrl                         ; .
            termio                         ; .
            select                         ; .
            status                         ; .
            histos                         ; .
            help                           ; .
            aiconv                         ; .
            phsmon                         ; input file
            -o                             ; enable linker output
            phsopt                         ; input file
            -b WORKPG = 0x0F00             ; value definition
            -b BUFSAV = bufsav             ; .
            -b PGMSAV = pgmsav             ; .
            -b IRQVEC = irqvec             ; value definition
            -e                             ; end of file

    and was invoked by the command line:

            aslink -f phsopt

    The linking process creates an overlay output file from the
    PHSOPT code using all the global symbols defined in the PHS
    files.  The order of the main project files MUST be identical
    to that in the main project .lnk file.

##### => Section Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: January 2006