## ASZ8 Assembler

####

    Z8 REGISTER SET

    The following is a list of the Z8 registers used by ASZ8:

            r0  ... r15     -        8-bit accumulators
            rr0 ... rr15    -       16-bit accumulators

    Z8 INSTRUCTION SET

         The  following  tables  list all Z8 mnemonics recognized by
    the ASZ8 assembler.  The designation [] refers to a required ad-
    dressing mode argument.  The following list specifies the format
    for each addressing mode supported by ASZ8:

            #data           immediate byte data

            addr            location/branch address

            r0  ... r15      8-bit registers

            rr0 ... rr15    16-bit registers

            @rn     or      register indirect addressing
            (rn)

            @rrn    or      register indirect addressing
            (rrn)

            @addr   or      indirect addressing
            (addr)

            offset(rn)      indexed register addressing

    The terms data, addr, and offset may all be expressions.

    The  designation  CC  refers  to a condition code argument.  The
    following table contains all the valid condition codes supported
    by ASZ8:

            f       Always False            -
            t       Always True             -
            c       Carry                   C=1
            nc      No Carry                C=0
            z       Zero                    Z=1
            nz      Non-Zero                Z=0
            pl      Plus                    S=0
            mi      Minus                   S=1
            ov      Overflow                V=1
            nov     No Overflow             V=0
            eq      Equal                   Z=1
            ne      Not Equal               Z=0
            ge      Greater Than or Equal   (S XOR V)=0
            lt      Less Than               (S XOR V)=1
            gt      Greater Than            (Z OR (S XOR V))=0
            le      Less Than or Equal      (Z OR (S XOR V))=1
            uge     Unsigned ge             C=0
            ult     Unsigned lt             C=1
            ugt     Unsigned gt             (C=0 AND Z=0)=1
            ule     Unsigned le             (C OR Z)=1

    Note that not all addressing modes are valid with every instruc-
    tion, refer to the Z8 technical data for valid modes.

    Load Instructions

            clr     []
            ld      [],[]           ldc     [],[]
            pop     []              push    []

    Arithmetic Instructions

            adc     [],[]           add     [],[]
            cp      [],[]           da      []
            dec     []              decw    []
            inc     []              incw    []
            sbc     [],[]           sub     [],[]

    Logical Instructions

            and     [],[]           com     []
            or      [],[]           xor     [],[]

    Program Control Instructions

            call    []              djnz    [],[]
            iret                    jp      CC,[]
            jr      CC,[]           ret

    Bit Manipulation Instructions

            tcm     [],[]           tm      [],[]
            and     [],[]           or      [],[]
            xor     [],[]

    Block Transfer Instructions

            ldci    [],[]

    Rotate and Shift Instructions

            rl      []              rlc     []
            rr      []              rrc     []
            sra     []              swap    []

    Cpu Control Instructions

            ccf
            di                      ei
            halt                    nop
            rcf                     scf
            srp     []
            stop                    wait

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: January 2006