## ASEZ80 Assembler

####

    PROCESSOR SPECIFIC DIRECTIVES

       The  ASEZ80 assembler is a port of the ASZ80 assembler.  This
    assembler can process EZ80 code in Z80 and ADL modes in any com-
    bination  within  the  source  file.   The  following  processor
    specific assembler directives specify which mode  the  assembler
    is  to  process  the assembler source code.  The default mode of
    the assembler is Z80.

    .z80 Directive

    Format:

            .z80    [n]

    The  assembler is informed by the .z80 directive to assemble the
    subsequent code using the banked 16-Bit addressing  capabilities
    of the EZ80 processor.  The optional argument, n, allows the as-
    sembly mode to be controlled by a varaible.   A  non-zero  value
    for  n  enables  Z80 mode and a zero value enables the ADL mode.
    The default mode of the assembler is Z80.

    .adl Directive

    Format:

            .adl    [n]

    The  assembler is informed by the .adl directive to assemble the
    subsequent code using the full 24-Bit addressing capabilities of
    the EZ80 processor.  The optional argument, n, allows the assem-
    bly mode to be controlled by a varaible.  A non-zero value for n
    enables  ADL  mode  and  a zero value enables the Z80 mode.  The
    default mode of the assembler is Z80.

    .msb Directive

    Format:

            .msb    n

       The  assembler operator '>' selects the upper byte (MSB) when
    included in an assembler instruction.  The normal assembler mode
    is  to select bits <15:8> as the MSB.  The .msb directive allows
    the programmer to specify a particular byte as  the  'MSB'  when
    the address space is larger than 16-bits.

       For a 24-bit EZ80 address the assembler directive .msb n con-
    figures the assembler to select a particular byte as MSB.  Given
    a  24-bit  address  of  Mmn (M is <23:16>, m is <15:8>, and n is
    <7:0>) the following examples show how to  select  a  particular
    address byte:

            .msb 1          ;select byte 1 of address
                            ;
            LD A,>Mmn       ;byte m <15:8> ==>> A
            ...

            .msb 2          ;select byte 2 of address
                            ;
            LD A,>Mmn       ;byte M <23:16> ==>> A
            LD MB,A         ;place in MBASE register

    EZ80 ADDRESSING AND INSTRUCTIONS

    Instruction Symbols

            b          Bit select
                            (000 = bit 0, 001 = bit 1,
                             010 = bit 2, 011 = bit 3,
                             100 = bit 4, 101 = bit 5,
                             110 = bit 6, 111 = bit 7)
            cc         condition code C, NC, Z, NZ, P, M, PE, PO
                       test of single bit in FLAGS register
            cc'        condition code C, NC, Z, NZ
                       test of single bit in FLAGS register
            d          an 8-bit two's complement displacement with
                       value from -128 to 127.
            I          Interrupt Page Address Register
            ir or ir'  8-bit CPU register IXH(IX:[15:8]),
                       IXL (IX:[7:0], IYH (IY:[15:8]), IYL (IY:[7:0])
            IX/Y       CPU register IX or IY
            (IX/Y+d)   A location in memory with address formed by the
                       sum of the contents of the Index Register, IX
                       or IY, and the two's complement displacement d.
            MB         Z80 Memory Mode Base Address Register
            Mmn        A 24-bit immediate data value
            (Mmn)      A 24-bit value indicating a location in
                       memory at this address.
            mn         A 16-bit immediate data value
            (mn)       A 16-bit value indicating a location in
                       memory at this address.
            n          8-bit immediate data value
            R          Refresh Counter Register
            r or r'    8-bit CPU register A, B, C, D, E, H, L
            rr         16 or 24-bit CPU register BC, DE, HL
            rxy        16 or 24-bit CPU register BC, DE, HL, IX, IY
            SP         Stack Pointer, Can indicate either the
                       StackPointer Short register (SPS) or the
                       StackPointer Long register (SPL).

            C  -    carry bit set
            NC -    carry bit clear
            Z  -    zero bit set
            NZ -    zero bit clear
            M  -    sign bit set
            P  -    sign bit clear
            PE -    parity even
            PO -    parity odd

            The terms b, d, Mmn, mn, and n may all be expressions.

    EZ80 Instructions

       The  following list of instructions (with explicit addressing
    modes) are available for the EZ80.

    -----------------------------------------------------------------------

            ADC A,(HL)              DEC (HL)                INI
            ADC A,ir                DEC ir                  INI2
            ADC A,(IX/Y+d)          DEC IX/Y                INI2R
            ADC A,n                 DEC (IX/Y+d)
            ADC A,r                 DEC r                   INIM
            ADC HL,rr               DEC rr                  INIMR
            ADC HL,SP               DEC SP
                                                            INIR
            ADD A,(HL)              DI                      INIRX
            ADD A,ir
            ADD A,(IX/Y+d)          DJNZ d                  JP cc,Mmn
            ADD A,n                                         JP HL
            ADD A,r                 EI                      JP IX/Y
            ADD HL,rr                                       JP Mmn
            ADD HL,SP               EX AF,AF'
            ADD IX/Y,rxy            EX DE,HL                JR cc',d
            ADD IX/Y,SP             EX (SP),HL              JR d
                                    EX (SP),IX/Y
            AND A,HL                                        LD A,I
            AND A,ir                EXX                     LD A,(IX/Y+d)
            AND A,(IX/Y+d)                                  LD A,MB
            AND A,n                 HALT                    LD A,(Mmn)
            AND A,r                                         LD A,R
                                    IM n                    LD A,(rr)
            BIT b,(HL)              IM A,(n)                LD (HL),IX/Y
            BIT b, (IX/Y+d)         IN r,(BC)               LD (HL),n
            BIT b,r                                         LD (HL),r
                                    IN0 r,(n)               LD (HL),rr
            CALL cc,Mmn                                     LD IY,(SP+n)
            CALL mn                 INC (HL)                LD I,HL
                                    INC ir                  LD I,A
            CP A,(HL)               INC IX/Y                LD ir,ir'
            CP A,ir                 INC (IX/Y+d)            LD ir,n
            CP A,(IX/Y+d)           INC r                   LD ir,r
            CP A,r                  INC SP                  LD IX/Y,(HL)
                                                            LD IX/Y,(IX/Y+d)
            CPD                     IND                     LD IX/Y,Mmn
            CPDR                    IND2                    LD IX/Y,(Mmn)
                                    IND2R                   LD (IX/Y+d),IX/Y
            CPI                                             LD (IX/Y+d),n
            CPIR                    INDM                    LD (IX/Y+d),r
                                    INDMR                   LD (IX/Y+d),rr
            CPL                                             LD MB,A
                                    INDR                    LD (Mmn),A
            DAA                     INDRX                   LD (Mmn),IX/Y

    -----------------------------------------------------------------------

            LD (Mmn),rr             OTDR                    RL r
            LD (Mmn),SP             OTDRX
            LD R,A                                          RLA
            LD r,(HL)               OTI2R
            LD r,ir                                         RLC (HL)
            LD r,(IX/Y+d)           OTIM                    RLC (IX/Y+d)
            LD r,n                  OTIMR                   RLC r
            LD r,r'
            LD rr,(HL)              OTIR                    RLCA
            LD rr,(IX/Y+d)          OTIRX
            LD rr,Mmn                                       RLD
            LD rr,(Mmn)             OUT (BC),r
            LD (rr),A               OUT (C),r               RR (HL)
            LD SP,HL                OUT (n),A               RR (IX/Y+d)
            LD SP,IX/Y                                      RR r
            LD SP,Mmn               OUTD
            LD SP,(Mmn)             OUTD2                   RRA

            LDD                     OUTI                    RRC (HL)
            LDDR                    OUTI2                   RRC (IX/Y+d)
                                    RL (IX+d)               RRC r
            LDI                     RL (IY+d
            LDIR                                            RRCA
                                    PEA IX+d
            LEA IX/Y,IX+d           PEA IY+d                RRD
            LEA IX/Y,IY+d
            LEA rr,IX+d             POP AF                  RSMIX
            LEA rr,IY+d             POP IX/Y
                                    POP rr                  RST n
            MLT rr
            MLT SP                  PUSH AF                 SBC A,(HL)
                                    PUSH IX/Y               SBC A,ir
            NEG                     PUSH rr                 SBC A,(IX/Y+d)
                                                            SBC A,n
            NOP                     RES b,(IX/Y+d)          SBC A,r
                                    RES b,r                 SBC HL,rr
            OR A,(HL)                                       SBC HL,SP
            OR A,ir                 RET
            OR A,(IX/Y+d)           RET cc                  SCF
            OR A,n
            OR A,r                  RETI                    SET b,(HL)
                                                            SET b,(IX/Y+d)
            OTD2R                   RETN                    SET b,r

            OTDM                    RL (HL)                 SLA (HL)
            OTDMR                   RL (IX/Y+d)             SLA (IX/Y+d)

    -----------------------------------------------------------------------

            SLA r                   STMIX                   TSTIO n

            SLP                     SUB A,(HL)              XOR A,(HL)
                                    SUB A,ir                XOR A,ir
            SRA (HL)                SUB A,(IX/Y+d)          XOR A,(IX/Y+d)
            SRA (IX/Y+d)            SUB A,n                 XOR A,n
            SRA r                   SUB A,r                 XOR A,r

            SRL (HL)                TST A,(HL)
            SRL (IX/Y+d)            TST A,n
            SRL r                   TST A,r

       The  accumulator  'A' argument is optional in all of the fol-
    lowing instructions:

            ADC A,...               CP A,...                SUB A,...
            ADD A,...               OR A,...                TST A,...
            AND A,...               SBC A,...               XOR A,...

       The  following  tables,  organized by instruction type, lists
    all possible EZ80/Z80  mnemonic  extensions  recognized  by  the
    ASEZ80  assembler.   The designation [] refers to a required ad-
    dressing mode argument shown in the table  above.   The  allowed
    mnemonic  suffixes  are  denoted within the enclosing delimiters
    ().  Mnemonics specified with illegal  or  unrecognized  suffixs
    will be flagged with q or a errors.

    Arithmetic Instructions

            adc (.l, .s)    [],[]
            add (.l, .s)    [],[]
            cp  (.l, .s)    [],[]
            daa
            dec (.l, .s)    []
            inc (.l, .s)    []
            mlt (.l, .s)    []
            neg
            sbc (.l, .s)    [],[]
            sub (.l, .s)    [],[]

    Bit Manipulation Instructions

            bit (.l, .s)    [],[]
            res (.l, .s)    [],[]
            set (.l, .s)    [],[]

    Block Transfer and Compare Instructions

            cpd (.l, .s)            cpdr (.l, .s)
            cpi (.l, .s)            cpir (.l, .s)
            ldd (.l, .s)            lddr (.l, .s)
            ldi (.l, .s)            ldir (.l, .s)

    Exchange Instructions

            ex (.l, .s)     [],[]
            exx

    Input/Output Instructions

            in      [],[]           in0     [],[]
            ind   (.l, .s)          indr  (.l, .s)
            indx  (.l, .s)
            ind2  (.l, .s)          ind2r (.l, .s)
            indm  (.l, .s)          indmr (.l, .s)
            ini   (.l, .s)          inir  (.l, .s)
            inim  (.l, .s)          inimr (.l, .s)
            otdm  (.l, .s)          otdmr (.l, .s)
            otdrx (.l, .s)
            otim  (.l, .s)          otimr (.l, .s)
            otirx (.l, .s)
            out   (.l, .s)  [],[]
            out0  (.l, .s)  [],[]
            outd  (.l, .s)          otdr  (.l, .s)
            outd2 (.l, .s)          otdr2 (.l, .s)
            outi  (.l, .s)          otir  (.l, .s)
            outi2 (.l, .s)          oti2r (.l, .s)
            tstio   []

    Load Instructions

            ld   (.l, .s, .il, .is, .lil, .sis)     [],[]
            lea  (.l, .s)   []      pea  (.l, .s)   []
            pop  (.l, .s)   []      push (.l, .s)   []

    Logical Instructions

            and (.l, .s)    [],[]
            cpl (.l, .s)
            or  (.l, .s)    [],[]
            tst (.l, .s)    [],[]
            xor (.l, .s)    [],[]

    Processor Control Instructions

            ccf             di              ei
            halt            im              nop
            rsmix           stmix
            scf             slp

    Program Flow Instructions

            call (.il, .is)         []
            call (.il, .is)         CC,[]
            djnz    []
            jp   (.l, .s, .lil, .sis)       []
            jp   (.l, .s, .lil, .sis)       CC,[]
            jr      []
            jr      CC,[]
            ret  (.l)
            ret  (.l)       CC
            reti (.l)
            retn (.l)
            rst  (.l, .s)   []

    Shift and Rotate Instructions

            rl  (.l, .s)    []      rla
            rlc (.l, .s)    []      rlca
            rld                     rrd
            rr  (.l, .s)    []      rra
            rrc (.1, .s)    []      rrca
            sla (.l, .s)    []
            sra (.l, .s)    []
            srl (.l, .s)    []

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: January 2006