## AS6812 Assembler

####

    PROCESSOR SPECIFIC DIRECTIVES

       The   AS6812  assembler  supports  the  68HC(S)12  series  of
    microprocessors which includes  the  68HC(S)8xx  and  68HC(S)9xx
    series.

    .hc12 Directive

    Format:

            .hc12

    The  .hc12 directive selects the HC12 core specific cycles count
    output when the -c command line option is specified.

    .hcs12 Directive

    Format:

            .hcs12

    The  .hcs12  directive  selects  the  HCS12 core specific cycles
    count output when the -c command line option is specified.

    The .__.CPU.  Variable

       The value of the pre-defined symbol '.__.CPU.' corresponds to
    the selected processor type.  The default value is 0 which  cor-
    responds  to  the  default  processor type.  The following table
    lists the processor types and associated values for  the  AS6812
    assembler:

            Processor Type            .__.CPU. Value
            --------------            --------------
                .hc12                        0
                .hcs12                       1

       The  variable  '.__.CPU.'  is by default defined as local and
    will not be output to the created .rel file.  The assembler com-
    mand line options -g or -a will not cause the local symbol to be
    output to the created .rel file.

       The  assembler  .globl  directive  may  be used to change the
    variable type to global causing its definition to be  output  to
    the  .rel file.  The inclusion of the definition of the variable
    '.__.CPU.' might be a useful means of validating that seperately
    assembled  files have been compiled for the same processor type.
    The linker will report an error for variables with multiple  non
    equal definitions.

    68HC(S)12 REGISTER SET

    The  following  is a list of the  68HC(S)12  registers  used  by
    AS6812:

            a,b     -       8-bit accumulators
            d       -       16-bit accumulator <a:b>
            x,y     -       index registers
            sp,s    -       stack pointer
            pc      -       program counter
            ccr,cc  -       condition code register

    68HC(S)12 INSTRUCTION SET

       The   following   tables   list   all   68HC(S)12   mnemonics
    recognized by the  AS6812 assembler.  The designation  [] refers
    to  a  required addressing  mode  argument.   The following list
    specifies  the  format  for  each  addressing   mode   supported
    by AS6812:

            #data           immediate data
                            byte or word data

            ext             extended addressing

            pg              memory page number

            *dir            direct page addressing
                            (see .setdp directive)
                            0 <= dir <= 255

            label           branch label

            r,r1,r2         registers
                            ccr,a,b,d,x,y,sp,pc

            -x      x-      register indexed, pre or
            ,-x     ,x-     post autodecrement by 1

            n,-x    n,x-    register indexed, pre or
                            post autodecrement by 1 - 8

            +x      x+      register indexed, pre or
            ,+x     ,x+     post autoincrement by 1

            n,+x    n,x+    register indexed, pre or
                            post autoincrement by 1 - 8

            offset,x        register indexed addressing
                               -16 <= offset <= 15    ---  5-bit
                              -256 <= offset <= -17   ---  9-bit
                                16 <= offset <= 255   ---  9-bit
                            -32768 <= offset <= -257  --- 16-bit
                               256 <= offset <= 32767 --- 16-bit
                            (external definition of offset
                             uses 16-bit mode)

            [offset,x]      register indexed indirect addressing
                            -32768 <= offset <= 32767 --- 16-bit

            [,x]            register indexed indirect addressing
                            zero offset

            a,x             accumulator offset indexed addressing

            [d,x]           d accumulator offset indexed
                            indirect addressing

    The  terms  data, dir, label, offset, and ext may all be expres-
    sions.

       Note  that  not all addressing modes are valid with every in-
    struction, refer to the 68HC(S)12 technical data for valid modes.

    Inherent Instructions

            aba             bgnd            cba
            daa             dex             dey
            ediv            edivs           emul
            emuls           fdiv            idiv
            idivs           inx             iny
            mem             mul             nop
            psha            pshb            pshc
            pshd            pshx            pshy
            pula            pulb            pulc
            puld            pulx            puly
            rev             revw            rtc
            rti             rts             sba
            stop            swi             tab
            tba             wai             wav
            wavr

    Short Branch Instructions

            bcc     label           bcs     label
            beq     label           bge     label
            bgt     label           bhi     label
            bhis    label           bhs     label
            ble     label           blo     label
            blos    label           bls     label
            blt     label           bmi     label
            bne     label           bpl     label
            bra     label           brn     label
            bvc     label           bvs     label
            bsr     label

    Long Branch Instructions

            lbcc    label           lbcs    label
            lbeq    label           lbge    label
            lbgt    label           lbhi    label
            lbhis   label           lbhs    label
            lble    label           lblo    label
            lblos   label           lbls    label
            lblt    label           lbmi    label
            lbne    label           lbpl    label
            lbra    label           lbrn    label
            lbvc    label           lbvs    label

    Branch on Decrement, Test, or Increment

            dbeq    r,label         dbne    r,label
            ibeq    r,label         ibne    r,label
            tbeq    r,label         tbne    r,label

    Bit Clear and Set Instructions

            bclr    [],#data
            bset    [],#data

    Branch on Bit Clear or Set

            brclr   [],#data,label
            brset   [],#data,label

    Single Operand Instructions

            asla            aslb
            asl     []

            asra            asrb
            asr     []

            clra            clrb
            clr     []

            coma            comb
            com     []

            deca            decb
            dec     []

            inca            incb
            inc     []

            lsla            lslb
            lsl     []

            lsra            lsrb
            lsr     []

            nega            negb
            neg     []

            rola            rolb
            rol     []

            rora            rorb
            ror     []

            tsta            tstb
            tst     []

    Double Operand Instructions

            adca    []              adcb    []

            adda    []              addb    []

            anda    []              andb    []

            bita    []              bitb    []

            cmpa    []              cmpb    []

            eora    []              eorb    []

            ldaa    []      <=>     lda     []

            ldab    []      <=>     ldb     []

            oraa    []      <=>     ora     []

            orab    []      <=>     orb     []

            sbca    []              sbcb    []

            staa    []      <=>     sta     []

            stab    []      <=>     stb     []

            suba    []              subb    []

    Move Instructions

            movb    [],[]           movw    [],[]

    D-register Instructions

            addd    []              subd    []
            cpd     []      <=>     cmpd    []
            ldd     []              std     []

    Index/Stack Register Instructions

            cps     []      <=>     cmps    []
            cpx     []      <=>     cmpx    []
            cpy     []      <=>     cmpy    []

            lds     []
            ldx     []              ldy     []

            leas    []
            leax    []              leay    []

            sts     []
            stx     []              sty     []

    Jump and Jump/Call to Subroutine Instructions

            call    [],pg
            jmp     []              jsr     []

    Other Special Instructions

            emacs   []
            emaxd   []              emaxm   []
            emind   []              eminm   []
            etbl    []
            maxa    []              maxm    []
            mina    []              minm    []
            tbl     []              trap    #data

    H.2.14  Register - Register Instructions

            exg     r1,r2           sex     r1,r2
            tfr     r1,r2

    Condition Code Register Instructions

            andcc   #data           orcc    #data

    M68HC11 Compatibility Mode Instructions

            abx             aby             clc
            cli             clv             des
            ins             sec             sei
            sev             tap             tpa
            tsx             tsy             txs
            tys             xgdx            xgdy

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page

######

Last Updated: January 2006