Subject: bad144 is missing the RP07 entry (#147) Index: etc/bad144.c 2.11BSD Description: The bad144 program does not recognize the 'rp07' drive type. Repeat-By: Attempt to add a sector to the bad block table on a RP07. Fix: Apply the patch below (thanks to Johnny Billquist for providing this fix), recompile and install 'bad144'. =============================cut here============================ *** /usr/src/etc/bad144.c.old Sat Aug 22 16:10:23 1987 --- /usr/src/etc/bad144.c Tue Aug 10 19:50:29 1993 *************** *** 17,22 **** --- 17,24 ---- * reformatting. To add a new bad sector the formatter must be used in * general since UNIX doesn't have on-line formatters to write the BSE * error in the header. + * + * RP07 entry added August 10, 1993 (thanks to Johnny Billquist) - SMS */ #include #ifndef BADSECT *************** *** 41,46 **** --- 43,49 ---- "rp04", 22*19*411L, 22, 19, "rp05", 22*19*411L, 22, 19, "rp06", 22*19*815L, 22, 19, + "rp07", 50*32*630L, 50, 32, "fuji160", 32*10*823L, 32, 10, "diva", 33*19*815L, 33, 19, "ampex9300", 33*19*815L, 33, 19,