Subject: Part 21 of 22 /boot,/mdec,[T]MSCP updates Index: /sys/, /usr/src/etc/ 2.11BSD Description: Repeat-By: Fix: See part 0 (the README) for the Description, the Reason and the instructions on how update your system. This is part 21 of 22 A new drive type 'rm2x' was added. This is used for the Fuji 160 with the Emulex SC01 or SC03 in RM80 emulation mode(10x32x823) *** /usr/src/etc/newfs.c.old Tue Aug 21 12:35:59 1990 --- /usr/src/etc/newfs.c Fri May 10 21:29:57 1991 *************** *** 4,18 **** * specifies the terms and conditions for redistribution. */ ! #ifndef lint char copyright[] = "@(#) Copyright (c) 1983 Regents of the University of California.\n\ All rights reserved.\n"; - #endif not lint ! #ifndef lint ! static char sccsid[] = "@(#)newfs.c 5.2 (Berkeley) 8/18/88"; ! #endif not lint /* * newfs: friendly front end to mkfs --- 4,16 ---- * specifies the terms and conditions for redistribution. */ ! #if !defined(lint) && defined(DOSCCS) char copyright[] = "@(#) Copyright (c) 1983 Regents of the University of California.\n\ All rights reserved.\n"; ! static char sccsid[] = "@(#)newfs.c 5.3 (2.11BSD) 5/10/91"; ! #endif /* * newfs: friendly front end to mkfs *************** *** 54,59 **** --- 52,58 ---- { "rp03", 16 }, { "br1538d", 17 }, { "ra82", 18 }, + { "rm2x", 19 }, /* Fuji 160 in pseudo RM80 mode */ { 0, 0 } }; *************** *** 102,107 **** --- 101,107 ---- /* RP03 */ { {16,304}, {15,304}, {12,304}, { 7,304}, {11,304}, { 5,304} }, /* BR1538D */ { {16,304}, {15,304}, {12,304}, { 7,304}, {11,304}, { 6,304} }, /* RA82 */ { {26,435}, {26,435}, {21,435}, {14,435}, {18,435}, {12,435} }, + /* RM2X */ { {11,160}, {10,160}, { 8,160}, { 6,160}, { 7,160}, { 5,160} }, }; main(argc, argv)