# 2.11BSD#431 - /usr/man/cat8/sysgen.0

    SYSGEN(1)	    UNIX Programmer's Manual		SYSGEN(1)

    NAME
         sysgen - assign DEC standard CSR and vector addresses

    SYNOPSIS
         sysgen

    DESCRIPTION
         This filter reads DEC Qbus or UNIBUS device names from stan-
         dard input, assigns CSR addresses and interrupt vectors to
         the devices according to the DEC standard algorithm for
         auto-configuration, and prints the resulting list of alloca-
         tions to standard output.

         Floating CSRs and vectors are identified by a trailing
         asterisk.

    COMPATIBILITY
         The program attempts to conform to the CONFIG command of the
         VMS SYSGEN program, but has simplified output.  Specifi-
         cally, it does not print information about VMS device naming
         and support.

    BUGS
         More device type aliases should be recognized.  There should
         be a ``help'' command to list known devices so that cat'ing
         the devices.h file is not necessary.

    Printed 11/26/99	  June 8, 1997				1

Generated: 2016-12-26 | Generated by man2html V0.25 page hit count: 583 |