# 2.11BSD#431 - /usr/src/sys/pdpif/if_qtreg.h

##### Macros

    ARQR_RRQ          X
    ARQR_SR           X
    ARQR_TRQ          X
    ICR_CMD           X
    INIT_MODE_DRT     X
    INIT_MODE_DTC     X
    INIT_MODE_INT     X
    INIT_MODE_LOP     X
    INIT_MODE_PRO     X
    INIT_OPTIONS_HIT  X
    INIT_OPTIONS_INT  X
    QT_MAX_RCV        X
    QT_MAX_XMT        X
    RMD0_BITS         X
    RMD0_BUF          X
    RMD0_CRC          X
    RMD0_ENP          X
    RMD0_ERR3         X
    RMD0_FRA          X
    RMD0_OFL          X
    RMD0_STP          X
    RMD1_MCNT         X
    RMD2_BBL          X
    RMD2_BITS         X
    RMD2_CER          X
    RMD2_EOR          X
    RMD2_ERR4         X
    RMD2_MIS          X
    RMD2_RON          X
    RMD2_TON          X
    RMD3_OWN          X
    RMD4_LADR         X
    RMD5_HADR         X
    SRQR_REQ          X
    SRR_BITS          X
    SRR_CHN           X
    SRR_FES           X
    SRR_IME           X
    SRR_NXM           X
    SRR_PER           X
    SRR_RESP          X
    SRR_TBL           X
    TMD0_DEF          X
    TMD0_ERR1         X
    TMD0_MOR          X
    TMD0_ONE          X
    TMD1_BITS         X
    TMD1_LCA          X
    TMD1_LCO          X
    TMD1_RTR          X
    TMD1_TDR          X
    TMD2_BBL          X
    TMD2_BITS         X
    TMD2_CER          X
    TMD2_EOR          X
    TMD2_ERR2         X
    TMD2_MIS          X
    TMD2_RON          X
    TMD2_TON          X
    TMD3_BCT          X
    TMD3_FOT          X
    TMD3_OWN          X
    TMD4_LADR         X
    TMD5_HADR         X
    ibah              X
    ibal              X
    icr               X
    sarom             X
    srqr              X
    xcr0              X
    xcr1              X

##### struct's

    qt_init           X
    qt_rring          X
    qt_tring          X
    qtcsr0            X
    qtdevice          X

       1: /*	@(#)if_qtreg.h	1.0 (GTE) 10/12/92 */
       2:
       3: /*
       4:  * Modification History
       5:  *  26 Feb 93 -- sms
       6:  *	Add defines for number of receive and transmit ring descriptors.
       7:  *
       8:  *  12 Oct 92 -- Steven M. Schultz (sms)
       9:  *	Created from the DELQA-PLUS Addendum to the DELQA User's Guide.
      10: */
      11:
      12: #define QT_MAX_RCV  32
      13: #define QT_MAX_XMT  12
      14:
      15: /* Receive ring descriptor and bit/field definitions */
      16:
      17:     struct  qt_rring
      18:         {
      19:         short   rmd0;
      20:         short   rmd1;
      21:         short   rmd2;
      22:         short   rmd3;
      23:         short   rmd4;
      24:         short   rmd5;
      25:         struct  qt_uba  *rhost0;
      26:         short   rhost1;
      27:         };
      28:
      29: #define RMD0_ERR3   0x4000      /* Error summary. FRA|CRC|OFL|BUF */
      30: #define RMD0_FRA    0x2000      /* Framing error */
      31: #define RMD0_OFL    0x1000      /* Overflow error.  Oversized packet */
      32: #define RMD0_CRC    0x0800      /* CRC error */
      33: #define RMD0_BUF    0x0400      /* Internal device buffer error */
      34: #define RMD0_STP    0x0200      /* Start of packet */
      35: #define RMD0_ENP    0x0100      /* End of packet */
      36:
      37: #define RMD1_MCNT   0x0fff      /* Message byte count */
      38:
      39: #define RMD2_ERR4   0x8000      /* Error summary.  BBL|CER|MIS */
      40: #define RMD2_BBL    0x4000      /* Babble error on transmit */
      41: #define RMD2_CER    0x2000      /* Collision error on transmit */
      42: #define RMD2_MIS    0x1000      /* Packet lost on receive */
      43: #define RMD2_EOR    0x0800      /* End of receive ring */
      44: #define RMD2_RON    0x0020      /* Receiver on */
      45: #define RMD2_TON    0x0010      /* Transmitter on */
      46:
      47: #define RMD3_OWN    0x8000      /* Ownership field. */
      48:
      49: #define RMD4_LADR   0xfff8      /* Octabyte aligned low address bits */
      50:
      51: #define RMD5_HADR   0x003f      /* High 6 bits of buffer address */
      52:
      53: #define RMD0_BITS   "\010\016FRA\015OFL\014CRC\013BUF\012STP\011ENP"
      54: #define RMD2_BITS   "\010\017BBL\014CER\013MIS\012EOR\06RON\05TON"
      55:
      56: /* Transmit ring descriptor and bit/field definitions */
      57:
      58:     struct  qt_tring
      59:         {
      60:         short   tmd0;
      61:         short   tmd1;
      62:         short   tmd2;
      63:         short   tmd3;
      64:         short   tmd4;
      65:         short   tmd5;
      66:         struct  qt_uba  *thost0;
      67:         short   thost1;
      68:         };
      69:
      70: #define TMD0_ERR1   0x4000      /* Error summary.  LCO|LCA|RTR */
      71: #define TMD0_MOR    0x1000      /* More than one retry on transmit */
      72: #define TMD0_ONE    0x0800      /* One retry on transmit */
      73: #define TMD0_DEF    0x0400      /* Deferral during transmit */
      74:
      75: #define TMD1_LCO    0x1000      /* Late collision on transmit */
      76: #define TMD1_LCA    0x0800      /* Loss of carrier on transmit */
      77: #define TMD1_RTR    0x0400      /* Retry error on transmit */
      78: #define TMD1_TDR    0x03ff      /* Time Domain Reflectometry value */
      79:
      80: #define TMD2_ERR2   0x8000      /* Error summary.  BBL|CER|MIS */
      81: #define TMD2_BBL    0x4000      /* Babble error on transmit */
      82: #define TMD2_CER    0x2000      /* Collision error on transmit */
      83: #define TMD2_MIS    0x1000      /* Packet lost on receive */
      84: #define TMD2_EOR    0x0800      /* Endof Receive ring reached */
      85: #define TMD2_RON    0x0020      /* Receiver on */
      86: #define TMD2_TON    0x0010      /* Transmitter on */
      87:
      88: #define TMD3_OWN    0x8000      /* Ownership field */
      89: #define TMD3_FOT    0x4000      /* First of two flag */
      90: #define TMD3_BCT    0x0fff      /* Byte count */
      91:
      92: #define TMD4_LADR   0xfff8      /* Octabyte aligned low address bits */
      93:
      94: #define TMD5_HADR   0x003f      /* High 6 bits of buffer address */
      95:
      96: #define TMD1_BITS   "\010\015LCO\014LCA\013RTR"
      97: #define TMD2_BITS   "\010\017BBL\016CER\015MIS\014EOR\06RON\05TON"
      98:
      99: /* DELQA-YM CSR layout */
     100:
     101:     struct  qtcsr0
     102:         {
     103:         short   Ibal;
     104:         short   Ibah;
     105:         short   Icr;
     106:         short   pad0;
     107:         short   Srqr;
     108:         short   pad1;
     109:         };
     110:
     111:     struct  qtdevice
     112:         {
     113:         union   {
     114:             u_char  Sarom[12];
     115:             struct  qtcsr0  csr0;
     116:             } qt_un0;
     117:         short   srr;
     118:         short   arqr;
     119:         };
     120:
     121: #define ibal    qt_un0.csr0.Ibal
     122: #define ibah    qt_un0.csr0.Ibah
     123: #define srqr    qt_un0.csr0.Srqr
     124: #define icr qt_un0.csr0.Icr
     125: #define sarom   qt_un0.Sarom
     126:
     127: /* SRR definitions */
     128:
     129: #define SRR_FES     0x8000
     130: #define SRR_CHN     0x4000
     131: #define SRR_NXM     0x1000
     132: #define SRR_PER     0x0800
     133: #define SRR_IME     0x0400
     134: #define SRR_TBL     0x0200
     135: #define SRR_RESP    0x0003
     136: #define SRR_BITS    "\010\017CHN\015NXM\014PER\013IME\012TBL"
     137:
     138: /* SRQR definitions */
     139:
     140: #define SRQR_REQ    0x0003
     141:
     142: /* ARQR definitions */
     143:
     144: #define ARQR_TRQ    0x8000
     145: #define ARQR_RRQ    0x0080
     146: #define ARQR_SR     0x0002
     147:
     148: /* define ICR definitions */
     149:
     150: #define ICR_CMD     0x0001
     151:
     152: /* DELQA registers used to shift into -T mode */
     153:
     154: #define xcr0    qt_un0.csr0.Ibal
     155: #define xcr1    qt_un0.csr0.Ibah
     156:
     157: /* INIT block structure and definitions */
     158:
     159:     struct  qt_init
     160:         {
     161:         short   mode;
     162:         u_char  paddr[6];   /* 48 bit physical address */
     163:         u_char  laddr[8];   /* 64 bit logical address filter */
     164:         u_short rx_lo;      /* low 16 bits of receive ring addr */
     165:         u_short rx_hi;      /* high 6 bits of receive ring addr */
     166:         u_short tx_lo;      /* low 16 bits of transmit ring addr */
     167:         u_short tx_hi;      /* high 6 bits of transmit ring addr */
     168:         u_short options;
     169:         u_short vector;
     170:         u_short hit;
     171:         char    passwd[6];
     172:         };
     173:
     174: #define INIT_MODE_PRO   0x8000      /* Promiscuous mode */
     175: #define INIT_MODE_INT   0x0040      /* Internal Loopback */
     176: #define INIT_MODE_DRT   0x0020      /* Disable Retry */
     177: #define INIT_MODE_DTC   0x0008      /* Disable Transmit CRC */
     178: #define INIT_MODE_LOP   0x0004      /* Loopback */
     179:
     180: #define INIT_OPTIONS_HIT 0x0002     /* Host Inactivity Timeout Flag */
     181: #define INIT_OPTIONS_INT 0x0001     /* Interrupt Enable Flag */

#### Defined struct's

qt_init defined in line 159; used 16 times

- in /usr/src/sys/pdpif/if_qt.c line 177(4), 199-202(4), 245(4), 765(4)

qt_rring defined in line 17; used 10 times

- in /usr/src/sys/pdpif/if_qt.c line 114-116(4), 203(2), 308(2), 527(2)

qt_tring defined in line 58; used 12 times

- in /usr/src/sys/pdpif/if_qt.c line 115-117(4), 204(2), 309(2), 384(2), 472(2)

qtcsr0 defined in line 101; used 2 times

- in line 115(2)

qtdevice defined in line 111; used 8 times

- in /usr/src/sys/pdpif/if_qt.c line 127(2), 198(2), 244(2), 306(2)

#### Defined macros

ARQR_RRQ defined in line 145; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 591

ARQR_SR defined in line 146; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 253

ARQR_TRQ defined in line 144; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 416

ICR_CMD defined in line 150; never used
INIT_MODE_DRT defined in line 176; never used
INIT_MODE_DTC defined in line 177; never used
INIT_MODE_INT defined in line 175; never used
INIT_MODE_LOP defined in line 178; never used
INIT_MODE_PRO defined in line 174; never used
INIT_OPTIONS_HIT defined in line 180; never used
INIT_OPTIONS_INT defined in line 181; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 215

QT_MAX_RCV defined in line 12; used 4 times

- in /usr/src/sys/pdpif/if_qt.c line 116, 322, 565, 592

QT_MAX_XMT defined in line 13; used 4 times

- in /usr/src/sys/pdpif/if_qt.c line 117, 332, 418, 513

RMD0_BITS defined in line 53; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 556

RMD0_BUF defined in line 33; never used
RMD0_CRC defined in line 32; never used
RMD0_ENP defined in line 35; used 2 times

- in /usr/src/sys/pdpif/if_qt.c line 543(2)

RMD0_ERR3 defined in line 29; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 552

RMD0_FRA defined in line 30; never used
RMD0_OFL defined in line 31; never used
RMD0_STP defined in line 34; used 2 times

- in /usr/src/sys/pdpif/if_qt.c line 543(2)

RMD1_MCNT defined in line 37; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 549

RMD2_BBL defined in line 40; never used
RMD2_BITS defined in line 54; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 557

RMD2_CER defined in line 41; never used
RMD2_EOR defined in line 43; never used
RMD2_ERR4 defined in line 39; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 552

RMD2_MIS defined in line 42; never used
RMD2_RON defined in line 44; never used
RMD2_TON defined in line 45; never used
RMD3_OWN defined in line 47; used 3 times

- in /usr/src/sys/pdpif/if_qt.c line 324, 532, 579

RMD4_LADR defined in line 49; never used
RMD5_HADR defined in line 51; never used
SRQR_REQ defined in line 140; never used
SRR_BITS defined in line 136; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 844

SRR_CHN defined in line 130; never used
SRR_FES defined in line 129; never used
SRR_IME defined in line 133; never used
SRR_NXM defined in line 131; never used
SRR_PER defined in line 132; never used
SRR_RESP defined in line 135; used 2 times

- in /usr/src/sys/pdpif/if_qt.c line 274, 444

SRR_TBL defined in line 134; never used
TMD0_DEF defined in line 73; never used
TMD0_ERR1 defined in line 70; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 505

TMD0_MOR defined in line 71; never used
TMD0_ONE defined in line 72; never used
TMD1_BITS defined in line 96; never used
TMD1_LCA defined in line 76; never used
TMD1_LCO defined in line 75; never used
TMD1_RTR defined in line 77; never used
TMD1_TDR defined in line 78; never used
TMD2_BBL defined in line 81; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 466

TMD2_BITS defined in line 97; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 509

TMD2_CER defined in line 82; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 503

TMD2_EOR defined in line 84; never used
TMD2_ERR2 defined in line 80; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 506

TMD2_MIS defined in line 83; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 466

TMD2_RON defined in line 85; never used
TMD2_TON defined in line 86; never used
TMD3_BCT defined in line 90; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 414

TMD3_FOT defined in line 89; never used
TMD3_OWN defined in line 88; used 3 times

- in /usr/src/sys/pdpif/if_qt.c line 334, 397, 478

TMD4_LADR defined in line 92; never used
TMD5_HADR defined in line 94; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 413

ibah defined in line 122; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 362

ibal defined in line 121; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 361

icr defined in line 124; never used
sarom defined in line 125; used 6 times

- in /usr/src/sys/pdpif/if_qt.c line 290-295(6)

srqr defined in line 123; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 363

xcr0 defined in line 154; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 270

xcr1 defined in line 155; used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 271

#### Usage of this include

if_qtreg.h used 1 times

- in /usr/src/sys/pdpif/if_qt.c line 89

Last modified: 1993-02-27 Generated: 2016-12-26 | Generated by src2html V0.67 page hit count: 1245 |