# 2.11BSD#431 - /usr/src/sys/autoconfig/uprobe.c

##### Variables

    uprobe            X

       1: /*
       2:  * Copyright (c) 1986 Regents of the University of California.
       3:  * All rights reserved.  The Berkeley software License Agreement
       4:  * specifies the terms and conditions for redistribution.
       5:  *
       6:  *	@(#)uprobe.c	2.1 (2.11BSD GTE) 6/16/93
       7:  */
       8:
       9: /*
      10:  * The uprobe table contains the pointers to the user-level probe routines
      11:  * that may attempt to make various devices interrupt.
      12:  *
      13:  * NOTES:
      14:  *	Reads and writes to kmem (done by grab, stuff) are currently done a
      15:  *	byte at a time in the kernel.  Also, many of these are untested and
      16:  *	some of them assume that if something is at the address, it is the
      17:  *	correct device.  Others assume that if something *isn't* at the
      18:  *	address, the correct device *is*.  Why are you looking at me like
      19:  *	that?
      20:  */
      21:
      22: #include "uprobe.h"
      23:
      24: int xpprobe(), hkprobe(), rlprobe(), rkprobe(), htprobe(), siprobe(),
      25:     tmprobe(), tsprobe(), cnprobe(), dzprobe(), dhprobe(), dmprobe(),
      26:     drprobe(), lpprobe(), dhuprobe(), raprobe(), rxprobe(), brprobe(),
      27:     dnprobe(), tmsprobe(), dhvprobe();
      28:
      29: UPROBE uprobe[] = {
      30:     "hk",   hkprobe,    /* hk -- rk611, rk06/07 */
      31:     "hp",   xpprobe,    /* hp -- rjp04/06, rwp04/06 */
      32:     "ra",   raprobe,    /* ra -- MSCP */
      33:     "rk",   rkprobe,    /* rk -- rk05 */
      34:     "rl",   rlprobe,    /* rl -- rl01/02 */
      35:     "si",   siprobe,    /* si -- SI 9500 for CDC 9766 */
      36:     "xp",   xpprobe,    /* xp -- rm02/03/05, rp04/05/06, Diva, Ampex, SI Eagle */
      37:     "ht",   htprobe,    /* ht -- tju77, twu77, tje16, twe16 */
      38:     "tm",   tmprobe,    /* tm -- tm11 */
      39:     "ts",   tsprobe,    /* ts -- ts11 */
      40:     "dh",   dhprobe,    /* dh -- DH11 */
      41:     "dm",   dmprobe,    /* dm -- DM11 */
      42:     "dr",   drprobe,    /* dr -- DR11W */
      43:     "du",   dhuprobe,   /* du -- DHU11 */
      44:     "dhv",  dhvprobe,   /* dhv -- DHV11 */
      45:     "dz",   dzprobe,    /* dz -- dz11 */
      46:     "cn",   cnprobe,    /* cn -- kl11, dl11 */
      47:     "lp",   lpprobe,    /* lp -- line printer */
      48:     "rx",   rxprobe,    /* rx -- RX01/02 */
      49:     "br",   brprobe,    /* br -- EATON 1538 BR1537/BR1711 */
      50:     "dn",   dnprobe,    /* dn -- dn11 autodialer */
      51:     "tms",  tmsprobe,   /* tms -- TMSCP tape controller */
      52:     0,  0,
      53: };

#### Defined variables

uprobe defined in line 29; never used

Last modified: 1993-06-17 Generated: 2016-12-26 | Generated by src2html V0.67 page hit count: 484 |