# 2.11BSD#431 - /usr/src/sys/pdpuba/hpreg.h

##### Macros

    HPCS2_BAI         X
    HPCS2_BITS        X
    HPCS2_CLR         X
    HPCS2_DLT         X
    HPCS2_IR          X
    HPCS2_MDPE        X
    HPCS2_MXF         X
    HPCS2_NED         X
    HPCS2_NEM         X
    HPCS2_OR          X
    HPCS2_PAT         X
    HPCS2_PGE         X
    HPCS2_UPE         X
    HPCS2_WCE         X
    HPCS3_APE         X
    HPCS3_BITS        X
    HPCS3_DPE         X
    HPCS3_DW          X
    HPCS3_IE          X
    HPCS3_WCE         X
    HPDS_ATA          X
    HPDS_BITS         X
    HPDS_DAE          X
    HPDS_DPR          X
    HPDS_DREADY       X
    HPDS_DRY          X
    HPDS_ERR          X
    HPDS_ILV          X
    HPDS_LST          X
    HPDS_MOL          X
    HPDS_OM           X
    HPDS_PIP          X
    HPDS_VV           X
    HPDS_WRL          X
    HPDT_DRR          X
    HPDT_MH           X
    HPDT_NBA          X
    HPDT_RM02         X
    HPDT_RM03         X
    HPDT_RM05         X
    HPDT_RM80         X
    HPDT_RP04         X
    HPDT_RP05         X
    HPDT_RP06         X
    HPDT_RP07         X
    HPDT_TAPE         X
    HPER1_AOE         X
    HPER1_BITS        X
    HPER1_DCK         X
    HPER1_DTE         X
    HPER1_ECH         X
    HPER1_FER         X
    HPER1_HCE         X
    HPER1_HCRC        X
    HPER1_IAE         X
    HPER1_ILF         X
    HPER1_ILR         X
    HPER1_OPI         X
    HPER1_PAR         X
    HPER1_RMR         X
    HPER1_UNS         X
    HPER1_WCF         X
    HPER1_WLE         X
    HPHR_MAXCYL       X
    HPHR_MAXSECT      X
    HPHR_MAXTRAK      X
    HPOF_BITS         X
    HPOF_ECI          X
    HPOF_FMT22        X
    HPOF_HCI          X
    HPOF_M1200        X
    HPOF_M400         X
    HPOF_M800         X
    HPOF_P1200        X
    HPOF_P400         X
    HPOF_P800         X
    HP_BITS           X
    HP_BOOT           X
    HP_DCLR           X
    HP_DVA            X
    HP_FORMAT         X
    HP_GO             X
    HP_IE             X
    HP_MCPE           X
    HP_NOP            X
    HP_OFFSET         X
    HP_PACK           X
    HP_PRESET         X
    HP_RCOM           X
    HP_RDY            X
    HP_RECAL          X
    HP_RELEASE        X
    HP_RHDR           X
    HP_RTC            X
    HP_SC             X
    HP_SEARCH         X
    HP_SEEK           X
    HP_TRE            X
    HP_UNLOAD         X
    HP_WCDATA         X
    HP_WCHDR          X
    HP_WCOM           X
    HP_WHDR           X
    RMER2_BITS        X
    RMER2_BSE         X
    RMER2_DPE         X
    RMER2_DVC         X
    RMER2_IVC         X
    RMER2_LBC         X
    RMER2_LSC         X
    RMER2_MDPE        X
    RMER2_SKI         X
    SI9730D           X
    SI9730M           X
    SI9751D           X
    SI9762            X
    SI9766            X
    SI9775D           X
    SI9775M           X
    SICAPD            X
    SICAPN            X
    SIMB_LU           X
    SIMB_MB           X
    SIMB_S6           X
    SIRM03            X
    SIRM05            X
    XP_CC             X
    XP_NOSEARCH       X
    rmer2             X
    rmhr              X
    rmmr2             X

##### struct's

    hpdevice          X

       1: /*
       2:  * Copyright (c) 1986 Regents of the University of California.
       3:  * All rights reserved.  The Berkeley software License Agreement
       4:  * specifies the terms and conditions for redistribution.
       5:  *
       6:  *	@(#)hpreg.h	2.0 (2.11BSD) 1995/07/20
       7:  */
       8:
       9: /*
      10:  * Definitions for SMD-type disk drives and drivers.
      11:  */
      12:
      13: #define XP_CC   0x1 /* drivedata[0] bit indicating presence of current
      14: 			 * cylinder 'hpcc' register.  Only set for RP04,5,6,7.
      15: 			*/
      16: #define XP_NOSEARCH 0x2 /* drivedata[0] bit indicating lack of search cmd */
      17:
      18: /*
      19:  *	Controller registers and bits
      20:  */
      21: struct hpdevice
      22: {
      23:     union   {
      24:         int w;
      25:         char    c[2];
      26:     }   hpcs1;      /* control and status 1 register */
      27:     short   hpwc;       /* word count register */
      28:     caddr_t hpba;       /* UNIBUS address register */
      29:     short   hpda;       /* desired address register */
      30:     union   {
      31:         int w;
      32:         char    c[2];
      33:     }   hpcs2;      /* control and status 2 register */
      34:     short   hpds;       /* drive status register */
      35:     short   hper1;      /* error register 1 */
      36:     short   hpas;       /* attention summary register */
      37:     short   hpla;       /* look ahead register */
      38:     short   hpdb;       /* data buffer register */
      39:     short   hpmr;       /* maintenance register (1) */
      40:     short   hpdt;       /* drive type register */
      41:     short   hpsn;       /* serial number register */
      42:     short   hpof;       /* offset register */
      43:     short   hpdc;       /* desired cylinder address register */
      44:     short   hpcc;       /* HP: current cylinder register */
      45: #define rmhr    hpcc        /* RM: holding register */
      46:     short   hper2;      /* HP: error register 2 */
      47: #define rmmr2   hper2       /* RM: maintenance register 2 */
      48:     short   hper3;      /* HP: error register 3 */
      49: #define rmer2   hper3       /* RM: error register 2 */
      50:     short   hpec1;      /* burst error bit position */
      51:     short   hpec2;      /* burst error bit pattern */
      52:     short   hpbae;      /* bus address extension register (RH70 only) */
      53:     short   hpcs3;      /* control and status 3 register (RH70 only) */
      54: };
      55:
      56: /* Other bits of hpcs1 */
      57: #define HP_SC       0100000     /* special condition */
      58: #define HP_TRE      0040000     /* transfer error */
      59: #define HP_MCPE     0020000     /* MASSBUS control bus read parity error */
      60: /* bit 12 is unused */
      61: #define HP_DVA      0004000     /* drive available */
      62: /* bits 9 and 8 are the extended address bits */
      63: #define HP_RDY      0000200     /* controller ready */
      64: #define HP_IE       0000100     /* interrupt enable */
      65: /* bits 5-1 are the command */
      66: #define HP_GO       0000001
      67: #define HP_BITS     \
      68: "\10\20SC\17TRE\16MCPE\14DVA\10RDY\7IE\1GO"
      69:
      70: /* commands */
      71: #define HP_NOP      000
      72: #define HP_UNLOAD   002     /* offline drive */
      73: #define HP_SEEK     004     /* seek */
      74: #define HP_RECAL    006     /* recalibrate */
      75: #define HP_DCLR     010     /* drive clear */
      76: #define HP_RELEASE  012     /* release */
      77: #define HP_OFFSET   014     /* offset */
      78: #define HP_RTC      016     /* return to center-line */
      79: #define HP_PRESET   020     /* read-in preset */
      80: #define HP_PACK     022     /* pack acknowledge */
      81: #define HP_SEARCH   030     /* search */
      82: #define HP_WCDATA   050     /* write check data */
      83: #define HP_WCHDR    052     /* write check header and data */
      84: #define HP_WCOM     060     /* write */
      85: #define HP_WHDR     062     /* write header and data */
      86: #define HP_RCOM     070     /* read data */
      87: #define HP_RHDR     072     /* read header and data */
      88: /* The following two are optionally enabled on some non-DEC controllers */
      89: #define HP_BOOT     074     /* boot */
      90: #define HP_FORMAT   076     /* format */
      91:
      92: /* hpcs2 */
      93: #define HPCS2_DLT   0100000     /* data late */
      94: #define HPCS2_WCE   0040000     /* write check error */
      95: #define HPCS2_UPE   0020000     /* UNIBUS parity error */
      96: #define HPCS2_NED   0010000     /* nonexistent drive */
      97: #define HPCS2_NEM   0004000     /* nonexistent memory */
      98: #define HPCS2_PGE   0002000     /* programming error */
      99: #define HPCS2_MXF   0001000     /* missed transfer */
     100: #define HPCS2_MDPE  0000400     /* MASSBUS data read parity error */
     101: #define HPCS2_OR    0000200     /* output ready */
     102: #define HPCS2_IR    0000100     /* input ready */
     103: #define HPCS2_CLR   0000040     /* controller clear */
     104: #define HPCS2_PAT   0000020     /* parity test */
     105: #define HPCS2_BAI   0000010     /* address increment inhibit */
     106: /* bits 2-0 are drive select */
     107:
     108: #define HPCS2_BITS \
     109: "\10\20DLT\17WCE\16UPE\15NED\14NEM\13PGE\12MXF\11MDPE\
     110: \10OR\7IR\6CLR\5PAT\4BAI"
     111:
     112: /* hpds */
     113: #define HPDS_ATA    0100000     /* attention active */
     114: #define HPDS_ERR    0040000     /* composite drive error */
     115: #define HPDS_PIP    0020000     /* positioning in progress */
     116: #define HPDS_MOL    0010000     /* medium on line */
     117: #define HPDS_WRL    0004000     /* write locked */
     118: #define HPDS_LST    0002000     /* last sector transferred */
     119: #define HPDS_DAE    0001000     /* dual access enabled (programmable) */
     120: #define HPDS_DPR    0000400     /* drive present */
     121: #define HPDS_DRY    0000200     /* drive ready */
     122: #define HPDS_VV     0000100     /* volume valid */
     123: /* bits 5-3, 1 are spare */
     124: #define HPDS_ILV    0000004     /* interleaved */
     125: #define HPDS_OM     0000001     /* offset mode */
     126:
     127: #define HPDS_DREADY (HPDS_DPR|HPDS_DRY|HPDS_MOL|HPDS_VV)
     128:
     129: #define HPDS_BITS \
     130: "\10\20ATA\17ERR\16PIP\15MOL\14WRL\13LST\12DAE\11DPR\10DRY\7VV\3ILV\1OM"
     131:
     132: /* hper1 */
     133: #define HPER1_DCK   0100000     /* data check */
     134: #define HPER1_UNS   0040000     /* drive unsafe */
     135: #define HPER1_OPI   0020000     /* operation incomplete */
     136: #define HPER1_DTE   0010000     /* drive timing error */
     137: #define HPER1_WLE   0004000     /* write lock error */
     138: #define HPER1_IAE   0002000     /* invalid address error */
     139: #define HPER1_AOE   0001000     /* address overflow error */
     140: #define HPER1_HCRC  0000400     /* header crc error */
     141: #define HPER1_HCE   0000200     /* header compare error */
     142: #define HPER1_ECH   0000100     /* ecc hard error */
     143: #define HPER1_WCF   0000040     /* write clock fail (0) */
     144: #define HPER1_FER   0000020     /* format error */
     145: #define HPER1_PAR   0000010     /* parity error */
     146: #define HPER1_RMR   0000004     /* register modification refused */
     147: #define HPER1_ILR   0000002     /* illegal register */
     148: #define HPER1_ILF   0000001     /* illegal function */
     149:
     150: #define HPER1_BITS \
     151: "\10\20DCK\17UNS\16OPI\15DTE\14WLE\13IAE\12AOE\11HCRC\10HCE\
     152: \7ECH\6WCF\5FER\4PAR\3RMR\2ILR\1ILF"
     153:
     154: /* hpdt */
     155: #define HPDT_NBA    0100000     /* not block addressed; always 0 */
     156: #define HPDT_TAPE   0040000     /* tape drive; always 0 */
     157: #define HPDT_MH     0020000     /* moving head; always 1 */
     158: /* bit 12 is unused */
     159: #define HPDT_DRR    0004000     /* drive request required  */
     160: /* bits 10-9 are unused */
     161: /* bits 8-0 are drive type; the correct values are hard to determine */
     162: #define HPDT_RM02   0000025     /* rm02, possibly rm03? */
     163: #define HPDT_RM80   0000026     /* rm80 */
     164: #define HPDT_RM05   0000027     /* rm05 */
     165: #define HPDT_RM03   0000024     /* rm03 */
     166: #define HPDT_RP04   0000020     /* rp04 */
     167: #define HPDT_RP05   0000021     /* rp05 */
     168: #define HPDT_RP06   0000022     /* rp06 */
     169: #define HPDT_RP07   0000042     /* rp07 */
     170:
     171: /* hpof */
     172: #define HPOF_FMT22  0010000     /* 16 bit format */
     173: #define HPOF_ECI    0004000     /* ecc inhibit */
     174: #define HPOF_HCI    0002000     /* header compare inhibit */
     175:
     176: /* THE SC21 ACTUALLY JUST IMPLEMENTS ADVANCE/RETARD... */
     177: #define HPOF_P400   0020        /*  +400 uinches */
     178: #define HPOF_M400   0220        /*  -400 uinches */
     179: #define HPOF_P800   0040        /*  +800 uinches */
     180: #define HPOF_M800   0240        /*  -800 uinches */
     181: #define HPOF_P1200  0060        /* +1200 uinches */
     182: #define HPOF_M1200  0260        /* -1200 uinches */
     183:
     184: #define HPOF_BITS   \
     185: "\10\15FMT22\14ECI\13HCI\10OD"
     186:
     187: /*
     188:  * rmhr
     189:  *
     190:  * Emulex (i.e non DEC) controllers implement the ability to query for
     191:  * the drive geometry by placing these codes into the 'holding register'.
     192: */
     193: #define HPHR_MAXCYL 0x8017      /* max cylinder */
     194: #define HPHR_MAXTRAK    0x8018      /* max track/cylinder */
     195: #define HPHR_MAXSECT    0x8019      /* max sector/track */
     196:
     197: /* rmer2: These are the bits for an RM error register 2 */
     198: #define RMER2_BSE   0100000     /* bad sector error */
     199: #define RMER2_SKI   0040000     /* seek incomplete */
     200: #define RMER2_DPE   0020000     /* drive plug error */
     201: #define RMER2_IVC   0010000     /* invalid command */
     202: #define RMER2_LSC   0004000     /* loss of system clock */
     203: #define RMER2_LBC   0002000     /* loss of bit clock */
     204: /* bits 9-8 are unused */
     205: #define RMER2_DVC   0000200     /* device check */
     206: /* bits 6-4 are unused */
     207: #define RMER2_MDPE  0000010     /* MASSBUS data read parity error */
     208: /* bits 2-0 are unused */
     209:
     210: #define RMER2_BITS \
     211: "\10\20BSE\17SKI\16DPE\15IVC\14LSC\13LBC\10DVC\4MDPE"
     212:
     213: /* hpcs3 */
     214: #define HPCS3_APE   0100000     /* address parity error */
     215: #define HPCS3_DPE   0060000     /* data parity error */
     216: #define HPCS3_WCE   0017000     /* write check error */
     217: #define HPCS3_DW    0002000     /* double word */
     218: /* bits 9-8 are unused */
     219: #define HPCS3_IE    0000100     /* interrupt enable */
     220: /* bits 5-4 are unused */
     221: /* bits 3-0 are inverted parity check */
     222:
     223: #define HPCS3_BITS  \
     224: "\10\20APE\17DPE\15WCE\13DW\7IE"
     225:
     226: /*
     227:  * Systems Industries kludge: use value in
     228:  * the serial # register to figure out real drive type.
     229:  */
     230: #define SIMB_MB 0xff00      /* model byte value */
     231: #define SIMB_S6 0x2000      /* switch s6 */
     232: #define SIMB_LU 0x0007      /* logical unit (should = drive #) */
     233:
     234: #define SI9775D 0x0700      /* 9775 direct */
     235: #define SI9775M 0x0e00      /* 9775 mapped */
     236: #define SI9730D 0x0b00      /* 9730 or 9784 direct */
     237: #define SI9730M 0x0d00      /* 9730 or 9784 mapped */
     238: #define SI9766  0x0300      /* 9766 */
     239: #define SI9762  0x0100      /* 9762 */
     240: #define SICAPD  0x0500      /* Capricorn direct */
     241: #define SICAPN  0x0400      /* Capricorn mapped */
     242: #define SI9751D 0x0f00      /* Eagle direct */
     243:
     244: #define SIRM03  0x8000      /* RM03 indication */
     245: #define SIRM05  0x0000      /* RM05 pseudo-indication */

#### Defined struct's

hpdevice defined in line 21; used 36 times

- in /usr/src/sys/autoconfig/xpauto.c line 23(2)
- in /usr/src/sys/pdpstand/xp.c line 19-23(8), 32(2), 76(2), 176(2)
- in /usr/src/sys/pdpuba/xp.c line 60(2), 121-125(4), 139(2), 175(2), 440(2), 566(2), 670(2), 804(2), 957(2)

#### Defined macros

HPCS2_BAI defined in line 105; never used
HPCS2_BITS defined in line 108; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 737

HPCS2_CLR defined in line 103; used 2 times

- in /usr/src/sys/pdpstand/xp.c line 51
- in /usr/src/sys/pdpuba/xp.c line 190

HPCS2_DLT defined in line 93; never used
HPCS2_IR defined in line 102; never used
HPCS2_MDPE defined in line 100; never used
HPCS2_MXF defined in line 99; never used
HPCS2_NED defined in line 96; used 2 times

- in /usr/src/sys/pdpstand/xp.c line 49
- in /usr/src/sys/pdpuba/xp.c line 189

HPCS2_NEM defined in line 97; never used
HPCS2_OR defined in line 101; never used
HPCS2_PAT defined in line 104; never used
HPCS2_PGE defined in line 98; never used
HPCS2_UPE defined in line 95; never used
HPCS2_WCE defined in line 94; never used
HPCS3_APE defined in line 214; never used
HPCS3_BITS defined in line 223; never used
HPCS3_DPE defined in line 215; never used
HPCS3_DW defined in line 217; never used
HPCS3_IE defined in line 219; never used
HPCS3_WCE defined in line 216; never used
HPDS_ATA defined in line 113; never used
HPDS_BITS defined in line 129; never used
HPDS_DAE defined in line 119; never used
HPDS_DPR defined in line 120; used 1 times

- in line 127

HPDS_DREADY defined in line 127; used 6 times

- in /usr/src/sys/pdpuba/xp.c line 503(2), 614(2), 994(2)

HPDS_DRY defined in line 121; used 8 times

- in line 127
- in /usr/src/sys/pdpuba/xp.c line 628(2), 704, 757(2), 764(2)

HPDS_ERR defined in line 114; never used
HPDS_ILV defined in line 124; never used
HPDS_LST defined in line 118; never used
HPDS_MOL defined in line 116; used 1 times

- in line 127

HPDS_OM defined in line 125; never used
HPDS_PIP defined in line 115; used 3 times

- in /usr/src/sys/pdpuba/xp.c line 628, 757, 764

HPDS_VV defined in line 122; used 4 times

- in line 127
- in /usr/src/sys/pdpstand/xp.c line 86
- in /usr/src/sys/pdpuba/xp.c line 469, 988

HPDS_WRL defined in line 117; never used
HPDT_DRR defined in line 159; never used
HPDT_MH defined in line 157; never used
HPDT_NBA defined in line 155; never used
HPDT_RM02 defined in line 162; never used
HPDT_RM03 defined in line 165; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 238

HPDT_RM05 defined in line 164; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 238

HPDT_RM80 defined in line 163; never used
HPDT_RP04 defined in line 166; never used
HPDT_RP05 defined in line 167; never used
HPDT_RP06 defined in line 168; never used
HPDT_RP07 defined in line 169; never used
HPDT_TAPE defined in line 156; never used
HPER1_AOE defined in line 139; never used
HPER1_BITS defined in line 150; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 738

HPER1_DCK defined in line 133; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 750(2)

HPER1_DTE defined in line 136; never used
HPER1_ECH defined in line 142; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 750

HPER1_FER defined in line 144; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 714

HPER1_HCE defined in line 141; never used
HPER1_HCRC defined in line 140; never used
HPER1_IAE defined in line 138; never used
HPER1_ILF defined in line 148; never used
HPER1_ILR defined in line 147; never used
HPER1_OPI defined in line 135; never used
HPER1_PAR defined in line 145; never used
HPER1_RMR defined in line 146; never used
HPER1_UNS defined in line 134; never used
HPER1_WCF defined in line 143; never used
HPER1_WLE defined in line 137; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 705

HPHR_MAXCYL defined in line 193; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 216

HPHR_MAXSECT defined in line 195; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 213

HPHR_MAXTRAK defined in line 194; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 210

HPOF_BITS defined in line 184; never used
HPOF_ECI defined in line 173; never used
HPOF_FMT22 defined in line 172; used 5 times

- in /usr/src/sys/pdpstand/xp.c line 88
- in /usr/src/sys/pdpuba/xp.c line 471, 626, 855, 992

HPOF_HCI defined in line 174; never used
HPOF_M1200 defined in line 182; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 53(2)

HPOF_M400 defined in line 178; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 51(2)

HPOF_M800 defined in line 180; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 52(2)

HPOF_P1200 defined in line 181; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 53(2)

HPOF_P400 defined in line 177; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 51(2)

HPOF_P800 defined in line 179; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 52(2)

HP_BITS defined in line 67; never used
HP_BOOT defined in line 89; never used
HP_DCLR defined in line 75; used 4 times

- in /usr/src/sys/pdpstand/xp.c line 219
- in /usr/src/sys/pdpuba/xp.c line 754, 921, 990

HP_DVA defined in line 61; never used
HP_FORMAT defined in line 90; never used
HP_GO defined in line 66; used 20 times

- in /usr/src/sys/pdpstand/xp.c line 46, 87, 100, 219
- in /usr/src/sys/pdpuba/xp.c line 186, 470, 532(2), 627, 639, 754-756(2), 763, 838, 921, 990-991(2), 1011, 1021-1025(2)

HP_IE defined in line 64; used 12 times

- in /usr/src/sys/autoconfig/xpauto.c line 25
- in /usr/src/sys/pdpuba/xp.c line 449, 470, 532(2), 639, 754-756(2), 774, 782, 838, 856

HP_MCPE defined in line 59; never used
HP_NOP defined in line 71; used 3 times

- in /usr/src/sys/pdpstand/xp.c line 44, 207
- in /usr/src/sys/pdpuba/xp.c line 184

HP_OFFSET defined in line 77; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 627

HP_PACK defined in line 80; never used
HP_PRESET defined in line 79; used 3 times

- in /usr/src/sys/pdpstand/xp.c line 87
- in /usr/src/sys/pdpuba/xp.c line 470, 991

HP_RCOM defined in line 86; used 3 times

- in /usr/src/sys/pdpstand/xp.c line 102
- in /usr/src/sys/pdpuba/xp.c line 644-647(2)

HP_RDY defined in line 63; used 3 times

- in /usr/src/sys/autoconfig/xpauto.c line 25
- in /usr/src/sys/pdpstand/xp.c line 106
- in /usr/src/sys/pdpuba/xp.c line 838

HP_RECAL defined in line 74; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 756

HP_RELEASE defined in line 76; never used
HP_RHDR defined in line 87; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 642

HP_RTC defined in line 78; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 763

HP_SC defined in line 57; never used
HP_SEARCH defined in line 81; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 532

HP_SEEK defined in line 73; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 532

HP_TRE defined in line 58; used 6 times

- in /usr/src/sys/pdpstand/xp.c line 108
- in /usr/src/sys/pdpuba/xp.c line 703, 754, 783, 921, 1027

HP_UNLOAD defined in line 72; never used
HP_WCDATA defined in line 82; never used
HP_WCHDR defined in line 83; never used
HP_WCOM defined in line 84; used 5 times

- in /usr/src/sys/pdpstand/xp.c line 104
- in /usr/src/sys/pdpuba/xp.c line 644-649(2), 1011, 1021

HP_WHDR defined in line 85; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 642

RMER2_BITS defined in line 210; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 739

RMER2_BSE defined in line 198; used 1 times

- in /usr/src/sys/pdpuba/xp.c line 713

RMER2_DPE defined in line 200; never used
RMER2_DVC defined in line 205; never used
RMER2_IVC defined in line 201; never used
RMER2_LBC defined in line 203; never used
RMER2_LSC defined in line 202; never used
RMER2_MDPE defined in line 207; never used
RMER2_SKI defined in line 199; never used
SI9730D defined in line 236; never used
SI9730M defined in line 237; never used
SI9751D defined in line 242; never used
SI9762 defined in line 239; never used
SI9766 defined in line 238; never used
SI9775D defined in line 234; never used
SI9775M defined in line 235; never used
SICAPD defined in line 240; never used
SICAPN defined in line 241; never used
SIMB_LU defined in line 232; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 241

SIMB_MB defined in line 230; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 243

SIMB_S6 defined in line 231; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 243

SIRM03 defined in line 244; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 243

SIRM05 defined in line 245; used 1 times

- in /usr/src/sys/pdpstand/xp.c line 243

XP_CC defined in line 13; used 4 times

- in /usr/src/sys/pdpstand/xp.c line 137-140(3)
- in /usr/src/sys/pdpuba/xp.c line 518

XP_NOSEARCH defined in line 16; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 521, 531

rmer2 defined in line 49; used 2 times

- in /usr/src/sys/pdpuba/xp.c line 713, 739

rmhr defined in line 45; used 6 times

- in /usr/src/sys/pdpstand/xp.c line 210-217(6)

rmmr2 defined in line 47; never used

#### Usage of this include

hpreg.h used 3 times

- in /usr/src/sys/autoconfig/xpauto.c line 20
- in /usr/src/sys/pdpstand/xp.c line 13
- in /usr/src/sys/pdpuba/xp.c line 24

Last modified: 1995-07-21 Generated: 2016-12-26 | Generated by src2html V0.67 page hit count: 2004 |