# 2.11BSD#431 - /usr/src/sys/pdpuba/rkreg.h

##### Macros

    RKCS_BITS         X
    RKCS_DRESET       X
    RKCS_ERR          X
    RKCS_FMT          X
    RKCS_GO           X
    RKCS_HE           X
    RKCS_IDE          X
    RKCS_INHBA        X
    RKCS_RCHK         X
    RKCS_RCOM         X
    RKCS_RDY          X
    RKCS_RESET        X
    RKCS_SCP          X
    RKCS_SEEK         X
    RKCS_SSE          X
    RKCS_WCHK         X
    RKCS_WCOM         X
    RKCS_WLCK         X
    RKDA_SUR          X
    RKER_BITS         X
    RKER_CSE          X
    RKER_DLT          X
    RKER_DRE          X
    RKER_NXC          X
    RKER_NXD          X
    RKER_NXM          X
    RKER_NXS          X
    RKER_OVR          X
    RKER_PGE          X
    RKER_SKE          X
    RKER_TE           X
    RKER_WCE          X
    RKER_WLO          X
    RK_BITS           X
    RK_DPL            X
    RK_DRU            X
    RK_DRY            X
    RK_RK05           X
    RK_RWSRDY         X
    RK_SIN            X
    RK_SKC            X
    RK_SOK            X
    RK_WPS            X

##### struct's

    rkdevice          X

       1: /*
       2:  * Copyright (c) 1986 Regents of the University of California.
       3:  * All rights reserved.  The Berkeley software License Agreement
       4:  * specifies the terms and conditions for redistribution.
       5:  *
       6:  *	@(#)rkreg.h	1.1 (2.10BSD Berkeley) 12/1/86
       7:  */
       8:
       9: struct  rkdevice
      10: {
      11:     short   rkds;
      12:     short   rker;
      13:     short   rkcs;
      14:     short   rkwc;
      15:     caddr_t rkba;
      16:     short   rkda;
      17: };
      18:
      19: /* bits in rkds; all are read only */
      20: /* bits 15-13 are drive identification */
      21: #define RK_DPL      0010000     /* drive power low */
      22: #define RK_RK05     0004000     /* drive is an rk05; always 1 */
      23: #define RK_DRU      0002000     /* drive unsafe */
      24: #define RK_SIN      0001000     /* seek incomplete */
      25: #define RK_SOK      0000400     /* sector counter ok */
      26: #define RK_DRY      0000200     /* drive ready */
      27: #define RK_RWSRDY   0000100     /* read/write/seek ready */
      28: #define RK_WPS      0000040     /* write protect status */
      29: #define RK_SKC      0000020     /* seek complete */
      30: /* bits 3-0 are sector counter */
      31: #define RK_BITS     \
      32: "\10\15DPL\13DRU\12SIN\11SOK\10DRY\7RWSRDY\6WPS\5SKC"
      33:
      34: /* bits in rker; all are read only */
      35: #define RKER_DRE    0100000     /* drive error */
      36: #define RKER_OVR    0040000     /* overrun */
      37: #define RKER_WLO    0020000     /* write lock out violation */
      38: #define RKER_SKE    0010000     /* seek error */
      39: #define RKER_PGE    0004000     /* programming error */
      40: #define RKER_NXM    0002000     /* nonexistent memory */
      41: #define RKER_DLT    0001000     /* data late */
      42: #define RKER_TE     0000400     /* timing error */
      43: #define RKER_NXD    0000200     /* nonexistent disk */
      44: #define RKER_NXC    0000100     /* nonexistent cylinder */
      45: #define RKER_NXS    0000040     /* nonexistent sector */
      46: /* bits 4-2 are unused */
      47: #define RKER_CSE    0000002     /* checksum error */
      48: #define RKER_WCE    0000001     /* write check error */
      49: #define RKER_BITS   \
      50: "\10\20DRE\17OVR\16WLO\15SKE\14PGE\13NXM\12DLT\11TE\10NXD\
      51: \7NXC\6NXS\2CSE\1WCE"
      52:
      53: /* bits in rkcs */
      54: #define RKCS_ERR    0100000     /* error */
      55: #define RKCS_HE     0040000     /* hard error */
      56: #define RKCS_SCP    0020000     /* search complete */
      57: /* bit 12 is unused */
      58: #define RKCS_INHBA  0004000     /* inhibit bus address increment */
      59: #define RKCS_FMT    0002000     /* format */
      60: /* bit 9 is unused */
      61: #define RKCS_SSE    0000400     /* stop on soft error */
      62: #define RKCS_RDY    0000200     /* control ready */
      63: #define RKCS_IDE    0000100     /* interrupt on done enable */
      64: /* bits 5-4 are the UNIBUS extension bits */
      65: /* bits 3-1 is the command */
      66: #define RKCS_GO     0000001     /* go */
      67: #define RKCS_BITS   \
      68: "\10\20ERR\17HE\16SCP\15INHBA\14FMT\13SSE\12RDY\11IDE\1GO"
      69:
      70: /* commands */
      71: #define RKCS_RESET  0000000     /* control reset */
      72: #define RKCS_WCOM   0000002     /* write */
      73: #define RKCS_RCOM   0000004     /* read */
      74: #define RKCS_WCHK   0000006     /* write check */
      75: #define RKCS_SEEK   0000010     /* seek */
      76: #define RKCS_RCHK   0000012     /* read check */
      77: #define RKCS_DRESET 0000014     /* drive reset */
      78: #define RKCS_WLCK   0000016     /* write lock */
      79:
      80: /* bits in rkda */
      81: /* bits 15-13 are drive select */
      82: /* bits 12-5 are cylinder address */
      83: #define RKDA_SUR    0000020     /* surface */
      84: /* bits 3-0 are sector address */

#### Defined struct's

rkdevice defined in line 9; used 20 times

- in /usr/src/sys/autoconfig/rkauto.c line 16(2)
- in /usr/src/sys/pdpstand/rk.c line 19-23(8), 30(2)
- in /usr/src/sys/pdpuba/rk.c line 29(2), 47(2), 115(2), 149(2)

#### Defined macros

RKCS_BITS defined in line 67; never used
RKCS_DRESET defined in line 77; used 1 times

- in /usr/src/sys/autoconfig/rkauto.c line 19

RKCS_ERR defined in line 54; used 1 times

- in /usr/src/sys/pdpuba/rk.c line 160

RKCS_FMT defined in line 59; never used
RKCS_GO defined in line 66; used 4 times

- in /usr/src/sys/autoconfig/rkauto.c line 19
- in /usr/src/sys/pdpstand/rk.c line 43
- in /usr/src/sys/pdpuba/rk.c line 131, 174

RKCS_HE defined in line 55; never used
RKCS_IDE defined in line 63; used 2 times

- in /usr/src/sys/autoconfig/rkauto.c line 19
- in /usr/src/sys/pdpuba/rk.c line 131

RKCS_INHBA defined in line 58; never used
RKCS_RCHK defined in line 76; never used
RKCS_RCOM defined in line 73; used 2 times

- in /usr/src/sys/pdpstand/rk.c line 45
- in /usr/src/sys/pdpuba/rk.c line 133

RKCS_RDY defined in line 62; used 3 times

- in /usr/src/sys/pdpstand/rk.c line 49
- in /usr/src/sys/pdpuba/rk.c line 161, 175

RKCS_RESET defined in line 71; used 1 times

- in /usr/src/sys/pdpuba/rk.c line 174

RKCS_SCP defined in line 56; never used
RKCS_SEEK defined in line 75; never used
RKCS_SSE defined in line 61; never used
RKCS_WCHK defined in line 74; never used
RKCS_WCOM defined in line 72; used 2 times

- in /usr/src/sys/pdpstand/rk.c line 47
- in /usr/src/sys/pdpuba/rk.c line 135

RKCS_WLCK defined in line 78; never used
RKDA_SUR defined in line 83; never used
RKER_BITS defined in line 49; used 1 times

- in /usr/src/sys/pdpuba/rk.c line 172

RKER_CSE defined in line 47; never used
RKER_DLT defined in line 41; never used
RKER_DRE defined in line 35; never used
RKER_NXC defined in line 44; never used
RKER_NXD defined in line 43; never used
RKER_NXM defined in line 40; never used
RKER_NXS defined in line 45; never used
RKER_OVR defined in line 36; never used
RKER_PGE defined in line 39; never used
RKER_SKE defined in line 38; never used
RKER_TE defined in line 42; never used
RKER_WCE defined in line 48; never used
RKER_WLO defined in line 37; used 1 times

- in /usr/src/sys/pdpuba/rk.c line 163

RK_BITS defined in line 31; used 1 times

- in /usr/src/sys/pdpuba/rk.c line 173

RK_DPL defined in line 21; never used
RK_DRU defined in line 23; never used
RK_DRY defined in line 26; never used
RK_RK05 defined in line 22; never used
RK_RWSRDY defined in line 27; never used
RK_SIN defined in line 24; never used
RK_SKC defined in line 29; never used
RK_SOK defined in line 25; never used
RK_WPS defined in line 28; never used

#### Usage of this include

rkreg.h used 3 times

- in /usr/src/sys/autoconfig/rkauto.c line 13
- in /usr/src/sys/pdpstand/rk.c line 14
- in /usr/src/sys/pdpuba/rk.c line 22

Last modified: 1987-01-09 Generated: 2016-12-26 | Generated by src2html V0.67 page hit count: 677 |