# 2.11BSD#431 - /usr/src/sys/vaxif/if_ilreg.h

##### Variables

    ildiag            X
    ilerrs            X

##### Macros

    ILC_ALLMC         X
    ILC_CALLMC        X
    ILC_CISA          X
    ILC_CLPBAK        X
    ILC_CLPRMSC       X
    ILC_CRCVERR       X
    ILC_DEFPA         X
    ILC_DELAYS        X
    ILC_DIAG          X
    ILC_FLUSH         X
    ILC_ILPBAK        X
    ILC_ISA           X
    ILC_LDGRPS        X
    ILC_LDPA          X
    ILC_LDXMIT        X
    ILC_MLPBAK        X
    ILC_OFFLINE       X
    ILC_ONLINE        X
    ILC_PRMSC         X
    ILC_RCV           X
    ILC_RCVERR        X
    ILC_RESET         X
    ILC_RMGRPS        X
    ILC_STAT          X
    ILC_XMIT          X
    ILDIAG_CHKSUMERR  X
    ILDIAG_DMAERR     X
    ILDIAG_LOOPBACK   X
    ILDIAG_RECVERR    X
    ILDIAG_SUCCESS    X
    ILDIAG_XMITERR    X
    ILERR_BADCMD      X
    ILERR_BUFALIGNMENTX
    ILERR_BUFSIZ      X
    ILERR_COLLISIONS  X
    ILERR_FRAMESIZ    X
    ILERR_INVCMD      X
    ILERR_NXM         X
    ILERR_RECVERR     X
    ILERR_RETRIES     X
    ILERR_SUCCESS     X
    ILFSTAT_A         X
    ILFSTAT_C         X
    ILFSTAT_L         X
    IL_BITS           X
    IL_CDONE          X
    IL_CIE            X
    IL_CMD            X
    IL_EUA            X
    IL_RDONE          X
    IL_RIE            X
    IL_STATUS         X
    NILDIAGS          X
    NILERRS           X

##### struct's

    ildevice          X

       1: /*
       2:  * Copyright (c) 1982, 1986 Regents of the University of California.
       3:  * All rights reserved.  The Berkeley software License Agreement
       4:  * specifies the terms and conditions for redistribution.
       5:  *
       6:  *	@(#)if_ilreg.h	7.1 (Berkeley) 6/5/86
       7:  */
       8:
       9: /*
      10:  * Interlan Ethernet Communications Controller interface
      11:  */
      12: struct ildevice {
      13:     short   il_csr;     /* Command and Status Register */
      14:     short   il_bar;     /* Buffer Address Register */
      15:     short   il_bcr;     /* Byte Count Register */
      16: };
      17:
      18: /*
      19:  * Command and status bits
      20:  */
      21: #define IL_EUA      0xc000      /* Extended Unibus Address */
      22: #define IL_CMD      0x3f00      /* Command Function Code */
      23: #define IL_CDONE    0x0080      /* Command Done */
      24: #define IL_CIE      0x0040      /* Command Interrupt Enable */
      25: #define IL_RDONE    0x0020      /* Receive DMA Done */
      26: #define IL_RIE      0x0010      /* Receive Interrupt Enable */
      27: #define IL_STATUS   0x000f      /* Command Status Code */
      28:
      29: #define IL_BITS     "\20\10CDONE\7CIE\6RDONE\5RIE"
      30:
      31: /* command definitions */
      32: #define ILC_MLPBAK  0x0100      /* Set Module Interface Loopback Mode */
      33: #define ILC_ILPBAK  0x0200      /* Set Internal Loopback Mode */
      34: #define ILC_CLPBAK  0x0300      /* Clear Loopback Mode */
      35: #define ILC_PRMSC   0x0400      /* Set Promiscuous Receive Mode */
      36: #define ILC_CLPRMSC 0x0500      /* Clear Promiscuous Receive Mode */
      37: #define ILC_RCVERR  0x0600      /* Set Receive-On-Error Bit */
      38: #define ILC_CRCVERR 0x0700      /* Clear Receive-On-Error Bit */
      39: #define ILC_OFFLINE 0x0800      /* Go Offline */
      40: #define ILC_ONLINE  0x0900      /* Go Online */
      41: #define ILC_DIAG    0x0a00      /* Run On-board Diagnostics */
      42: #define ILC_ISA     0x0d00      /* Set Insert Source Address Mode */
      43: #define ILC_CISA    0x0e00      /* Clear Insert Source Address Mode */
      44: #define ILC_DEFPA   0x0f00      /* Set Physical Address to Default */
      45: #define ILC_ALLMC   0x1000      /* Set Receive All Multicast Packets */
      46: #define ILC_CALLMC  0x1100      /* Clear Receive All Multicast */
      47: #define ILC_STAT    0x1800      /* Report and Reset Statistics */
      48: #define ILC_DELAYS  0x1900      /* Report Collision Delay Times */
      49: #define ILC_RCV     0x2000      /* Supply Receive Buffer */
      50: #define ILC_LDXMIT  0x2800      /* Load Transmit Data */
      51: #define ILC_XMIT    0x2900      /* Load Transmit Data and Send */
      52: #define ILC_LDGRPS  0x2a00      /* Load Group Addresses */
      53: #define ILC_RMGRPS  0x2b00      /* Delete Group Addresses */
      54: #define ILC_LDPA    0x2c00      /* Load Physical Address */
      55: #define ILC_FLUSH   0x3000      /* Flush Receive BAR/BCR Queue */
      56: #define ILC_RESET   0x3f00      /* Reset */
      57:
      58: /*
      59:  * Error codes found in the status bits of the csr.
      60:  */
      61: #define ILERR_SUCCESS       0   /* command successful */
      62: #define ILERR_RETRIES       1   /* " " with retries */
      63: #define ILERR_BADCMD        2   /* illegal command */
      64: #define ILERR_INVCMD        3   /* invalid command */
      65: #define ILERR_RECVERR       4   /* receiver error */
      66: #define ILERR_BUFSIZ        5   /* buffer size too big */
      67: #define ILERR_FRAMESIZ      6   /* frame size too small */
      68: #define ILERR_COLLISIONS    8   /* excessive collisions */
      69: #define ILERR_BUFALIGNMENT  10  /* buffer not word aligned */
      70: #define ILERR_NXM       15  /* non-existent memory */
      71:
      72: #define NILERRS         16
      73: #ifdef ILERRS
      74: char *ilerrs[NILERRS] = {
      75:     "success",          /*  0 */
      76:     "success with retries",     /*  1 */
      77:     "illegal command",      /*  2 */
      78:     "inappropriate command",    /*  3 */
      79:     "failure",          /*  4 */
      80:     "buffer size exceeded",     /*  5 */
      81:     "frame too small",      /*  6 */
      82:     0,              /*  7 */
      83:     "excessive collisions",     /*  8 */
      84:     0,              /*  9 */
      85:     "buffer alignment error",   /* 10 */
      86:     0,              /* 11 */
      87:     0,              /* 12 */
      88:     0,              /* 13 */
      89:     0,              /* 14 */
      90:     "non-existent memory"       /* 15 */
      91: };
      92: #endif
      93:
      94: /*
      95:  * Diagnostics codes.
      96:  */
      97: #define ILDIAG_SUCCESS      0   /* no problems */
      98: #define ILDIAG_CHKSUMERR    1   /* ROM/RAM checksum error */
      99: #define ILDIAG_DMAERR       2   /* DMA not working */
     100: #define ILDIAG_XMITERR      3   /* xmit circuitry failure */
     101: #define ILDIAG_RECVERR      4   /* rcvr circuitry failure */
     102: #define ILDIAG_LOOPBACK     5   /* loopback test failed */
     103:
     104: #define NILDIAGS        6
     105: #ifdef ILDIAGS
     106: char *ildiag[NILDIAGS] = {
     107:     "success",          /* 0 */
     108:     "checksum error",       /* 1 */
     109:     "NM10 dma error",       /* 2 */
     110:     "transmitter error",        /* 3 */
     111:     "receiver error",       /* 4 */
     112:     "loopback failure",     /* 5 */
     113: };
     114: #endif
     115:
     116: /*
     117:  * Frame status bits, returned in frame status byte
     118:  * at the top of each received packet.
     119:  */
     120: #define ILFSTAT_C   0x1     /* CRC error */
     121: #define ILFSTAT_A   0x2     /* alignment error */
     122: #define ILFSTAT_L   0x4     /* 1+ frames lost just before */

#### Defined variables

ildiag defined in line 106; never used
ilerrs defined in line 74; never used

#### Defined struct's

ildevice defined in line 12; never used

#### Defined macros

ILC_ALLMC defined in line 45; never used
ILC_CALLMC defined in line 46; never used
ILC_CISA defined in line 43; never used
ILC_CLPBAK defined in line 34; never used
ILC_CLPRMSC defined in line 36; never used
ILC_CRCVERR defined in line 38; never used
ILC_DEFPA defined in line 44; never used
ILC_DELAYS defined in line 48; never used
ILC_DIAG defined in line 41; never used
ILC_FLUSH defined in line 55; never used
ILC_ILPBAK defined in line 33; never used
ILC_ISA defined in line 42; never used
ILC_LDGRPS defined in line 52; never used
ILC_LDPA defined in line 54; never used
ILC_LDXMIT defined in line 50; never used
ILC_MLPBAK defined in line 32; never used
ILC_OFFLINE defined in line 39; never used
ILC_ONLINE defined in line 40; never used
ILC_PRMSC defined in line 35; never used
ILC_RCV defined in line 49; never used
ILC_RCVERR defined in line 37; never used
ILC_RESET defined in line 56; never used
ILC_RMGRPS defined in line 53; never used
ILC_STAT defined in line 47; never used
ILC_XMIT defined in line 51; never used
ILDIAG_CHKSUMERR defined in line 98; never used
ILDIAG_DMAERR defined in line 99; never used
ILDIAG_LOOPBACK defined in line 102; never used
ILDIAG_RECVERR defined in line 101; never used
ILDIAG_SUCCESS defined in line 97; never used
ILDIAG_XMITERR defined in line 100; never used
ILERR_BADCMD defined in line 63; never used
ILERR_BUFALIGNMENT defined in line 69; never used
ILERR_BUFSIZ defined in line 66; never used
ILERR_COLLISIONS defined in line 68; never used
ILERR_FRAMESIZ defined in line 67; never used
ILERR_INVCMD defined in line 64; never used
ILERR_NXM defined in line 70; never used
ILERR_RECVERR defined in line 65; never used
ILERR_RETRIES defined in line 62; never used
ILERR_SUCCESS defined in line 61; never used
ILFSTAT_A defined in line 121; never used
ILFSTAT_C defined in line 120; never used
ILFSTAT_L defined in line 122; never used
IL_BITS defined in line 29; never used
IL_CDONE defined in line 23; never used
IL_CIE defined in line 24; never used
IL_CMD defined in line 22; never used
IL_EUA defined in line 21; never used
IL_RDONE defined in line 25; never used
IL_RIE defined in line 26; never used
IL_STATUS defined in line 27; never used
NILDIAGS defined in line 104; used 1 times

- in line 106

NILERRS defined in line 72; used 1 times

- in line 74

Last modified: 1986-06-05 Generated: 2016-12-26 | Generated by src2html V0.67 page hit count: 311 |