MSRP Pricing |  |
| LINK MC5 Terminal The Link MC5 is the most advanced "multiple concept" display terminal and has some very visible differences. It offers high performance, plus ergonomics that are easy on the eyes. At a price that's very easy on the budget. The Link MC5's improved features includes a flat profile screen to reduce glare, overscanned video to eliminate distracting dark borders, extra fast 78 Hz refresh rate to eliminate screen flicker, contrast and brightness controls located on the front panel for easy access: Ergonomics with a clear difference. The MC5 also emulates ASCII (Wyse, TeleVideo, Zentec/ADM and ADDS); ANSI (DEC VT220/VT100/VT52); and PCTerm. The MC5 has interchangeable keyboards, a parallel printer port, and lets you communicate with any two hosts. Designed to keep functionality at its highest, and your overall system costs at their lowest. The Link MC5. Carrying on the tradition of high quality and flawless performance that you've come to expect from Link terminals. Value that's a step ahead of the competition. At a price that's a step below. MC5 Features: ASCII, ANSI, PCTerm, SCO Console Virtual Terminals Communicates with two different hosts Interchangeable Keyboards (EPC, ANSI, ASCII) Two Serial Ports and a PC Compatible Parallel Printer Port 78 Hz Refresh External Brightness and Contrast Controls Flat Screen Green, Amber, or White Screen Color with Full Overscan 24, 25 or 43 Line Display 80 or 132 Columns 512 Displayable Characters Designed for use with a wide range of multiuser systems, including PC MOS, Alloy, Unix/Xenix, Pick, Concurrent DOS and THEOS MC5 Specifications Display Screen: 14" diagonal flat screen, green, amber, or white phosphor with fully overscanned video Screen Refresh: 78 Hz or 60 Hz, selectable Screen Formats: 24, 25 or 43 scrollable lines plus 1 status line, 80 or 132 columns Virtual Terrninals: Simultaneous connection to two different hosts Screen Attributes: Normal, Dim, Bold, Blank, Reverse, Underscore, Blink and protect attributes in all combinations. Video attributes can be set for embedded, non-embedded, line or character. Horizontal split screen and scrolling regions. External brightness and contrast controls Line Attributes: Double high, double wide Character Cell Size: 10x16 (60 Hz); 10x13 (78 Hz) Character Set: 512 displayable characters. 7 resident character sets including ASCII, DEC Multinational, DEC Special Graphics, PC Multinational, and soft font Display Memory: Up to 7 pages screen memory (80 column, embedded mode) Terminal Set-up: Full-page Menu, non-volatile Cursor Attributes: Blinking or steady, block or underline, cursor or no cursor Scrolling: Jump or smooth scroll-3 speeds, software selectable Keyboards: ASCII, Enhanced PC or ANSI. Detached, adjustable low profile with 6-foot coiled RJ11 cord. 450 bytes NVM for function key memory and answerback Communications: Main Port RS232C up to 115.2K bps Aux Port RS232 (Optional RS422) up to 115.2K bps Parallel Port: IBM PC Compatible Software Compatibility: Wyse WY60, WY50+; Televideo 910+, 925, 950, 955; Zentec ADM 3A, 5; ADDS Viewpoint, Viewpoint 60; DEC VT220/100/52; ANSI.SYS (SCO console), Word Perfect keyboard support and PCTerm Power: Auto-sensing 120 to 240 VAC + 10%, 47 to 63 Hz Dimensions: Height:12.5 inches (31.75cm); Depth: 12.2 inches (30.99 cm); Width: 13.3 inches (33.78 cm); Footprint: 9.5 inches (20.90 cm) Shipping Weight: Terminal: 22 pounds Regulatory: UL, CSA, TÜV-GS, FCC-A Note: The keyboard is not included with the terminal and must be ordered separately.
| (800) GET-WYSE | (408) 473-1200 Privacy Notice HOME | Winterm Thin Clients | Wyse Solutions | Industry Alliances Service & Support | General Purpose Terminals | Wyse Partners About Wyse | Contact Us | In the News | Search | Site Map | Find Resellers © Copyright 1996-1999 Wyse Technology, Inc.