





                       GETTING OF THE AIR WITH RSX-11/IAS RUNOFF

 
       I.  Building RUNOFF



        1.0  RSX-11M




        1.1  RSX
-11M MAPPED SYSTEMS


        All command files follow the standard RSX-11M c
onventions.

             1.  [100,10] should contain all source modules.

 
            2.  [100,20] should contain the  file  RNOASM.CMD.   [1,24]
       
          will receive the object output files.

             3.  [100,30] wil
l receive listing files.

             4.  [1,24] should contain the file RNOB
LM.ODL

             5.  [1,24] should contain the file RNOBLM.CMD

        
     6.  [1,34] will receive the map output file.

             7.  [1,54] wil
l receive the task image file.

        Procedure:

             1.  Use UFD
 to set up the proper UFDs, if necessary.   Note
                 that all comm
and files must be changed if you do not do
                 this.

          
   2.  Use FLX to move the files to their proper UICs.

             3.  Set t
he UIC to [1,24] and assemble.
                   SET /UIC=[1,24]
            
       MAC @[100,20]RNOASM

             4.  Use PIP to construct a concatenat
ed object file for all
                 RNO files:
                   PIP>RNO.
OBS=*.OBJ

             5.  Build a library containing the RNO object files:
                   LBR>RNO/CR=RNO.OBS

             6.  Build the task image f
ile.  The map will go  to  [1,34]
                 and the task image to [1,54]
.
                  TKB @[1,24]RNOBLM

        Alternatively, you  may  use  
the  indirect  MCR  command  file,


                                         
                         PAGE 2



        [1,24]RNO11MM.CMD, to perform the
se steps after transferring the
        files to the proper UFDs (i.e.  [1,24]R
NO11MM.CMD  will  perform
        steps  3 through 6).  You will probably have 
to edit the command
        files to match installation dependent conditions.



        1.2  RSX-11M UNMAPPED SYSTEMS


        All command files follo
w the standard RSX-11M conventions.

             1.  [100,10] should contain 
all source modules.

             2.  [100,20] should contain the  file  RNOAS
M.CMD.   [1,20]
                 will receive the object output files.

     
        3.  [100,30] will receive listing files.

             4.  [1,20] shou
ld contain the file RNOBLM.ODL

             5.  [1,20] should contain the fil
e RNOBLU.CMD

             6.  [1,30] will receive the map output file.

   
          7.  [1,50] will receive the task image file.

        Procedure:

             1.  Use UFD to set up the proper UFDs, if necessary.   Note
      
           that all command files must be changed if you do not do
            
     this.

             2.  Use FLX to move the files to their proper UICs.

             3.  Set the UIC to [1,20] and assemble.
                   SET /
UIC=[1,20]
                   MAC @[100,20]RNOASM

             4.  Use PIP t
o construct a concatenated object file for all
                 RNO files:
   
                PIP>RNO.OBS=*.OBJ

             5.  Build a library containing
 the RNO object files:
                   LBR>RNO/CR=RNO.OBS

             6.
  Build the task image file.  The map will go  to  [1,30]
                 and 
the task image to [1,50].
                  TKB @[1,20]RNOBLU

        Altern
atively, you  may  use  the  indirect  MCR  command  file,
        [1,20]RNO11M
U.CMD, to perform these steps after transferring the
        files to the prope
r UFDs (i.e.  [1,20]RNO11MU.CMD  will  perform
        steps  3 through 6).  Yo
u will probably have to edit the command
        files to match installation de
pendent conditions.


                                                        
          PAGE 3



        2.0  RSX-11D


        All command files foll
ow the standard RSX-11D conventions.

             1.  [311,25] should contain
 all source modules.

             2.  [311,25] should contain the file RNOMAC
D.CMD.   [11,25]
                 will receive the object output files.

    
         3.  [211,25] will receive listing files.

             4.  [11,25] sh
ould contain the file RNOBLD.ODL

             5.  [11,25] should contain the 
file RNOBLD.CMD

             6.  [111,25] will receive the map output file.

             7.  [11,1] will receive the task image file.

        Procedure
:

             1.  Use UFD to set up the proper UFDs, if necessary.   Note
 
                that all command files must be changed if you do not do
       
          this.

             2.  Use FLX to move the files to their proper UI
Cs.

             3.  Set the UIC to [11,25] and assemble.
                  
 SET /UIC=[11,25]
                   MAC @[311,25]RNOMACD

             4.  U
se PIP to construct a concatenated object file for all
                 RNO fil
es:
                   PIP>RNO.OBS=*.OBJ

             5.  Build a library co
ntaining the RNO object files:
                   LBR>RNO/CR=RNO.OBS

       
      6.  Build the task image file.  The map will go to [111,25]
             
    and the task image to [11,1].
                  TKB @[11,25]RNOBLD

     
   Alternatively,   you   may   use   the   Batch    input    file,
        [11
,25]RNO11D.BIS, to perform these steps after transferring the
        files to 
the proper UFDs (i.e.  [11,25]RNO11D.BIS  will  perform
        steps 3 through
 6).  You will probably have to edit the files to
        match installation de
pendent conditions.


                                                        
          PAGE 4



        3.0  IAS


        IAS users have  the  optio
n  of  following  the  procedures  for
        RSX-11D  under  MCR or of using 
the following PDS commands.  All
        command files follow the standard IAS 
conventions.

             1.  [311,25] should contain all source modules.

             2.  [311,25] should contain the file RNOMACI.CMD.   [11,25]
      
           will receive the object output files.

             3.  [211,25] wi
ll receive listing files.

             4.  [11,25] should contain the file RN
OBLD.ODL

             5.  [11,25] should contain the file RNOBLI.CMD

     
        6.  [111,25] will receive the map output file.

             7.  [11,1
] will receive the task image file.

        Procedure:

             1.  Th
e system manager should use SCI>CREATE to set up  the
                 proper U
FDs, if necessary.  Note that all command files
                 must be change
d if you do not do this.

             2.  Use COPY to move the files to their
 proper UICs.

             3.  Set the UIC to [11,25] and assemble.
        
           SET DEFAULT [11,25]
                   PDS> @[311,25]RNOMACI

    
         4.  Use COPY to construct a concatenated  object  file  for
          
       all RNO files:
                   COPY *.OBJ RNO.OBS

             5. 
 Build a library containing the RNO object files:
                   LIBRARIAN/
CREATE RNO RNO.OBS

             6.  Build the task image file.  The map will 
go to [111,25]
                 and the task image to [11,1].
                
  PDS>@[11,25]RNOBLI

        Alternatively,   you   may   use   the   Batch  
  input    file,
        [11,25]RNOIAS.BIS,   or   the   PDS   indirect   comma
nd   file,
        [11,25]RNOIAS.CMD, to perform these steps after transferring
 the
        files   to   the   proper   UFDs  (i.e.   [11,25]RNOIAS.BIS  and
        [11,25]RNOIAS.CMD will perform steps 3  through  6).   You  will
      
  probably  have to edit the files to match installation dependent
        cond
itions.


                                                                  PA
GE 5



        II.  RUNOFF Documentation

        Runoff is documented in
 the file, RUNOFF.RNO  which  you  should
        transfer  to the same UFD as 
the source files.  You may then ob-
        tain a copy of the RUNOFF manual, b
y installing  RUNOFF  (RUNOFF
        has  the  task name ...RNO under RSX-11M/
D and $$$RNO under IAS,
        so it may be run as an MCR command (PDS Library
 Task under IAS),
        and  then  issuing one of the following command lines
 or equiva-
        lent:

        RSX-11M:

         MCR>RNO LP:=[100,10]R
UNOFF

        RSX-11D:
         MCR>RNO LP:=[311,25]RUNOFF

        IAS:
         PDS>RNO LP:=[311,25]RUNOFF




