These are corrections/enhancements to two programs in the KMS-FUSION set.
Jim Downward has been given these and he might also put them in
his next release.

My system is a straight base-level 26, so his CKP did not work. Thes one
here does, and it does a good job, especially in kicking out
the que-manager, de-spoolers, and RMD if they happen to be in the middle
of GEN (which does happen when there are a lot uf users working.)

This CVL adds another switch, plus will let a non-privileged user read a
volume label of a disk he has allocated. When we switched from IAS to
M3.2, nobody could mount their RK-05 disks, because of not knowing the
volume labels.

	Ray Van Tassle
	Motorola
	1301 E. Algonquin Rd.
	Room 4135
	Schaumburg, Ill.
	(312)-576-6017
