.PAGE SIZE 60,85
.LEFT MARGIN 10
.RIGHT MARGIN 75
.AUTOPARAGRAPH
	This  distribution  kit  contains  the  RSX-11M/M-Plus  user
monitor files.  Note that this version of the monitor was
upgraded with the release of RSX-11M V4.0 and M-Plus V2.0.
	This distribution corrects bugs in the version 
distributed in the Multi-Tasker and corrects the deficiency which
prevented the monitor from logging out its own TI: .  The problem
of the monitor logging out terminals remoted to other systems
via DECnet RMT/RMTACP has also been corrected - but only works
on the new versions of RSX, as it requires the GCII$ directive.
Problems with the monitor refusing to log out the last logged-in
terminal on the system have also been (hopefully) finally eliminated.
	This version introduces time limiting.  This
means that the monitor may be built to run only during time periods
specified at generation time.  This may be 
useful to sites which do not wish to log idle terminals out during
normal working hours.
	To build the monitor, log in on a privileged account and copy the
distribution files into a chosen UIC.  Invoke the build command
file, USERGEN.   This command file is reasonably intelligent,
UIC-independent, and is usually able to build a task without
intervention.  If this is not the case, it may  be  necessary  to
run  the  command  file  with  the /-MC switch and build
manually from the produced build command files.
	Users of RSX-11M V3.2 / M-Plus V1.0 systems or earlier,
take note.  The build command file uses some features released in the
M V4.0 / M-Plus V2.0 Indirect which may not be available on older
versions of RSX.  This means there may be difficulties which require
manual intervention.
.SKIP 4
.LEFT MARGIN +25
.NO FILL
.NO JUSTIFY
Bruce R. Mitchell
Machine Intelligence and Industrial Magic
PO Box 601
Hudson, Wisconsin
54016
