README.1ST	[310,7]

Intel 8080/8085 cross assembler. Uses the Intel input and output format but
allows for 12 character names. Optional Cross reference output. Modified from
an 1802 package from Dofasco Ltd.
