README.1ST	[310,1]

Assorted Fortran files on this account from TARLUG:

CPU		- Taken from the Spring '83 US RSX tape [370,1] and modified
		  to run on a VT100 or equivalent and give a full 0-100% range
		  on an 11/44 with M-Plus.

DISKUSAGE
SNAPDISK	- Two versions of a program to spawn PIP to determine the
		  disk usage by account. DISKUSAGE reports to the logfile
		  and SNAPDISK spools to the line printer. Both rely on an
		  account file set up to have seperate group values for each
		  account. These programs sum the disk blocks allocated over
		  all members of an account group.

DTCCHECK	- Routine to spawn to the Indirect Command File Processor a
DTC.CMD		  command file to check the calendar for the users and prompt
		  them of upcoming appointments.. This program will usually
		  be placed in the clock queue to run at some predetermined
		  time. The command file and DTC are setup to run every 30
		  minutes. 

GETPORT		  Routine to spawn to the Indirect Command File Processor a
PORTSTAT.CMD	  command file to check the status of a user specified port.
		  It determines	(from the exit status) from ICP that the port
		  is Logged in or not, allocated, or attached. If none of these
		  is the case, The baud rate is asked for and set. The primary
		  use is to be able to remotely dial out of the system using
		  the TALK program and an auto-bauding auto-dial modem such as
		  the RIXON 212A.

LISTEN		- Prints on the issuing terminal all input to a specified
		  terminal port. All characters received are displayed,
		  including control characters. I have found this program
		  simple but invaluable in testing RS232 equipment.

SCREEN		- A program that uses the Get CLI Information (GCII) directive
		  to determine the logged out terminals and to write to those
		  terminals, their terminal number, Time of day, and number
		  of users logged on. This is written at the top line of
		  the crt and is walked across the line. I have this run
		  every minute. Off working hours it just clears the screen
		  of every logged off terminal.

SHOWTASK	- Routine to Show the attributes of a task image. Information
		  displayed:

			Name
			Partition
			Task Ident
			Size
			Creation date
			Priority
			Number of Luns
			Libraries
			Attributes including:	privileged	checkpointable
				generates_pmd	external_header	contains_pic
				memory_overlays	maps_i/o_page
		  Output can be directed to a file to facilitate a command file
		  scanning the output files searching for a given pattern

SINGLETKB	- A simple program to prevent multiple copies of TKB from
		  running on the system. Applies to BP2 and F77 as well.

T2T		- Another tape to tape program. Does a fast tape to tape
		  copy of any structured tape that ends with an EOV as all
		  tapes should do. Will even handle the large (32256) VMS
		  backup tapes.

