                             
spacewar 4.8  7/24/63 dfw  _ pt 1

3/	jmp sbf		/ ignore seq. break
	jmp a40
	nop


/ interesting and often changed constants

/symb loc   usual value (all instructions are executed,
	/ and may be replaced by jda or jsp)

tno,  6,	law i 41 	/ number of torps + 1
tvl,  7,	sar 4s	/ torpedo velocity
rlt, 10,	law i 20	/ torpedo reload time
tlf, 11,	law i 140	/ torpedo life
foo, 12,	-20000	/ fuel supply
maa, 13,	40	/ spaceship angular acceleration
sac, 14,	sar 4s	/ spaceship acceleration
str, 15,	100	/ star capture radius
me1, 16,	6000	/ collision "radius"
me2, 17,	3000	/ above/2
ddd, 20,	-0	/ 0 to save space for ddt
the, 21,	sar 9s	/ amount of torpedo space warpage
mhs, 22,	law i 10	/ number of hyperspace shots
hd1, 23,	law i 40	/ time in hyperspace before breakout
hd2, 24,	law i 100	/ time in hyperspace breakout
hd3, 25,	law i 200	/ time to recharge hyperfield generators
hr1, 26,	scl 9s	/ scale on hyperspatial displacement
hr2, 27,	scl 4s	/ scale on hyperspatially induced velocity
hur, 30,	40000	/ hyperspatial uncertancy
ran, 31,	0	/ random number
grv, 32,	sar 6s	/ gravitational constant

/ place to build a private control word routine.  
/ it should leave the control word in the io as follows_.
/ high order 6 bits, high acceleration, normal acceleration,
/ rotate cw, rotate ccw, fire torpedo, and hyperspace.
/ Routine is entered by jsp cwg for ss1 and by jsp dwg
/ for ss2.

40/

cwr,	jmp mg1	/ normally iot 11 control
dwr,	jmp mg2	/ normally iot 111 control
. 20/	/ space
          
                                                                  
/ routine to flush sequence breakes, if they occur.

sbf,	tyi
	lio 2
	lac 0
	lsm
	jmp i 1

	define
xincr X,Y,INS
	lac Y
	INS .ssn
	dac Y
	lac X
	INS .scn
	dac X
	term

	define
yincr X,Y,INS
	lac Y
	INS .scn
	dac Y
	lac X
	-INS+add+sub .ssn
	dac X
	terminate

	define
dispatch
	add (. 3
	dap . 1
	jmp .
	term

	define
dispt A,Y,B
	repeat 6	B=B+B
	lio Y
	dpy-A+B
	term

	define
scale A,B,C
	lac A
	sar B
	dac C
	term
          
                                                                 
	defin
diff V,S,SF
	add i V
	dac i V
	xct SF
	add i S
	dac i S
	term


	define
random
	lac ran
	rar 1s
	xor (355670
	add (355670
	dac ran
	term

	define
ranct S,SS,C
	random
	S
	SS
	sma
	cma
	dac C
	terminate
          
                                                                 
define
	varsft
	dzm .xys
	dac .t1
	idx .xys
v2,	idx .xys
	lac .t1
	scr 2s
	dac .t1
	sza
	jmp v2+R
	scr 2s
	swap
	terminate
define
	undosft
	dac t1
	dio .t2
	lac .xys
	add stb
	dap .+1
	lac .
	dac .+6
	dac .+6
	xor (10000	/ change scr to scl or scl to scr.
	dac .xyt
	lac .t1
	dio .t2
	scr .
	scr .
	terminate
define
	integrate A,B
	cli
	lac i A
	scr 9s
	scr 1s
	div .t1
	hlt
	cma+cli-opr
	xct .xyt
	xct grv
	dac B
	terminate

stb,	lac .-1
	scr 7s
	scr 6s
	scr 5s
	scr 4s
	scr 3s
	scr 2s
	scr 1s
	scr
	scl 1s
          
                                                                  
/sine-cosine subroutine_ Adams associates
/calling sequence= number in AC, jda sin or jdacos.
/argument is between .+2 pi, with binary point to right of bit 3.
/answer has binary point to right bit 0.  Time = 2.35-? ms.
/changed for auto-multiply , ddp 1/19/63

cos,	0
	dap csx
	lac (62210
	add cos
	dac sin
	jmp .+4

sin,	0
	dap csx
	lac sin
	spa
si1,	add (311040
	sub (62210
	sma
	jmp si2
	add (62210

si3,	ral 2s
	mul (242763
	dac sin
	mul sin
	dac cos
	mul (756103
	add (121312
	mul cos
	add (532511
	mul cos
	add (144417
	mul sin
	scl 3s
	dac cos
	xor sin
	sma
	jmp csx-1
	lac (377777
	lio sin
	spi
	cma
	jmp csx

	lac cos
csx,	jmp .

si2,	cma
	add (62210
	sma
	jmp si3
	add (62210
	spa
	jmp .+3
	sub (62210
	jmp si3

	sub (62210
	jmp si1
          
                                                                 
/integer square root
/input in ac, binary point to right of bit 17, jda sqt
/answer in ac with binary point between bits 8 and 9
/largest input number = 177777

sqt,	0
	dap sqx
	law i 23
	dac sq1
	dzm sq2
	lio sqt
	dzm sqt

sq3,	isp sq1
	jmp .+3
	lac sq2
sqx,	jmp .

	lac sq2
	sal 1s
	dac sq2
	lac sqt
	rcl 2s
	sza i
	jmp sq3
	dac sqt
	lac sq2
	sal 1s
	add (1
	sub sqt
	sma+sza-skp
	jmp sq3
	spa
	cma
	dac sqt
	idx sq2
	jmp sq3

sq1,	0
sq2,	0
          
                                                                 
/outline compiler
/ac=where to compile to, call   jda oc
			/ot=address of outline table

define
	plinst A
	lac A
	dac i oc
	idx oc
	terminate

define
	comtab A, B
	plinst A
	jsp ocs
	lac B
	jmp oce
	terminate

ocs,	dap ocz		/puts in swap
	dio i oc
	idx oc
	dio i oc
	idx oc
ocz,	jmp .

oc,	0		/outline compiler proper
	dap ocx
	lac i ocx
	dap ocg
	plinst (stf 5
	dap ocm
	idx ocx
ock,	plinst (lac .sx1
	plinst (lio .sy1
	clf 6
ocj,	setup .occ,6
ocg,	lio .		/outline table
och,	cla
	rcl 3s
	dio .oci
	lio (rcl 9s
	dispatch
	opr
	jmp oc1
oco,	jmp oc2
ocq,	jmp oc3
ocp,	jmp oc4
ocr,	jmp oc5
	jmp oc6
          
                                                                 
	plinst (szf 5	/7 code
	add (4
	dap ocn
	plinst ocn
	plinst (dac .sx1
	plinst (dio .sy1
	plinst (jmp sq6
	plinst (clf 5
	plinst (lac .scm
	plinst (cma
	plinst (dac .scm
	plinst (lac .ssm
	plinst (cma
	plinst (dac .ssm
	plinst (lac .csm
	plinst (lio .ssd
	plinst (dac .ssd
	plinst (dio .csm

	plinst (lac .ssc
	plinst (lio .csn
	plinst (dac .csn
	plinst (dio .ssc
	plinst ocm
ocx,	jmp .

ocm,	jmp .
ocn,	jmp .

oc1,	plinst (add .ssn
	jsp ocs
	lac (sub .scn
oce,	dac i oc
	idx oc
	jsp ocs
	plinst (ioh
	lac (dpy-4000
ocd,	dac i oc
	idx oc
	lio .oci
	count .occ, och
	idx ocg
	jmp ocj

oc2,	comtab (add .scm, (add .ssm
oc3,	comtab (add .ssc, (sub .csm
oc4,	comtab (sub .scm, (sub .ssm
oc5,	comtab (add .csn, (sub .ssd
oc6,	szf 6
	jmp oc9
	stf 6
	plinst (dac .ssa
	lac (dio .ssi
	jmp ocd
oc9,	clf 6
	plinst (lac .ssa
	lac (lio .ssi
	jmp ocd
          
                                                                 
/display a star

define
	starp
	add .bx
	swap
	add .by
	swap
	ioh
	dpy-4000
	terminate

blp,	dap blx		/star
	szs 60
	jmp blx
	random
	rar 9s
	and (400700
	spa
	xor (377777
	dac .bx
	lac ran
	ral 4s
	and (400700
	spa
	xor (377777
	dac .by
	jsp bpt
	ioh
blx,	jmp .

bpt,	dap bpx
	random
	sar 9s
	sar 6s
	spa
	cma
	sal 3s
	add (bds
	dap bjm
	cla cli clf 6-opr-opr
	dpy-4000
bjm,	jmp .
bds,	repeat 10, starp
	szf 6
bpx,	jmp .
	stf 6
	cma
	swap
	cma
	swap
	jmp bjm

          
                                                                 
/background display _  3/13/62, prs.

	define
dislis J, Q, B
	repeat 6, B=B+B
	clf 5
	lac flo+R
	dap fpo+R
fs,	dap fin+R
	dap fyn+R
	idx fyn+R

fin,	lac	/lac X
	sub fpr	/right margin
	sma
	jmp fgr+R
	add (2000
frr,	spq
fou,	jmp fuu+R
fie,	sub (1000
	sal 8s
fyn,	lio	/lio Y
	dpy-i+B
	stf 5
fid,	idx fyn+R
	sad (lio Q+2
	jmp flp+R
	sad fpo+R
	jmp fx+R
	dap fin+R
	idx fyn+R
	jmp fin+R

fgr,	add (-20000+2000
	jmp frr+R

fuu,	szf 5
fx,	jmp flo+R+1	/return
	idx flo+R
	idx flo+R
	sas (Q+2
	jmp fid+R
	law J
	dac flo+R
	jmp fid+R

flp,	lac (lio J
	sad fpo+R
	jmp fx+R
	dap fin+R
	law J+1
	dap fyn+R
	jmp fin+R

fpo,	lio
flo,	J
	terminate
          
                                                                 
	define
background
	jsp bck
	termin

bck,	dap bcx
	szs 40
	jmp bcx
	isp bcc
bcx,	jmp .
	law i 2
	dac bcc
	dislis 1j,1q,3
	dislis 2j,2q,2
	dislis 3j,3q,1
	dislis 4j,4q,0
	isp bkc
	jmp bcx
	law i 20
	dac bkc
	law i 1
	add fpr
	spa
	add (20000
	dac fpr
	jmp bcx

bcc,	0
bkc,	0
fpr,	10000



mul=mus
div=dis


start


          
                                                                          
                                                                                                        

