FOR FAMILY OF PDP-11 COMPUTERS

WORD FORMAT:

PROGRAM COUNTER ADDRESSING:

Mode Name Symbolic Description 0 1 2 3 4 5 6 7 register register deferred auto-increment auto-incr deferred auto-decrement auto-decr deferred index index deferred

(R) is operand [ex. R2=2] (R) is address (R) is adrs; (R)=(1 or 2) (R) is adrs of adrs; (R)+2 (R) -(1 or 2); (R) is adrs (R) -2; (R) is adrs of adrs (R) +X is adrs (R) +X is adrs of adrs

R (R) (R)+ @(R)+ -(R) @-(R) X(R) @X(R)

2 3 4 5 auto-increment auto-incr deferred auto-decrement auto-decr deferred

(R) is adrs; (R)=(1 or 2) (R) is adrs of adrs; (R)+2 (R) -(1 or 2); (R) is adrs (R) -2; (R) is adrs of adrs

(R)+ @(R)+ -(R) @-(R)

LEGEND:

OP Codes

(R) is operand [ex. R2=2] (R) is address (R) is adrs; (R)=(1 or 2) (R) is adrs of adrs; (R)+2 (R) -(1 or 2); (R) is adrs (R) -2; (R) is adrs of adrs (R) +X is adrs (R) +X is adrs of adrs

Operations

(R) is operand [ex. R2=2] (R) is address (R) is adrs; (R)=(1 or 2) (R) is adrs of adrs; (R)+2 (R) -(1 or 2); (R) is adrs (R) -2; (R) is adrs of adrs (R) +X is adrs (R) +X is adrs of adrs

Boolean

(R) is operand [ex. R2=2] (R) is address (R) is adrs; (R)=(1 or 2) (R) is adrs of adrs; (R)+2

Condition Codes

(R) is operand [ex. R2=2] (R) is address (R) is adrs; (R)=(1 or 2) (R) is adrs of adrs; (R)+2

digital equipment corporation

MLO-003570