I/O PAGE

MEMORY 28K

1000 776 500 476

SYSTEM DEVICE HANDLER

BG JOB HIGH LIMIT ^ / / /

USR KEYBOARD MONITOR USR SWAP SPACE

60 56 40 36 0

RESIDENT MONITOR

DEFAULT BACKGROND STACK

FETCHED HANDLER SPACE (USUALLY PART OF THE VARIABLE AREA)

INTERRUPT VECTORS

VARIABLE SIZE DATA AREA (OBTAINED BY .SETTOP

SYSTEM COMMUNICATION AREA

FIXED DATA AREA (ASSEMBLED)

TRAP VECTORS

CODE AREA (ASSEMBLED)

STACK