15 14* 13* 12* 11* 10+ 9 8+ 1= NO USR SWAPPING (SJ ONLY)

1= LOWER CASE ENABLED

1= REENTER CAN START JOB

1= TT SPECIAL MODE

1= PASS LINE TO KMON

1= VIRTUAL JOB (XM ONLY)

1= OVERLAID JOB CHAIN BIT

7* 6* 2 0

BITS MARKED WITH AN ASTERISK (*) ARE BITS THAT YOU CAN SET DURING EXECUTION. ) CAN BE SET AT LOAD TIME.

5* 4* 3* 1

1= HALT ON I/O ERROR (SJ ONLY)

1= NO TT WAIT STATE 1= SPECIAL CHAIN EXIT

1= DISABLE SL EDITOR

1= NON- TERMINATING .GTLIN

RESERVED

BITS MARKED WITH A PLUS SIGN (