15 14 13 12 11 10 8 7 5 4 3 2 1 0

CONDITION CODES T BIT PRIORITY GENERAL REGISTER SET (MAPPED MONITORS ONLY) PREVIOUS MODE (MAPPED MONITORS ONLY) CURRENT MODE (MAPPED MONITORS ONLY)psw

T N Z V C