First data block 1

BCL Low-order eight bits of byte count High-order eight bits of byte count Low-order byte of absolute load address

High-order byte of load address of data bytes in the block

Data bytes

Checksum byte

intermediate blocks.

Intermediate data blocks

0

BCH

Low byte of start address, or odd number High byte of start address, or odd number

This pattern is repeated for al+

Data bytes

Checksum byte

Last data block

1

ADL

Checksum byte

0

ADH

1

. . .

0

BCL

6

BCH

0

ADL ADH

. . .

JL JH