maindec-08-dhcra-a-pb 01/31/77; cr8e/cr8f card reader test; replaces: maindec-8e-d2eb-pb; (c)1971,72
maindec-08-dhkma-c-pb 01/09/78; pdp-8e extended memory data & checkerboard test; 0021=0000 0022=0400; (c)1972,75,76
maindec-08-dhkmc-b-pb 01/09/78; pdp-8e extended memory address test (ea8e); (c)1976
maindec-08-dhlaa-b-pb 2/1/74; decwriter (la30) exerciser test; (c)1971,73,74
maindec-08-dhpca-a-pb 06/03/77; highspeed reader/punch tests; replaces: md-8e-d2ca-pb; (c)1971,77
maindec-08-dhvtc-d-pb 08/22/77; vt50-vt52 video terminal acceptance test; (c)1975,76
maindec-08-dilab-d-pb 04/22/77; la36 terminal diagnostic; (c)1974,75
maindec-08-dilac-b-pb 05/31/77; la180 printer diagnostic; (c)1975,76
maindec-08-divtc-a-pb 08/24/77; vt55 video terminal acceptance test; (c)1975
maindec-08-djdka-c-pb1 11/10/76; dkc8-aa option test #1; (c)1974,75,76
maindec-08-djexb-a-pb 01/13/78; 2k to 32k pdp-8a processor exerciser; (c)1974
maindec-08-djkka-c-pb1 06/24/77; pdp-8/a cpu test; (c)1974,77
maindec-08-djkla-c-pb 05/20/77; kl8-a multiple serial line unit diagnostic; (c)1975,76
maindec-08-djmsa-a-pb 08/04/77; 1-4k ms8-a mos memory test; (c)1974
