maindec-08-d01a-pb.bin 3/10/66 instruction test part 2a
maindec-08-d02b-pb.bin 1/3/68 instruction test part 2b
maindec-08-d05b-pb.bin 12/28/67 random jmp jms test load 200 start 215
maindec-08-d05b.pb.bin 12/28/67 random jmp jms test
maindec-08-d07b-pb.bin 12/28/67 random isz test load 0037 start 4000
maindec-08-d1ac-pb.bin 9/16/68 pdp-8 memory power on/off test
maindec-08-d1eb-pb.bin 5/1/68 pdp-8,8i ext. mem. checkerboard
maindec-08-d1gd-pb.bin 7/27/70 pdp-8, 8i, 8s extended memory control load 200 start bit 08 & no of fields bits 9 thru 11
maindec-08-d1ha-pb.bin 10/1/68 pdp-8 8/i extended memory address test load 200 start 0
maindec-08-d1kb-pb.bin 1/29/71 kp8i/kr01 power fail test
maindec-08-d1l1-pm.bin 2/27/68 basic pdp-8, 8i meory checkboard (low) load 0005 start 0101
maindec-08-d1l2-pm.bin 6/7/68 basic pdp-8, 8i memory checkerboard (high) load 7430 start 0101
maindec-08-d1ma-pm1.bin 2/11/71 memory address test (low) load 0004 start 4000
maindec-08-d1ma-pm2.bin 2/11/71 memory address test (high) load 7400 start 4000
maindec-08-d2pe-pb.bin 2/21/69 family of 8 asr 33/35 teletype test part 1
maindec-08-d2qd-pb.bin 6/4/68 family of 8 asr33/35 teletype tests part 2
maindec-08-d3eb-pb.bin 1/5/68 tc01 extended memory exerciser
maindec-8e-d0hc-pb.bin 6/11/71 random jmp test load & start 200
maindec-8e-d1ib-pb1.bin 1/17/72 mi8e bootstrap diagnostic (low)
maindec-8e-d1ib-pb2.bin 1/17/72 mi8e bootstrap diagnostic (high)
maindec-8i-d01c-pb.bin 12/10/69 instruction test 1 load 144 start 7777 halts at 146 ac=0 cont.
maindec-8i-d02b-pb.bin 3/21/68 instruction test 2 load & start 201
maindec-8i-d0aa-pb.bin 3/13/68 pdp-8 instruction test part 3a (eae) load 200 start 5000
maindec-8i-d0ba-pb.bin 4/22/68 extended arithmetic pdp-8i instruction test part 3b l&s 200 cont 400
maindec-8i-d8ae-pb.bin 7/7/71 kw8i real time clock
maindec-8l-d0ab-pb.bin 5/6/71 8l memory protect test load 202 protect to 0
maindec-8l-d1gc-pb.bin 1/28/71 pdp-8l extended memory control test 8l l&s 200 8 l-200 s-0001 8i l-200 s-0011
maindec-8l-d1ha-pb.bin 3/27/70 8/l extended memory control test (12k) load 200 start 0002
