/SYMBOL DEFINITIONS
AX1=10
AX2=11
BUFF=1400
READ=3
SYSIO=7642
TEM1=174
TEM2=175
WRITE=5
/
*200
BEGN,	JMS CRLF
	JMS TMES
	MSG2
	JMS RMES
CHAR,	BUFF
	TAD I .-1
	CIA
	TAD ("L
	SNA CLA		/LOAD OR DUMP?
	JMP LOAD
	TAD I CHAR
	CIA
	TAD ("V
	SNA CLA		/OR VERIFY?
	JMP VRFY
	TAD I CHAR
	CIA
	TAD ("D
	SZA CLA
	JMP BEGN
DUMP,	JMS TMES
	MSG3
	JMS ROCT
	DCA N
	JMS TMES
	MSG1
	JMS ROCT
	DCA LB
	TAD (200
	PLS
	CLA
	TAD (120
	DCA .+2
PLOT,	JMS LDLP
	100
	JMS SYSIO	/READ BLOCK N
	READ
N,	0
	BUFF		/CORE LOC'N
L,	0
	HLT
	TAD N
	DCA BUFF+200
	TAD L
	DCA BUFF+201
	TAD (-202	/COMPUTE CHECKSUM
	DCA INDX
	TAD (BUFF-1
	DCA Z AX1
LP01,	TAD I AX1
	ISZ INDX
	JMP LP01
	DCA BUFF+202
	JMS PBIN
	203
	BUFF
	TAD (14
	DCA PLOT+1
	ISZ N
	TAD N
	CIA
	TAD LB
	SMA CLA
	JMP PLOT
	JMS LDLP
	40
	JMP BEGN
LB,	0
INDX,	0
/
LOAD,   JMS TMES
        MSG1
        JMS ROCT
        DCA LB
	RFC
        JMS LOOK        /READ ONE BLOCK FROM THE TAPE
LP03,   TAD BUFF+200
        DCA BN
        TAD BN
        CIA
        TAD LB
        SPA CLA         /IS THIS BLOCK NR OK?
        JMP ENDP
        TAD BUFF+201
        DCA LN
        JMS I (SYSIO
        WRITE
BN,     0       /BLOCK NUMBER
        BUFF
LN,     0       /LINK NUMBER
        HLT
        TAD BN
        CIA
        TAD LB
        SZA CLA
        JMP LOAD+5
ENDP,   JMS CRLF
        JMS TMES
        MSG4
        JMS CRLF
        JMP BEGN
CKSM,   0
/
        PAGE

*BEGN+200
RBIN,   0               /SPECIAL BINARY LOADER
        TAD I RBIN
        ISZ RBIN        /CALL AS FOLLOWS...
        CIA
        DCA KNDX        / JMS RBIN
        CMA             / N     (N = NR OF 12-BIT WORDS)
        TAD I RBIN      / LOC   (LOC = BUFFER ADDRESS)
        ISZ RBIN
        DCA AX1
        TAD (JMP LP04
        DCA SWHH
LP04,   JMS I [PTRI
        TAD (-200
        SNA
SWHH,   JMP LP04
        TAD (200
        CLL RTL
        RTL
        RTL
        DCA TEM1
        JMS I [PTRI
        TAD TEM1
        DCA I AX1
        TAD (JMP I RBIN
        DCA SWHH
        ISZ KNDX
        JMP LP04
        JMS I [PTRI
        TAD (-200
        SZA CLA
        JMP .-3
        JMP I RBIN
/
PTRI,   0               /HI-SPEED READER ROUTINE
        RSF
        JMP WAIT
        DCA PTRF        /SET READER FLAG
        RRB RFC
        JMP I PTRI
WAIT,   DCA PBIN
        ISZ PTRF
        JMP PTRI+1
        JMS CRLF
        JMS TMES
        MSG5
        TAD BN
        JMS TOCT
        JMS CRLF
        HLT
        JMP BEGN
PTRF,   0
/
PBIN,   0               /SPECIAL BINARY PUNCH ROUTINE
        TAD I PBIN
        ISZ PBIN        /CALL AS FOLLOWS...
        CIA
        DCA KNDX        / JMS PBIN
        CMA             / N     (N = NR OF 12-BIT WORDS)
        TAD I PBIN      / LOC   (LOC = BUFFER ADDRESS)
        ISZ PBIN
        DCA AX1
LP05,   TAD I AX1
        DCA TEM1
        TAD TEM1
        RTR
        RTR
        RTR
        AND (77
        JMS I [PTPO
        TAD TEM1
        AND (77
        JMS I [PTPO
        ISZ KNDX
        JMP LP05
        JMP I PBIN
/
PTPO,   0               /HI-SPEED PUNCH ROUTINE
        PSF
        JMP .-1
        PLS
        CLA
        JMP I PTPO
/
LDLP,   0               /LEADER-TRAILER PUNCH ROUTINE
        TAD I LDLP
        ISZ LDLP
        CIA
        DCA KNDX
        TAD (200
        JMS I [PTPO
        ISZ KNDX
        JMP .-3
        JMP I LDLP
/
CRLF,   0
        TAD (215
        JMS TTYO
        TAD (212
        JMS TTYO
        JMP I CRLF
/
KNDX,   0
/
ERR1,   0               /CHECKSUM ERROR ON READ
        JMS TMES
        MSG6
        TAD BN
        JMS TOCT
        JMS CRLF
        JMS TMES
        MSG7
        JMS RMES
        BUFF+204
        TAD I .-1
        CIA
        TAD ("R
        SZA CLA
        JMP BEGN        /RESTART
	RFC
        JMP I ERR1      /RETRY
/
        PAGE

*BEGN+400
TMES,   0               /MESSAGE TYPEOUT ROUTINE
        TAD I TMES
        ISZ TMES
        DCA POIN
LP08,   TAD I POIN
        CLL RTR
        RTR
        RTR
        JMS OTCH
        JMP I TMES
        TAD I POIN
        ISZ POIN
        JMS OTCH
        JMP I TMES
        JMP LP08
POIN,   0
/
OTCH,   0               /CHARACTER TYPEOUT ROUTINE
        AND (77
        SNA             /END OF LIST?
        JMP I OTCH      /YES
        TAD (-40
        SPA
        TAD (100
        TAD (240
        JMS TTYO
        ISZ OTCH
        JMP I OTCH
/
TTYO,   0
        TLS
        TSF
        JMP .-1
        CLA
        JMP I TTYO
/
ROCT,   0               /OCTAL READ-IN ROUTINE
        DCA TEM1
        DCA TEM2
        TAD (JMP QUES
        DCA SWHP
        JMS RMES
        BUFF
        CMA
        TAD .-2
        DCA AX1
LP07,   TAD I AX1
        SNA
SWHP,   JMP QUES
        TAD (-260
        SPA
        JMP QUES
        TAD (-10
        SMA
        JMP QUES
        TAD (10
        TAD TEM2
        DCA TEM1
        TAD TEM1
        CLL RAL
        RTL
        DCA TEM2
        TAD (JMP BYP2
        DCA SWHP
        JMP LP07
BYP2,   TAD TEM1
        JMP I ROCT
QUES,   TAD ("?
        JMS TTYO
        JMS CRLF
        JMP ROCT+1
/
RMES,   0               /MESSAGE READ-IN ROUTINE
        KCC
        CMA
        TAD I RMES
        ISZ RMES
        DCA AX1
LP06,   JMS TTYI
        DCA TEM1
        TAD TEM1
        TAD (-377
        SNA CLA
        JMP RBOT
        TAD TEM1
        JMS TTYO
        TAD TEM1
        TAD (-215
        SNA CLA
        JMP BYP0
        TAD TEM1
        DCA I AX1
        JMP LP06
BYP0,   DCA I AX1
        TAD (212
        JMS TTYO
        JMP I RMES
RBOT,   TAD ("\
        JMS TTYO
        CMA
        TAD AX1
        DCA AX1
        JMP LP06
/
TTYI,   0               /TELETYPE INPUT ROUTINE
        KSF
        JMP .-1
        KRB
        TAD (-203
        SNA             /IS IT A ^C?
        JMP I (7600
        TAD (203
        JMP I TTYI
/
        PAGE
/
*BEGN+600
VRFY,   JMS TMES        /TAPE VERIFICATION ROUTINE
        MSG1
        JMS ROCT
        DCA LB
	RFC
        JMS LOOK        /READ ONE BLOCK FROM THE TAPE
        TAD BUFF+200
        DCA BLK
        TAD BLK
        DCA BN
        JMS I (SYSIO
        READ
BLK,    0
        BUFF+400
LNK,    0
        HLT
        TAD (BUFF-1
        DCA AX1
        TAD (BUFF+377
        DCA AX2
        TAD (-200
        DCA IX
        TAD I AX1
        CIA
        TAD I AX2
        SZA CLA
        JMP ERR2
        ISZ IX
        JMP .-6
        TAD LNK
        CIA
        TAD BUFF+201
        SZA CLA
        JMP ERR2
        TAD LB
        CIA
        TAD BLK
        SPA CLA         /WAS THIS THE LAST BLOCK?
        JMP VRFY+5
        JMS CRLF
        JMS TMES
        MSG8            /TAPE VERIFIED!
        JMS CRLF
        JMP BEGN
IX,     0
/
LOOK,   0
        RFC
        JMS RBIN
        203
        BUFF
        TAD (-202
        DCA IX
        TAD (BUFF-1
        DCA AX1
        DCA CKSM
LP02,   TAD I AX1
        ISZ IX
        JMP LP02
        CIA
        TAD BUFF+202
        SNA CLA
        JMP .+3
        JMS ERR1
        JMP LOOK+1
        JMP I LOOK
/
ERR2,   JMS TMES
        MSG9            /ERROR IN BLOCK NR
        TAD BLK
        JMS TOCT
        JMS CRLF
        JMS TMES
        MSG7
        JMS RMES
        BUFF+204
        TAD I .-1
        CIA
        TAD ("R
        SZA CLA
        JMP BEGN
        JMP VRFY+4
/
TOCT,   0               /OCTAL TYPEOUT ROUTINE
        CLL RAL
        DCA TEM1
        TAD (-4
        DCA TEM2
LP10,   TAD TEM1
        RTL
        RAL
        DCA TEM1
        TAD TEM1
        AND (7
        TAD (260
        JMS TTYO
        ISZ TEM2
        JMP LP10
        JMP I TOCT
/
        PAGE
/
/
*BEGN+1000
MSG1,   TEXT /ENTER LAST BLOCK NR - /
MSG2,	TEXT /LOAD DUMP OR VERIFY - /
MSG3,   TEXT /ENTER FIRST BLOCK NR - /
MSG4,   TEXT /TAPE LOADED!/
MSG5,   TEXT /RAN OUT OF TAPE AFTER BLOCK /
MSG6,   TEXT /CHECKSUM AFTER BLOCK NR /
MSG7,   TEXT /TYPE "R" TO RETRY, "S" TO RESTART - /
MSG8,   TEXT /TAPE VERIFIED!/
MSG9,   TEXT /ERROR IN BLOCK /
        PAGE
        $
*U*5