THE STANDARD COMMAND STRING FORMAT IS:

     #DEV:[/FORMAT OPTION]<DEV:/OPTIONS:N

DEVICE NAMES ARE "DF:" (RF11 DISK), "DK0:" TO "DK7:" (RK11
UNITS 0 - 7), "DP0:" TO "DP7:" (RP03 DISK PACK UNITS
0 - 7), "DC:" (RC11 DISK), "DT:" (DECTAPE -- IF SEVERAL
UNITS ARE NEEDED, UNIT 0 IS USED FIRST, UNIT 1 NEXT, ETC.),
NOTE: ROLLIN ALSO RECOGNIZES "RF","RC","RK","RP"
SHOULD YOU PERFER THOSE DEVICE NAMES. FOR MAGTAPE USE
"MT0:NAME" TO "MT7:NAME" (MAGTAPE UNITS 0 - 7).  NOTE
THAT MAGTAPE ALWAYS REQUIRES A FILENAME, EXCEPT FOR THE
MAGTAPE COPY FUNCTION.
"CT0:NAME" OR "CT1:NAME" (TA-11 DRIVE 0 OR 1 )
NOTE: IF NAME NOT SPECIFIED ON CASSETTES THEN DEFAULT 
OF "NONAME" WILL BE USED.

OPTION SWITCHES ARE AS FOLLOWS:

/AUTO              AUTOMATIC <CR> REPLY TO CASSETTE
                   MOUNT REQUESTS.
/BLOCK:N           N IS THE NUMBER OF BLOCKS TO TRANSFER 
                   WHERE A BLOCK IS 256 WORDS.
/BOOT:DEV          BOOTSTRAP FROM SPECIFIED DEVICE.
                   DEV MAY BE "DF" (RF11), "DK" (RK11),
                   "DC" (RC11), "DT" (DECTAPE), "MT"
                   (MAGTAPE), OR "DP" (RP03 DISK),
                   OR "CT" (TA-11 CASSETTE).
/DATE:01-JAN-70    USED IN WRITING MAGTAPE & CASSETTE LABEL (OPTIONAL).
/FIND              ON INPUT FROM MAGTAPE AND CASSETTE, PERFORM A SEARCH
                   FOR THE SPECIFIED FILE.  ON OUTPUT 
                   SKIP TO END OF DATA.
                   /FIND IS ASSUMED UNLESS /STAY OR /REWIND USED 
/FORMAT            FORMAT DISK PACK PRIOR TO OPERATION.
                   OUTPUT DEV MUST BE RK OR RP.
/HELP              TYPE THIS DOCUMENT.
/IGNORE            IGNORE SOFT DISK ERRORS 
/LIST              CAUSES LABELS ON MAGTAPE AND CASSETTE 
                   TO BE LISTED IF THEY DO NOT MATCH 
                   THE NAME SPECIFIED.
/NOLABEL           ON DISK TO DECTAPE DUMPS, PREVENTS THE
                   LABEL RECORD FROM BEING WRITTEN.
/NUMBER:N          N IS THE NUMBER OF 1K TRACKS TO
                   DUMP OR RESTORE.
/PLATTERS:N        FOR RF11 OR RC11 ONLY, N IS THE NUMBER
                   OF DISK PLATTERS TO DUMP OR RESTORE.
/REWIND            REWIND THE MAGTAPE OR CASSETTE BEFORE USE.
/RSTS              BOOTSTRAP RSTS FROM RF11 ONLY.
/SECTOR:N          N IS THE STARTING BLOCK NUMBER.
/SKIP:N            SKIP PAST N FILES ON MAGTAPE BEFORE USE.
/STAY              SUPPRESS AUTO /FIND AND AUTO /REWIND. 
/TEST              DO A READ AFTER WRITE ON CASSETTES (ONLY) 
/TRACK:N           N IS THE NUMBER OF THE FIRST 1K TRACK TO
                   DUMP OR RESTORE.
/UNBOOT            DELETES WRITING ROLLIN OUT ON CASSETTE (ONLY)
                   THEREBY MAKING OUTPUT UNBOOTABLE.
/V4A               SPECIAL OPTION FOR RSTS V4A.
/VERIFY            USED WITH MAGTAPE OR DISK COPY FUNC-
                   TIONS (ONLY) TO VERIFY THE COPY.
                   (DOES NOT WORK WITH CASSETTES) 
/WL                WILL WRITE LOCK AN RK11 DISK.

TELETYPE OUTPUT MAY BE STOPPED BY TYPING CTRL/O.
