    >@SYSGEN
    >;
    >; RSX-11M-PLUS  V4.6  BL87  SYSGEN
    >;
    >; Copyright (c) 1995-1999 by Mentec Inc., U.S.A.
    >;
    >SET /DPRO=[RWED,RWED,RWE,R]
    >;
    >; To exit from the SYSGEN procedure at any time, type CTRL/Z.
    >;
    >; If you are unsure of the answer to a question for which a de-
    >; fault answer exists, use the default answer.
    >;
    >;
    >;
    >;===================================================
    >;  Choosing SYSGEN Options      01-MAY-21 at 13:08
    >;===================================================
    >;
    >;
    >;
    >; Every question is preceded by a question number (for example SU010)
    >; which you can use to find the explanation of the question in the
    >; RSX-11M-PLUS System Generation and Installation Guide.
    >;
    >; An explanation of every question is also available by pressing
    >; the ESC key (or the ALTMODE key) in response to the question.
    >;
    >; If you are unfamiliar with the SYSGEN procedure, the explanation of
    >; each question can be printed automatically before the question.
    >;
    >* SU010   Do you always want the explanation printed? [Y/N D:N]:
    >;
    >; SYSGEN always creates saved answer files containing your responses
    >; to the SYSGEN questions:
    >;
    >;    SYSGENSA1.CMD     Setup questions, Executive options
    >;    SYSGENSA2.CMD     Peripheral configuration
    >;    SYSGENSA3.CMD     Nonprivileged task builds
    >;
    >; You should perform a PREPGEN first to create saved answer files, and
    >; then perform a SYSGEN, specifying those saved answer files as input
    >; to the Executive, peripheral, and nonprivileged task build sections.
    >;
    >* SU020   Do you want to use a saved answer file as input for
    >*         the Executive options? [Y/N D:N]:
    >;
    >* SU040   Do you want to use a saved answer file as input for
    >*         the peripheral configuration? [Y/N D:N]:
    >;
    >* SU060   Do you want to use a saved answer file as input for
    >*         the nonprivileged task builds? [Y/N D:N]:
    >;
    >* SU080   Do you want to do a PREPGEN? [Y/N D:N]:
    >;
    >* SU090   Enter the name of the disk drive containing your
    >*         target system disk [ddnn:] [S R:2-5]: SY
    >;
    >ASN SY:=IN:
    >ASN SY:=OU:
    >ASN SY:=LB:
    >ASN SY:=WK:
    >ASN SY:=TK:
    >ASN SY:=BC:
    >ASN SY:=LI:
    >ASN SY:=OB:
    >ASN SY:=EX:
    >ASN SY:=MP:
    >;
    >* SU100   Do you want to run Autoconfigure on the host system
    >*         hardware? [Y/N D:N]: Y
    >;
    >; Running Autoconfigure:
    >;
    >INS $ACF
    >ACF
    >INS $ACO
    >ACO SHOW
    Processor Type:  11/83          Memory Size:  2044. Kw

    Options:

            Floating Point Processor (FP11)
            Extended Instruction Set (EIS)
            Extended (22-Bit) Addressing
            Cache Memory
            Parity Memory

    Name    Vector     CSR      Unit    Type      Remark
    LPA      200      177514
    YLA      060      177560
    YLB      300      176500
    YLC      310      176510
    YLD      320      176520
    YLE      330      176530
    DAA      174      177220
                                 0      AZ11
                                 1      AZ11
                                 2      AZ11
                                 3      AZ11
                                 4      AZ11
                                 5      AZ11
                                 6      AZ11
                                 7      AZ11
                                 10     AZ11
                                 11     AZ11
                                 12     UNKNOWN
                                 13     UNKNOWN
                                 14     UNKNOWN
                                 15     UNKNOWN
                                 16     UNKNOWN
                                 17     UNKNOWN
                                 20     UNKNOWN
                                 21     UNKNOWN
                                 22     UNKNOWN
                                 23     UNKNOWN
                                 24     UNKNOWN
                                 25     UNKNOWN
                                 26     UNKNOWN
                                 27     UNKNOWN
                                 30     UNKNOWN
                                 31     UNKNOWN
                                 32     UNKNOWN
                                 33     UNKNOWN
                                 34     UNKNOWN
                                 35     AZ11
                                 36     AZ11
                                 37     AZ11

    >ACO SYSGEN
    >;
    >* SU110   Do you want to override the Autoconfigure results? [Y/N D:N]: Y
    >;
    >; You can:
    >;
    >;    o  do a complete SYSGEN
    >;
    >;    o  continue a previous SYSGEN from where you left off
    >;
    >;    o  do an individual section of SYSGEN
    >;
    >;
    >* SU120   Do you want to do a complete SYSGEN? [Y/N D:Y]:
    >;
    >INS [3,54]MAC/TASK=MACT0
    >INS [3,54]PIP/TASK=PIPT0
    >INS [3,54]LBR/TASK=LBRT0
    >INS [3,54]TKB/TASK=TKBT0
    >INS [3,54]VMR/TASK=VMRT0
    >;
    >;
    >;
    >;======================================================
    >;  Choosing Executive Options      01-MAY-21 at 13:08
    >;======================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >; Enter a comment for inclusion in the SYSGENSA1 saved answer file.
    >; The comment may contain more than one line.  The "V" in the right
    >; margin below marks the maximum line length.  When you are done,
    >; press RETURN in response to the prompt.
    >;                                                                             V
    >* Comment [S R:0.-55.]: PDP-11/83
    >* Comment [S R:0.-55.]:
    >;
    >* CE010   What is your target processor type? [S R:3.-12. D:"11/83"]:
    >;
    >* CE020   Do you want the Full-functionality Executive? [Y/N D:Y]:
    >;
    >* CE115   Do you want to use ICB pool as backup for primary pool ? [Y/N D:N]: Y
    >;
    >* CE120   Do you want support for communications products
    >*         (such as DECnet, PSI, and LAT)? [Y/N D:N]: Y
    >;
    >* CE130   What is the system name? [S R:0-6 D:"RSXMPL"]: BIGSYS
    >;
    >* CE215   Do you want the default date format to be
    >*         ISO 8601:1988 compliant? [Y/N D:N]:
    >;
    >* CE216   Do you want the default date format to include
    >*         a four digit year? [Y/N D:N]:
    >;
    >* CE264   Do you want IP11 industrial I/O subsystem support? [Y/N D:N]:
    >;
    >* CE270   Do you want to include XDT? [Y/N D:N]: Y
    >;
    >* CE280   Enter the crash notification device CSR
    >*         address [O R:160000-177700 D:177564]:
    >;
    >; Note:  Enter both the device and the logical unit number.
    >;        For example, MM0: or DL1:.
    >;
    >; Note:  Enter XX: if you desire loadable DA:, DU:, DL:, MU:, MS: or MM:
    >;        crash driver support.
    >;
    >* CE290   On what device and unit do you want crash dumps
    >*         to be written? [S R:2-6]: XX:
    >;
    >* CE300   Enter the initial number of virtual disks to be
    >*         included [D R:0.-16. D:2.]:
    >;
    >* CE310   Enter memory size (in K words) [D R:256.-2044. D:2044.]: 256
    >;
    >* CE315   Support UNIBUS memory occupying UNIBUS map address space? [Y/N D:N]:
    >;
    >* CE330   Is your system clock programmable (KW11-P)? [Y/N D:N]:
    >;
    >* CE350   Is your line frequency 50 Hz? [Y/N D:N]: Y
    >;
    >;
    >;
    >;=============================================================
    >;  Choosing Peripheral Configuration      01-MAY-21 at 13:09
    >;=============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA2.CMD.
    >;
    >; Enter a comment for inclusion in the SYSGENSA2 saved answer file.
    >; The comment may contain more than one line.  The "V" in the right
    >; margin below marks the maximum line length.  When you are done,
    >; press RETURN in response to the prompt.
    >;                                                                             V
    >* Comment [S R:0.-55.]: PDP-11/83
    >* Comment [S R:0.-55.]:
    >;
    >;
    >* CP0604  How many RH controllers do you have? [D R:0.-15. D:0.]:
    >;
    >;
    >;   DK:    controller:  RK11		devices: RK05, RK05F
    >;
    >* CP2204  How many RK11 cartridge disk controllers do you have? [O D:0]:
    >;
    >;
    >;   DM:    controllers: RK611, RK711	devices: RK06, RK07
    >;
    >* CP2404  How many RK611/711 disk cartridge controllers do
    >*         you have? [O D:0]:
    >;
    >;
    >;   DL:    controllers: RL11, RLV12	devices: RL01, RL02
    >;
    >* CP2604  How many RL11/RLV11 disk cartridge controllers do
    >*         you have? [O D:0]:
    >;
    >;
    >;   DP:    controller:  RP11		devices: RP02, RPR02, RP03
    >;
    >* CP2804  How many RP11 disk pack controllers do you have? [O D:0]:
    >;
    >;   DU:    controllers: RQZX1, RQDX1, RQDX2, RQDX3,
    >;                       RUX50, RQC25, KDA50, UDA50
    >;
    >;          devices:     RX33, RX50, RD31, RD51, RD52, RD53, RD54,
    >;                       RC25, RA60, RA70, RA71, RA72, RA80, RA81,
    >;                       RA82, RA90, RA92, RZ23L, RZ24L, RZ26x, RZ29B
    >;
    >;   The total of DU and MU controllers cannot be greater than 10.
    >;
    >* CP3004  How many MSCP disk controllers do you have? [D R:0.-10. D:0.]: 1
    >;
    >* CP3008  How many physical MSCP disk drives do you have? [D D:1.]: 4
    >;
    >;
    >* CP3036  What is the physical unit number of DU0:? [O R:0-377 D:0]:
    >;
    >;
    >* CP3036  What is the physical unit number of DU1:? [O R:0-377 D:1]:
    >;
    >;
    >* CP3036  What is the physical unit number of DU2:? [O R:0-377 D:2]:
    >;
    >;
    >* CP3036  What is the physical unit number of DU3:? [O R:0-377 D:3]:
    >;
    >;
    >* CP3068  Enter the vector address of DUA [O R:60-774 D:154]:
    >;
    >* CP3072  What is its CSR address? [O R:160000-177700 D:172150]:
    >;
    >;
    >;   MU:    controllers: TK50, TU81, TU81E, TQ81E, RQZX1
    >;
    >* CP3404  How many TMSCP tape controllers do you have? [D R:0.-9. D:0.]: 1
    >;
    >;
    >* CP3436  What is the physical unit number of MU0:? [O R:0-377 D:0]:
    >;
    >;
    >* CP3468  Enter the vector address of MUA [O R:60-774 D:260]:
    >;
    >* CP3472  What is its CSR address? [O R:160000-177700 D:174500]:
    >;
    >;
    >;   DA:    controller: AZ11
    >;
    >* CP3604  How many AZ11 disk image controllers do you have? [O R:0-1 D:1]:
    >;
    >* CP3608  How many AZ11 disk drives do you have? [D R:1.-32. D:32.]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA0:? [O R:0-37 D:0]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA1:? [O R:0-37 D:1]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA2:? [O R:0-37 D:2]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA3:? [O R:0-37 D:3]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA4:? [O R:0-37 D:4]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA5:? [O R:0-37 D:5]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA6:? [O R:0-37 D:6]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA7:? [O R:0-37 D:7]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA10:? [O R:0-37 D:10]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA11:? [O R:0-37 D:11]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA12:? [O R:0-37 D:12]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA13:? [O R:0-37 D:13]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA14:? [O R:0-37 D:14]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA15:? [O R:0-37 D:15]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA16:? [O R:0-37 D:16]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA17:? [O R:0-37 D:17]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA20:? [O R:0-37 D:20]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA21:? [O R:0-37 D:21]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA22:? [O R:0-37 D:22]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA23:? [O R:0-37 D:23]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA24:? [O R:0-37 D:24]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA25:? [O R:0-37 D:25]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA26:? [O R:0-37 D:26]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA27:? [O R:0-37 D:27]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA30:? [O R:0-37 D:30]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA31:? [O R:0-37 D:31]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA32:? [O R:0-37 D:32]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA33:? [O R:0-37 D:33]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA34:? [O R:0-37 D:34]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA35:? [O R:0-37 D:35]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA36:? [O R:0-37 D:36]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA37:? [O R:0-37 D:37]:
    >;
    >;
    >* CP3668  Enter the vector address of DAA [O R:60-774 D:174]:
    >;
    >* CP3672  What is its CSR address? [O R:160000-177700 D:177220]:
    >;
    >;			  DA Configuration
    >;
    >; 			Physical Unit Number
    >;
    >; 	0	1	2	3	4	5	6	7
    >;
    >; DAA	DA0:	DA1:	DA2:	DA3:	DA4:	DA5:	DA6:	DA7:
    >;
    >;
    >;
    >;   VF:    Virtual disk/tape driver
    >;
    >;
    >;
    >;   CR:    controllers: CM11, CR11
    >;
    >* CP4004  How many CM/CR11 card readers do you have? [O D:0]:
    >;
    >;
    >;   CT:    controller:  TA11		device:  TU60
    >;
    >* CP4204  How many TA11 dual cassettes do you have? [O D:0]:
    >;
    >;
    >;   MS:    controllers: TS11, TU80, TSV05, TK25
    >;
    >* CP4404  How many TS11/TU80/TSV05/TK25
    >*         magtape controllers do you have? [O D:0]:
    >;
    >;
    >;   DT:    controller:  TC11		device:  TU56
    >;
    >* CP4604  How many TC11 DECtape controllers do you have? [O D:0]:
    >;
    >;
    >;   DX:    controller:  RX11		device:  RX01
    >;
    >* CP4804  How many RX11 disk controllers do you have? [O D:0]:
    >;
    >;
    >;   DY:    controller:  RX211, RXV21	device:  RX02
    >;
    >* CP5004  How many RX211/RXV21 disk controllers do you have? [O D:0]:
    >;
    >;
    >;   DD:    controller:  DL11		device:  TU58
    >;
    >* CP5204  How many TU58 controllers do you have? [O D:0]:
    >;
    >;
    >;   LP:    controllers: LA180, LN01, LP11, LS11, LV11
    >;          devices:     LA180, LG01, LG02, LN01, LP01, LP02, LP04, LP05,
    >;                       LP06,  LP07, LP14, LP25, LP26, LP27, LS11, LV01
    >;
    >* CP5404  How many LP/LS/LV/LG/LN/LA180 line printers do you have? [O D:1]:
    >;
    >* CP5408  Enter the number of seconds between
    >*         line printer-not-ready messages [D R:0.-255. D:15.]: 120
    >;
    >* CP5468  Enter vector address of the next line
    >*         printer [O R:60-774 D:200]:
    >;
    >* CP5472  What is its CSR address? [O R:160000-177700 D:177514]:
    >;
    >* CP5480  Enter line printer type for LPA [S R:4-5 D:"LP25"]:
    >;
    >* CP5484  Does LPA have lowercase characters? [Y/N D:N]:
    >;
    >;
    >;   MT:    controllers: TM11, TMA11, TMB11   devices: TE10, TU10, TU10W, TS03
    >;
    >* CP5604  How many TM/TMA/TMB11 magtape controllers do you have? [O D:0]:
    >;
    >;
    >;   PP:    controller:  PC11
    >;
    >* CP5804  How many PC11 paper tape reader/punches do you have? [O D:0]:
    >;
    >;
    >;   PR:    controller:  PR11
    >;
    >* CP6004  How many PR11 paper tape readers do you have? [O D:0]:
    >;
    >;
    >;   LA:    controller:  LPA11
    >;
    >* CP6204  How many LPA11 lab subsystems do you have? [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:    controllers: DL11, DLV11    controller mnemonic: YL
    >;
    >* CP6804  Enter number of additional DL11/DLV11 line interfaces [O D:4]:
    >;
    >* CP6820  Do any of the DL11/DLV11 lines require modem support? [Y/N D:N]:
    >;
    >* CP6832  Enter terminal type for YLA [S R:4-6 D:"LA120"]: VT2XX
    >;
    >* CP6868  Enter vector address of YLB [O R:300-770 D:300]:
    >;
    >* CP6872  What is its CSR address? [O R:160000-177700 D:176500]:
    >;
    >* CP6832  Enter terminal type for YLB [S R:4-6 D:"LA120"]: VT2XX
    >;
    >* CP6868  Enter vector address of YLC [O R:300-770 D:310]:
    >;
    >* CP6872  What is its CSR address? [O R:160000-177700 D:176510]:
    >;
    >* CP6832  Enter terminal type for YLC [S R:4-6 D:"LA120"]: VT2XX
    >;
    >* CP6868  Enter vector address of YLD [O R:300-770 D:320]:
    >;
    >* CP6872  What is its CSR address? [O R:160000-177700 D:176520]:
    >;
    >* CP6832  Enter terminal type for YLD [S R:4-6 D:"LA120"]: VT2XX
    >;
    >* CP6868  Enter vector address of YLE [O R:300-770 D:330]:
    >;
    >* CP6872  What is its CSR address? [O R:160000-177700 D:176530]:
    >;
    >* CP6832  Enter terminal type for YLE [S R:4-6 D:"LA120"]: VT2XX
    >;
    >;
    >;   TT:    controller:  DH11           controller mnemonic: YH
    >;
    >* CP7004  Enter number of DH11 asynchronous line
    >*         multiplexers [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:    				   controller mnemonic: YV
    >;
    >;   	controllers: DHU11, DHV11, CXA16, CXB16, CXY08
    >;
    >;
    >* CP7104  Enter number of DHU11/DHV11/CXA16/CXB16/CXY08 (YV:-type)
    >*         asynchronous line multiplexers [D R:0.-32. D:0.]:
    >;
    >;
    >;   TT:    controller:  DJ11           controller mnemonic: YJ
    >;
    >* CP7204  Enter number of DJ11 asynchronous line
    >*         multiplexers [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:    controllers: DZ11, DZQ11, DZV11, DFA01    controller mnemonic: YZ
    >;
    >* CP7404  Enter number of DZ11/DZQ11/DZV11/DFA01 asynchronous line
    >*         multiplexers [D R:0.-32. D:0.]:
    >;
    >;
    >* CP7604  Do you have any intercomputer communication devices? [Y/N D:N]:
    >;
    >;
    >; Enter device mnemonics for any user-supplied drivers.  The driver
    >; source files must reside in [11,10] and be named ddDRV.MAC and
    >; ddTAB.MAC where dd is the device mnemonic.
    >;
    >; You may enter the mnemonics on more than one line.  When you have
    >; listed all the drivers, press RETURN when asked for the device
    >; mnemonic.
    >;
    >; The device mnemonic must not include a colon.
    >;
    >* CP9604  Enter device mnemonics for user-supplied drivers [S]:
    >;
    >;
    >; The highest vector among the devices you specified in this SYSGEN
    >; is 374(octal).  This is the default response for this question.
    >;
    >* CP9632  What is the highest interrupt vector
    >*         address? [O R:374-774 D:374]:
    >;
    >;
    >;
    >;================================================================
    >;  Assembling the Executive and Drivers      01-MAY-21 at 13:15
    >;================================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >PIP RSXMC3.MAC=RSXMC1.MAC,RSXMC2.MAC
    >PIP RSXMC.MAC=RSXMC3.MAC,RSXMC0.MAC
    >;
    >SET /UIC=[1,24]
    >PIP [11,10]/NV=[200,200]RSXMC.MAC
    >PIP [11,10]/NV=[200,200]SYSTB.MAC
    >PIP [11,24]/NV=[200,200]RSXASM.CMD
    >PIP [11,24]/NV=[200,200]DRIVERS.ASM
    >;
    >;
    >* AE010   Do you want assembly listings of the Executive and
    >*         drivers? [Y/N D:N]:
    >;
    >ASN NL:=LS:
    >;
    >;
    >* AE030   Do you wish to pause to edit any files before
    >*         assembling? [Y/N D:N]:
    >;
    >SET /UIC=[11,24]
    >;
    >PIP *.OBJ;*/DE/NM,*.TTY;*
    >;
    >TIME
    13:16:26 1-MAY-21
    >;
    >MAC @RSXASM
    >;
    >TIME
    14:00:32 1-MAY-21
    >;
    >MAC @DRIVERS.ASM
    >;
    >TIME
    14:26:46 1-MAY-21
    >;
    >PIP RSX11M.OBS=*.OBJ
    >PIP TTDRV.OBS=*.TTY
    >;
    >SET /UIC=[200,200]
    >PIP /NV=[11,10]RSXMC.MAC
    >;
    >SET /UIC=[1,24]
    >PIP RSXBLD.CMD/PU/NM
    >PIP RSX11M.OLB;*/DE/NM
    >PIP [200,200]RSXMC.MAC/PU/NM
    >;
    >LBR RSX11M/CR:256.::256./-EP=[11,24]RSX11M.OBS
    >PIP [11,24]RSX11M.OBS;*,*.OBJ;*/DE
    >;
    >LBR TTDRV/CR:40.:392.:128.=[11,24]TTDRV.OBS
    >PIP [11,24]TTDRV.OBS;*,*.TTY;*/DE
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;==============================================================
    >;  Building the Executive and Drivers      01-MAY-21 at 14:31
    >;==============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >;
    >; Allocate space to be used later for the system image file.
    >;
    >SET /UIC=[1,54]
    >PIP RSX11M.TMP/CO/BL:1026.=NL:
    >;
    >SET /UIC=[200,200]
    >;
    >SET /UIC=[1,24]
    >SET /UIC=[200,200]
    >SET /UIC=[1,54]
    >PIP SYSVMR.CMD=[200,200]SYSVMR.CMD,VMRTTY.CMD
    >;
    >SET /UIC=[200,200]
    >;
    >* BE030   Do you want to pause to edit any files before
    >*         task-building? [Y/N D:N]:
    >;
    >SET /UIC=[1,24]
    >PIP [1,24]/NV/NM=[200,200]RSXBLD.CMD,RSX11M,DSP11M,LDR11M
    >PIP [1,24]/NV=[200,200]DIR11M.CMD,DR211M,DIRCOM,DR2COM,DIR
    >PIP [1,24]/NV=[200,200]DR311M.CMD,DR411M,DR3COM,DR4COM
    >PIP [1,24]/NV=[200,200]VEC11M.CMD,DCM11M,VECCOM
    >;
    >TIME
    14:33:17 1-MAY-21
    >;
    >TKB @RSXBLD
    >;
    >TIME
    14:48:48 1-MAY-21
    >;
    >TKB @[200,200]DRIVERS.BLD
    >;
    >TIME
    14:54:32 1-MAY-21
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;=========================================================
    >;  Building the Privileged Task      01-MAY-21 at 14:54
    >;=========================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >;
    >* BP040   Do you want the maps of the privileged tasks? [Y/N D:N]: Y
    >;
    >* BP050   What is to be the map device [ddu:]? [S R:2-5 D:"SY:"]:
    >;
    >ASN SY:=MP:
    >;
    >SET /UIC=[1,24]
    >;
    >TIME
    14:54:41 1-MAY-21
    >;
    >TKB @SAVBLD
    >;
    >TIME
    14:57:36 1-MAY-21
    >;
    >ASN LB:=OU:
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;============================================================
    >;  Rebuilding Supplied System Tasks      01-MAY-21 at 14:57
    >;============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA3.CMD.
    >;
    >;
    >* BN010   Do you want to rebuild any system tasks? [Y/N D:N]:
    >;
    >;
    >;
    >;==========================================================
    >;  Creating the System Image File      01-MAY-21 at 14:57
    >;==========================================================
    >;
    >;
    >SET /UIC=[1,54]
    >;
    >PIP RSX11M.TMP;*/DE/NM
    >;
    >PIP RSX11M.SYS/CO/NV/BL:1026.=RSX11M.TSK
    >;
    >ASN LB:=SY:
    >VMR @SYSVMR

    Loading Executive data space
    Data space loading completed
    VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
    SET /TOP=SYSPAR:-*
    VMR -- *DIAG*-Loadable driver larger than 4K
    LOA TT:
    VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
    SET /TOP=DRVPAR:-*
    SECPOL 117734 00200400 00100000  SEC POOL
    SYSPAR 117670 00300400 00205600  MAIN
           117624 00300400 00115300  RO COM !DIR11M!
           117434 00415700 00005200  TASK   [...LDR]
           117230 00423100 00033500  TASK   [MCR...]
           117024 00456600 00010500  TASK   [TKTN  ]
           116620 00467300 00003200  TASK   [SHF...]
           116414 00472500 00013500  TASK   [RCT...]
    DRVPAR 116334 00506200 00145300  MAIN
           116270 00506200 00006600  RO COM !TTEXT !
           116204 00515000 00020600  RO COM !TTCOM !
           116120 00535600 00034200  DRIVER (TT:)
           116054 00572000 00005100  RO COM !PUCOM !
           115254 00577100 00014000  DRIVER (DU:)
           114720 00613100 00011500  DRIVER (MU:)
           112310 00624600 00000700  DRIVER (DA:)
           112070 00625500 00001300  DRIVER (LP:)
           111700 00627000 00000100  DRIVER (NL:)
           111634 00627100 00017700  DRIVER (VF:)
           111570 00647000 00000300  DRIVER (CO:)
           111524 00647300 00002500  DRIVER (VT:)
           111460 00652000 00001500  DRIVER (RD:)
    GEN    111414 00653500 01124300  MAIN
    ...LDR 12.01  117500  SYSPAR 248. 00005200 LB0:-00344344 FIXED
    TKTN   07.01  117070  SYSPAR 248. 00010500 LB0:-00233555 FIXED
    F11MSG 15.00  107334  GEN    200. 00006300 LB0:-00222042
    MTAACP 17.00  106740  GEN    200. 00016200 LB0:-00226524
    SHE... 06.01  106470  GEN    200. 00014500 LB0:-00232173
    MCR... 07.00  117274  SYSPAR 160. 00033500 LB0:-00225503 FIXED
    F11ACP 07.00D 111200  GEN    149. 00041000 LB0:-00220562
    ERRLOG 05.03  110640  GEN    148. 00056200 LB0:-00220430
    PMT... 02.02  110200  GEN    148. 00007500 LB0:-00227434
    COT... 02.04  107460  GEN    145. 00014300 LB0:-00214666
    HRC... 05.00  107064  GEN    140. 00042500 LB0:-00222626
    PMD... 07.05  106614  GEN    140. 00017600 LB0:-00227404
    SYSLOG 04.03  107730  GEN    130. 00024500 LB0:-00232433
    SHF... 07.01  116664  SYSPAR 105. 00003200 LB0:-00232212 FIXED
    RCT... 06.02  116460  SYSPAR 100. 00013500 LB0:-00230077 FIXED
    FXR... 03.02  107210  GEN    100. 00003300 LB0:-00222034
    BAP0   04.11  110764  GEN     80. 00050300 LB0:-00212344
    QMG... 06.04  110054  GEN     75. 00037300 LB0:-00230036
    LP0    07.04  110420  GEN     70. 00020300 LB0:-00225021
    ACNT   06.04  107604  GEN     50. 00057100 LB0:-00211727
    SHUTUP 04.04  106344  GEN     50. 00016500 LB0:-00232217
    ...RMD 05.00  002042+ GEN    225. 00042000 LB0:-00230121
    ...DCL 06.01  002016+ GEN    160. 00062500 LB0:-00215172
    ...DMO 04.02  002020+ GEN    160. 00017300 LB0:-00216145
    ...MCR 07.00  002034+ GEN    160. 00040300 LB0:-00225541
    ...MOU 26.06  002036+ GEN    160. 00045600 LB0:-00226433
    ...CA. 01.00  002072+ GEN    150. 00026100 LB0:-00232462
    ...INS 16.00  002032+ GEN    100. 00053200 LB0:-00223514
    ...SAV 11.00  002066+ GEN    100. 00071100 LB0:-00347613
    ...UFD 07.02  002074+ GEN    100. 00014500 LB0:-00233570
    ...VCP V04.10 002076+ GEN     90. 00020300 LB0:-00233756
    ...ACS 04.00  002050+ GEN     70. 00006200 LB0:-00212164
    ...ACC 05.00  002010+ GEN     65. 00032100 LB0:-00211470
    ...SHA 06.01  002070+ GEN     65. 00032000 LB0:-00232020
    ...AT. 10.0   002024+ GEN     64. 00056500 LB0:-00223100
    ...INI 24.00  002026+ GEN     60. 00037200 LB0:-00223420
    ...HOM 24.00  002030+ GEN     60. 00037200 LB0:-00223420
    ...BRO 09.10  002012+ GEN     50. 00041500 LB0:-00212472
    ...BYE 05.01  002014+ GEN     50. 00021700 LB0:-00212777
    ...HEL 06.00  002022+ GEN     50. 00031600 LB0:-00222172
    ...PIP 21.00  002040+ GEN     50. 00027500 LB0:-00227131
    ...UNL 05.04  002044+ GEN     50. 00021500 LB0:-00233704
    ...ACD 03.00  002046+ GEN     50. 00042500 LB0:-00211561
    ...BOO 03.10  002052+ GEN     50. 00047600 LB0:-00212271
    ...CON 05.00  002054+ GEN     50. 00135600 LB0:-00214464
    ...ELI 04.03  002056+ GEN     50. 00032600 LB0:-00220373
    ...LOA 05.03  002060+ GEN     50. 00040000 LB0:-00224624
    ...MAG 03.00  002062+ GEN     50. 00037300 LB0:-00225441
    ...PSW 03.02  002064+ GEN     50. 00017500 LB0:-00227521
    YLA	OFL	CPA	CSR=177560	VEC=60	PRI=5
    YLB	OFL	CPA	CSR=176500	VEC=300	PRI=5
    YLC	OFL	CPA	CSR=176510	VEC=310	PRI=5
    YLD	OFL	CPA	CSR=176520	VEC=320	PRI=5
    YLE	OFL	CPA	CSR=176530	VEC=330	PRI=5
    DUA	OFL	CPA	CSR=172150	VEC=154	PRI=5
    MUA	OFL	CPA	CSR=174500	VEC=260	PRI=5
    DAA	OFL	CPA	CSR=177220	VEC=174	PRI=4
    LPA	OFL	CPA	CSR=177514	VEC=200	PRI=4
    VF0:			OFL	DRIVER
    VF1:			OFL	DRIVER
    CO0:			OFL	DRIVER
    TT0:	YLA0:		OFL	DRIVER
    TT1:	YLB0:		OFL	DRIVER
    TT2:	YLC0:		OFL	DRIVER
    TT3:	YLD0:		OFL	DRIVER
    TT4:	YLE0:		OFL	DRIVER
    VT0:			OFL	DRIVER
    RD0:			ONL	DRIVER
    DU0:	DUA0:		OFL	DRIVER
    DU1:	DUA1:		OFL	DRIVER
    DU2:	DUA2:		OFL	DRIVER
    DU3:	DUA3:		OFL	DRIVER
    MU0:	MUA0:		OFL	DRIVER
    DA0:	DAA0:		OFL	DRIVER
    DA1:	DAA1:		OFL	DRIVER
    DA2:	DAA2:		OFL	DRIVER
    DA3:	DAA3:		OFL	DRIVER
    DA4:	DAA4:		OFL	DRIVER
    DA5:	DAA5:		OFL	DRIVER
    DA6:	DAA6:		OFL	DRIVER
    DA7:	DAA7:		OFL	DRIVER
    DA10:	DAA10:		OFL	DRIVER
    DA11:	DAA11:		OFL	DRIVER
    DA12:	DAA12:		OFL	DRIVER
    DA13:	DAA13:		OFL	DRIVER
    DA14:	DAA14:		OFL	DRIVER
    DA15:	DAA15:		OFL	DRIVER
    DA16:	DAA16:		OFL	DRIVER
    DA17:	DAA17:		OFL	DRIVER
    DA20:	DAA20:		OFL	DRIVER
    DA21:	DAA21:		OFL	DRIVER
    DA22:	DAA22:		OFL	DRIVER
    DA23:	DAA23:		OFL	DRIVER
    DA24:	DAA24:		OFL	DRIVER
    DA25:	DAA25:		OFL	DRIVER
    DA26:	DAA26:		OFL	DRIVER
    DA27:	DAA27:		OFL	DRIVER
    DA30:	DAA30:		OFL	DRIVER
    DA31:	DAA31:		OFL	DRIVER
    DA32:	DAA32:		OFL	DRIVER
    DA33:	DAA33:		OFL	DRIVER
    DA34:	DAA34:		OFL	DRIVER
    DA35:	DAA35:		OFL	DRIVER
    DA36:	DAA36:		OFL	DRIVER
    DA37:	DAA37:		OFL	DRIVER
    LP0:	LPA0:		OFL	DRIVER
    NL0:			OFL	DRIVER
    POOL=1200:12900.:12900.:2004
    >SET /UIC=[200,200]
    >;
    >REM MACT0
    >REM PIPT0
    >REM LBRT0
    >REM TKBT0
    >REM VMRT0
    >;
    >; End of SYSGEN
    >;
    >TIME
    15:05:03 1-MAY-21
    >;
    >ASN =
    >;
    >@
    >BOO [1,54]
    XDT: 87

    XDT>G
    RSX-11M-PLUS V4.6   BL87

    >

    >TIM 15:07 1-MAY-2021
    >SAV /WB/MOU="/ACP=UNIQUE"

    RSX-11M-PLUS V4.6  BL87   2044.KW  System:"BIGSYS"
    >RED DA37:=SY:
    >RED DA37:=LB:
    >RED DA37:=SP:
    >MOU DA37:"RSX11MPBL87"/ACP=UNIQUE
    >@DA37:[1,2]STARTUP
    >; 			PLEASE NOTE
    >;
    >;	If you have not yet read the system release notes, please do so
    >;	now before attempting to perform a SYSGEN or to utilize the new
    >;	features of this system.
    >;
    >;
    >* Please enter time and date (HH:MM DD-MMM-YYYY) [S]: