    >@SYSGEN
    >;
    >; RSX-11M-PLUS  V4.6  BL87  SYSGEN
    >;
    >; Copyright (c) 1995-1999 by Mentec Inc., U.S.A.
    >;
    >SET /DPRO=[RWED,RWED,RWE,R]
    >;
    >; To exit from the SYSGEN procedure at any time, type CTRL/Z.
    >;
    >; If you are unsure of the answer to a question for which a de-
    >; fault answer exists, use the default answer.
    >;
    >;
    >;
    >;===================================================
    >;  Choosing SYSGEN Options      16-APR-21 at 18:24
    >;===================================================
    >;
    >;
    >;
    >; Every question is preceded by a question number (for example SU010)
    >; which you can use to find the explanation of the question in the
    >; RSX-11M-PLUS System Generation and Installation Guide.
    >;
    >; An explanation of every question is also available by pressing
    >; the ESC key (or the ALTMODE key) in response to the question.
    >;
    >; If you are unfamiliar with the SYSGEN procedure, the explanation of
    >; each question can be printed automatically before the question.
    >;
    >* SU010   Do you always want the explanation printed? [Y/N D:N]:
    >;
    >; SYSGEN always creates saved answer files containing your responses
    >; to the SYSGEN questions:
    >;
    >;    SYSGENSA1.CMD     Setup questions, Executive options
    >;    SYSGENSA2.CMD     Peripheral configuration
    >;    SYSGENSA3.CMD     Nonprivileged task builds
    >;
    >; You should perform a PREPGEN first to create saved answer files, and
    >; then perform a SYSGEN, specifying those saved answer files as input
    >; to the Executive, peripheral, and nonprivileged task build sections.
    >;
    >* SU020   Do you want to use a saved answer file as input for
    >*         the Executive options? [Y/N D:N]:
    >;
    >* SU040   Do you want to use a saved answer file as input for
    >*         the peripheral configuration? [Y/N D:N]:
    >;
    >* SU060   Do you want to use a saved answer file as input for
    >*         the nonprivileged task builds? [Y/N D:N]:
    >;
    >* SU080   Do you want to do a PREPGEN? [Y/N D:N]:
    >;
    >* SU090   Enter the name of the disk drive containing your
    >*         target system disk [ddnn:] [S R:2-5]: DA37
    >;
    >ASN DA37:=IN:
    >ASN DA37:=OU:
    >ASN DA37:=LB:
    >ASN DA37:=WK:
    >ASN DA37:=TK:
    >ASN DA37:=BC:
    >ASN DA37:=LI:
    >ASN DA37:=OB:
    >ASN DA37:=EX:
    >ASN DA37:=MP:
    >;
    >* SU100   Do you want to run Autoconfigure on the host system
    >*         hardware? [Y/N D:N]:
    >;
    >; You can:
    >;
    >;    o  do a complete SYSGEN
    >;
    >;    o  continue a previous SYSGEN from where you left off
    >;
    >;    o  do an individual section of SYSGEN
    >;
    >;
    >* SU120   Do you want to do a complete SYSGEN? [Y/N D:Y]:
    >;
    >INS [3,54]MAC/TASK=MACT0
    >INS [3,54]PIP/TASK=PIPT0
    >INS [3,54]LBR/TASK=LBRT0
    >INS [3,54]TKB/TASK=TKBT0
    >INS [3,54]VMR/TASK=VMRT0
    >;
    >;
    >;
    >;======================================================
    >;  Choosing Executive Options      16-APR-21 at 18:31
    >;======================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >; Enter a comment for inclusion in the SYSGENSA1 saved answer file.
    >; The comment may contain more than one line.  The "V" in the right
    >; margin below marks the maximum line length.  When you are done,
    >; press RETURN in response to the prompt.
    >;                                                                             V
    >* Comment [S R:0.-55.]: VM3
    >* Comment [S R:0.-55.]:
    >;
    >* CE010   What is your target processor type? [S R:3.-12. D:"11/70"]: 11/23-PLUS
    >;
    >* CE020   Do you want the Full-functionality Executive? [Y/N D:Y]:
    >;
    >* CE120   Do you want support for communications products
    >*         (such as DECnet, PSI, and LAT)? [Y/N D:N]: Y
    >;
    >* CE130   What is the system name? [S R:0-6 D:"RSXMPL"]:
    >;
    >* CE215   Do you want the default date format to be
    >*         ISO 8601:1988 compliant? [Y/N D:N]:
    >;
    >* CE216   Do you want the default date format to include
    >*         a four digit year? [Y/N D:N]:
    >;
    >* CE264   Do you want IP11 industrial I/O subsystem support? [Y/N D:N]:
    >;
    >* CE270   Do you want to include XDT? [Y/N D:N]:
    >;
    >* CE280   Enter the crash notification device CSR
    >*         address [O R:160000-177700 D:177564]:
    >;
    >; Note:  Enter both the device and the logical unit number.
    >;        For example, MM0: or DL1:.
    >;
    >; Note:  Enter XX: if you desire loadable DU:, DL:, MU:, MS: or MM:
    >;        crash driver support.
    >;
    >* CE290   On what device and unit do you want crash dumps
    >*         to be written? [S R:2-6]: XX:
    >;
    >* CE300   Enter the initial number of virtual disks to be
    >*         included [D R:0.-16. D:2.]:
    >;
    >* CE310   Enter memory size (in K words) [D R:256.-2044. D:256.]:
    >;
    >* CE315   Support UNIBUS memory occupying UNIBUS map address space? [Y/N D:N]:
    >;
    >* CE320   Do you want floating point processor support? [Y/N D:N]:
    >;
    >* CE330   Is your system clock programmable (KW11-P)? [Y/N D:N]:
    >;
    >* CE350   Is your line frequency 50 Hz? [Y/N D:N]: Y
    >;
    >;
    >;
    >;=============================================================
    >;  Choosing Peripheral Configuration      16-APR-21 at 18:31
    >;=============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA2.CMD.
    >;
    >; Enter a comment for inclusion in the SYSGENSA2 saved answer file.
    >; The comment may contain more than one line.  The "V" in the right
    >; margin below marks the maximum line length.  When you are done,
    >; press RETURN in response to the prompt.
    >;                                                                             V
    >* Comment [S R:0.-55.]: VM3
    >* Comment [S R:0.-55.]:
    >;
    >;
    >* CP0604  How many RH controllers do you have? [D R:0.-15. D:4.]: 0
    >;
    >;
    >;   DK:    controller:  RK11		devices: RK05, RK05F
    >;
    >* CP2204  How many RK11 cartridge disk controllers do you have? [O D:0]:
    >;
    >;
    >;   DM:    controllers: RK611, RK711	devices: RK06, RK07
    >;
    >* CP2404  How many RK611/711 disk cartridge controllers do
    >*         you have? [O D:0]:
    >;
    >;
    >;   DL:    controllers: RL11, RLV12	devices: RL01, RL02
    >;
    >* CP2604  How many RL11/RLV11 disk cartridge controllers do
    >*         you have? [O D:0]:
    >;
    >;
    >;   DP:    controller:  RP11		devices: RP02, RPR02, RP03
    >;
    >* CP2804  How many RP11 disk pack controllers do you have? [O D:0]:
    >;
    >;   DU:    controllers: RQZX1, RQDX1, RQDX2, RQDX3,
    >;                       RUX50, RQC25, KDA50, UDA50
    >;
    >;          devices:     RX33, RX50, RD31, RD51, RD52, RD53, RD54,
    >;                       RC25, RA60, RA70, RA71, RA72, RA80, RA81,
    >;                       RA82, RA90, RA92, RZ23L, RZ24L, RZ26x, RZ29B
    >;
    >;   The total of DU and MU controllers cannot be greater than 10.
    >;
    >* CP3004  How many MSCP disk controllers do you have? [D R:0.-10. D:0.]:
    >;
    >;
    >;   MU:    controllers: TK50, TU81, TU81E, TQ81E, RQZX1
    >;
    >* CP3404  How many TMSCP tape controllers do you have? [D R:0.-10. D:0.]:
    >;
    >;
    >;   DA:    controller: AZ11
    >;
    >* CP3604  How many AZ11 disk image controllers do you have? [O R:0-1 D:0]: 1
    >;
    >* CP3608  How many AZ11 disk drives do you have? [D R:1.-32. D:32.]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA0:? [O R:0-37 D:0]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA1:? [O R:0-37 D:1]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA2:? [O R:0-37 D:2]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA3:? [O R:0-37 D:3]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA4:? [O R:0-37 D:4]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA5:? [O R:0-37 D:5]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA6:? [O R:0-37 D:6]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA7:? [O R:0-37 D:7]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA10:? [O R:0-37 D:10]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA11:? [O R:0-37 D:11]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA12:? [O R:0-37 D:12]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA13:? [O R:0-37 D:13]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA14:? [O R:0-37 D:14]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA15:? [O R:0-37 D:15]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA16:? [O R:0-37 D:16]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA17:? [O R:0-37 D:17]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA20:? [O R:0-37 D:20]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA21:? [O R:0-37 D:21]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA22:? [O R:0-37 D:22]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA23:? [O R:0-37 D:23]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA24:? [O R:0-37 D:24]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA25:? [O R:0-37 D:25]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA26:? [O R:0-37 D:26]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA27:? [O R:0-37 D:27]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA30:? [O R:0-37 D:30]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA31:? [O R:0-37 D:31]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA32:? [O R:0-37 D:32]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA33:? [O R:0-37 D:33]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA34:? [O R:0-37 D:34]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA35:? [O R:0-37 D:35]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA36:? [O R:0-37 D:36]:
    >;
    >;
    >* CP3636  What is the physical unit number of DA37:? [O R:0-37 D:37]:
    >;
    >;
    >* CP3668  Enter the vector address of DAA [O R:60-774 D:174]:
    >;
    >* CP3672  What is its CSR address? [O R:160000-177700 D:177220]:
    >;
    >;			  DA Configuration
    >;
    >; 			Physical Unit Number
    >;
    >; 	0	1	2	3	4	5	6	7
    >;
    >; DAA	DA0:	DA1:	DA2:	DA3:	DA4:	DA5:	DA6:	DA7:
    >;
    >;
    >;
    >;   VF:    Virtual disk/tape driver
    >;
    >;
    >;
    >;   CR:    controllers: CM11, CR11
    >;
    >* CP4004  How many CM/CR11 card readers do you have? [O D:0]:
    >;
    >;
    >;   CT:    controller:  TA11		device:  TU60
    >;
    >* CP4204  How many TA11 dual cassettes do you have? [O D:0]:
    >;
    >;
    >;   MS:    controllers: TS11, TU80, TSV05, TK25
    >;
    >* CP4404  How many TS11/TU80/TSV05/TK25
    >*         magtape controllers do you have? [O D:0]:
    >;
    >;
    >;   DT:    controller:  TC11		device:  TU56
    >;
    >* CP4604  How many TC11 DECtape controllers do you have? [O D:0]:
    >;
    >;
    >;   DX:    controller:  RX11		device:  RX01
    >;
    >* CP4804  How many RX11 disk controllers do you have? [O D:0]:
    >;
    >;
    >;   DY:    controller:  RX211, RXV21	device:  RX02
    >;
    >* CP5004  How many RX211/RXV21 disk controllers do you have? [O D:0]:
    >;
    >;
    >;   DD:    controller:  DL11		device:  TU58
    >;
    >* CP5204  How many TU58 controllers do you have? [O D:0]:
    >;
    >;
    >;   LP:    controllers: LA180, LN01, LP11, LS11, LV11
    >;          devices:     LA180, LG01, LG02, LN01, LP01, LP02, LP04, LP05,
    >;                       LP06,  LP07, LP14, LP25, LP26, LP27, LS11, LV01
    >;
    >* CP5404  How many LP/LS/LV/LG/LN/LA180 line printers do you have? [O D:0]:
    >;
    >;
    >;   MT:    controllers: TM11, TMA11, TMB11   devices: TE10, TU10, TU10W, TS03
    >;
    >* CP5604  How many TM/TMA/TMB11 magtape controllers do you have? [O D:0]:
    >;
    >;
    >;   PP:    controller:  PC11
    >;
    >* CP5804  How many PC11 paper tape reader/punches do you have? [O D:0]:
    >;
    >;
    >;   PR:    controller:  PR11
    >;
    >* CP6004  How many PR11 paper tape readers do you have? [O D:0]:
    >;
    >;
    >;   LA:    controller:  LPA11
    >;
    >* CP6204  How many LPA11 lab subsystems do you have? [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:    controllers: DL11, DLV11    controller mnemonic: YL
    >;
    >* CP6804  Enter number of additional DL11/DLV11 line interfaces [O D:0]:
    >;
    >* CP6832  Enter terminal type for YLA [S R:4-6 D:"LA120"]: VT52
    >;
    >;
    >;   TT:    controller:  DH11           controller mnemonic: YH
    >;
    >* CP7004  Enter number of DH11 asynchronous line
    >*         multiplexers [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:    				   controller mnemonic: YV
    >;
    >;   	controllers: DHU11, DHV11, CXA16, CXB16, CXY08
    >;
    >;
    >* CP7104  Enter number of DHU11/DHV11/CXA16/CXB16/CXY08 (YV:-type)
    >*         asynchronous line multiplexers [D R:0.-32. D:0.]:
    >;
    >;
    >;   TT:    controller:  DJ11           controller mnemonic: YJ
    >;
    >* CP7204  Enter number of DJ11 asynchronous line
    >*         multiplexers [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:    controllers: DZ11, DZQ11, DZV11, DFA01    controller mnemonic: YZ
    >;
    >* CP7404  Enter number of DZ11/DZQ11/DZV11/DFA01 asynchronous line
    >*         multiplexers [D R:0.-32. D:0.]:
    >;
    >;
    >* CP7604  Do you have any intercomputer communication devices? [Y/N D:N]:
    >;
    >;
    >; Enter device mnemonics for any user-supplied drivers.  The driver
    >; source files must reside in [11,10] and be named ddDRV.MAC and
    >; ddTAB.MAC where dd is the device mnemonic.
    >;
    >; You may enter the mnemonics on more than one line.  When you have
    >; listed all the drivers, press RETURN when asked for the device
    >; mnemonic.
    >;
    >; The device mnemonic must not include a colon.
    >;
    >* CP9604  Enter device mnemonics for user-supplied drivers [S]:
    >;
    >;
    >; The highest vector among the devices you specified in this SYSGEN
    >; is 374(octal).  This is the default response for this question.
    >;
    >* CP9632  What is the highest interrupt vector
    >*         address? [O R:374-774 D:374]:
    >;
    >;
    >;
    >;================================================================
    >;  Assembling the Executive and Drivers      16-APR-21 at 19:09
    >;================================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >PIP RSXMC3.MAC=RSXMC1.MAC,RSXMC2.MAC
    >PIP RSXMC.MAC=RSXMC3.MAC,RSXMC0.MAC
    >;
    >SET /UIC=[1,24]
    >PIP [11,10]/NV=[200,200]RSXMC.MAC
    >PIP [11,10]/NV=[200,200]SYSTB.MAC
    >PIP [11,24]/NV=[200,200]RSXASM.CMD
    >PIP [11,24]/NV=[200,200]DRIVERS.ASM
    >;
    >;
    >* AE010   Do you want assembly listings of the Executive and
    >*         drivers? [Y/N D:N]:
    >;
    >ASN NL:=LS:
    >;
    >;
    >* AE030   Do you wish to pause to edit any files before
    >*         assembling? [Y/N D:N]:
    >;
    >SET /UIC=[11,24]
    >;
    >PIP *.OBJ;*/DE/NM,*.TTY;*
    >;
    >TIME
    19:11:28 16-APR-21
    >;
    >MAC @RSXASM
    >;
    >TIME
    20:53:17 16-APR-21
    >;
    >MAC @DRIVERS.ASM
    >;
    >TIME
    21:38:26 16-APR-21
    >;
    >PIP RSX11M.OBS=*.OBJ
    >PIP TTDRV.OBS=*.TTY
    >;
    >SET /UIC=[200,200]
    >PIP /NV=[11,10]RSXMC.MAC
    >;
    >SET /UIC=[1,24]
    >PIP RSXBLD.CMD/PU/NM
    >PIP RSX11M.OLB;*/DE/NM
    >PIP [200,200]RSXMC.MAC/PU/NM
    >;
    >LBR RSX11M/CR:256.::256./-EP=[11,24]RSX11M.OBS
    >PIP [11,24]RSX11M.OBS;*,*.OBJ;*/DE
    >;
    >LBR TTDRV/CR:40.:392.:128.=[11,24]TTDRV.OBS
    >PIP [11,24]TTDRV.OBS;*,*.TTY;*/DE
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;==============================================================
    >;  Building the Executive and Drivers      16-APR-21 at 21:42
    >;==============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >;
    >; Allocate space to be used later for the system image file.
    >;
    >SET /UIC=[1,54]
    >PIP RSX11M.TMP/CO/BL:1026.=NL:
    >;
    >SET /UIC=[200,200]
    >;
    >SET /UIC=[1,24]
    >SET /UIC=[200,200]
    >SET /UIC=[1,54]
    >PIP SYSVMR.CMD=[200,200]SYSVMR.CMD,VMRTTY.CMD
    >;
    >SET /UIC=[200,200]
    >;
    >* BE030   Do you want to pause to edit any files before
    >*         task-building? [Y/N D:N]:
    >;
    >SET /UIC=[1,24]
    >PIP [1,24]/NV/NM=[200,200]RSXBLD.CMD,RSX11M,DSP11M,LDR11M
    >PIP [1,24]/NV=[200,200]DIR11M.CMD,DR211M,DIRCOM,DR2COM,DIR
    >PIP [1,24]/NV=[200,200]DR311M.CMD,DR411M,DR3COM,DR4COM
    >PIP [1,24]/NV=[200,200]VEC11M.CMD,DCM11M,VECCOM
    >;
    >TIME
    22:19:00 16-APR-21
    >;
    >TKB @RSXBLD
    >;
    >TIME
    22:47:08 16-APR-21
    >;
    >TKB @[200,200]DRIVERS.BLD
    >;
    >TIME
    22:51:46 16-APR-21
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;=========================================================
    >;  Building the Privileged Task      16-APR-21 at 22:51
    >;=========================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >;
    >* BP040   Do you want the maps of the privileged tasks? [Y/N D:N]: Y
    >;
    >* BP050   What is to be the map device [ddu:]? [S R:2-5 D:"SY:"]:
    >;
    >ASN SY:=MP:
    >;
    >SET /UIC=[1,24]
    >;
    >TIME
    22:54:44 16-APR-21
    >;
    >TKB @SAVBLD
    >;
    >TIME
    23:00:49 16-APR-21
    >;
    >ASN LB:=OU:
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;============================================================
    >;  Rebuilding Supplied System Tasks      16-APR-21 at 23:00
    >;============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA3.CMD.
    >;
    >;
    >* BN010   Do you want to rebuild any system tasks? [Y/N D:N]:
    >;
    >;
    >;
    >;==========================================================
    >;  Creating the System Image File      16-APR-21 at 23:11
    >;==========================================================
    >;
    >;
    >SET /UIC=[1,54]
    >;
    >PIP RSX11M.TMP;*/DE/NM
    >;
    >PIP RSX11M.SYS/CO/NV/BL:1026.=RSX11M.TSK
    >;
    >ASN LB:=SY:
    >VMR @SYSVMR
    VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
    SET /TOP=SYSPAR:-*
    VMR -- *DIAG*-Loadable driver larger than 4K
    LOA TT:/SIZE=16300
    VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
    SET /TOP=DRVPAR:-*
    SECPOL 117734 00120000 00100000  SEC POOL
    SYSPAR 117670 00220000 00166100  MAIN
           117624 00220000 00112100  RO COM !DIR11M!
           117440 00332100 00004400  TASK   [...LDR]
           117240 00336500 00033500  TASK   [MCR...]
           117040 00372200 00010500  TASK   [TKTN  ]
           116640 00402700 00003200  TASK   [SHF...]
    DRVPAR 116560 00406100 00072300  MAIN
           116514 00406100 00006700  RO COM !TTEXT !
           116430 00415000 00036000  DRIVER (TT:)
           114000 00453000 00000700  DRIVER (DA:)
           113570 00453700 00000100  DRIVER (NL:)
           113524 00454000 00017700  DRIVER (VF:)
           113460 00473700 00000300  DRIVER (CO:)
           113414 00474200 00002500  DRIVER (VT:)
           113350 00476700 00001500  DRIVER (RD:)
    GEN    113304 00500400 01277400  MAIN
    ...LDR 12.01  117504  SYSPAR 248. 00004400 LB0:-00215722 FIXED
    TKTN   07.01  117104  SYSPAR 248. 00010500 LB0:-00111705 FIXED
    F11MSG 15.00  111274  GEN    200. 00006300 LB0:-00100173
    MTAACP 17.00  110714  GEN    200. 00016200 LB0:-00104654
    SHE... 06.01  110454  GEN    200. 00014500 LB0:-00110323
    MCR... 07.00  117304  SYSPAR 160. 00033500 LB0:-00103633 FIXED
    F11ACP 07.00  113074  GEN    149. 00011100 LB0:-00076643
    ERRLOG 05.03  112544  GEN    148. 00056200 LB0:-00076561
    PMT... 02.02  112114  GEN    148. 00007500 LB0:-00105564
    COT... 02.04  111414  GEN    145. 00014300 LB0:-00073017
    HRC... 05.00  111034  GEN    140. 00042500 LB0:-00100757
    PMD... 07.05  110574  GEN    140. 00017600 LB0:-00105534
    SYSLOG 04.03  111654  GEN    130. 00024500 LB0:-00110563
    SHF... 07.01  116704  SYSPAR 105. 00003200 LB0:-00110342 FIXED
    FXR... 03.02  111154  GEN    100. 00003300 LB0:-00100165
    BAP0   04.11  112664  GEN     80. 00050300 LB0:-00070475
    QMG... 06.04  111774  GEN     75. 00037300 LB0:-00106166
    LP0    07.04  112330  GEN     70. 00020300 LB0:-00103151
    ACNT   06.04  111534  GEN     50. 00057600 LB0:-00070137
    SHUTUP 04.04  110334  GEN     50. 00016500 LB0:-00110347
    ...RMD 05.00  001236+ GEN    225. 00042000 LB0:-00106251
    ...DCL 06.01  001212+ GEN    160. 00062500 LB0:-00073323
    ...DMO 04.02  001214+ GEN    160. 00017300 LB0:-00074276
    ...MCR 07.00  001230+ GEN    160. 00040300 LB0:-00103671
    ...MOU 26.06  001232+ GEN    160. 00045600 LB0:-00104563
    ...CA. 01.00  001266+ GEN    150. 00026100 LB0:-00110612
    ...INS 16.00  001226+ GEN    100. 00053200 LB0:-00101645
    ...SAV 11.00  001262+ GEN    100. 00071100 LB0:-00216170
    ...UFD 07.02  001270+ GEN    100. 00014500 LB0:-00111720
    ...VCP V04.10 001272+ GEN     90. 00020300 LB0:-00112106
    ...ACS 04.00  001244+ GEN     70. 00006200 LB0:-00070315
    ...ACC 05.00  001204+ GEN     65. 00032100 LB0:-00067623
    ...SHA 06.01  001264+ GEN     65. 00032000 LB0:-00110150
    ...AT. 10.0   001220+ GEN     64. 00056700 LB0:-00101400
    ...INI 24.00  001222+ GEN     60. 00037200 LB0:-00101551
    ...HOM 24.00  001224+ GEN     60. 00037200 LB0:-00101551
    ...BRO 09.10  001206+ GEN     50. 00041500 LB0:-00070623
    ...BYE 05.01  001210+ GEN     50. 00021700 LB0:-00071130
    ...HEL 06.00  001216+ GEN     50. 00031600 LB0:-00100323
    ...PIP 21.00  001234+ GEN     50. 00036400 LB0:-00105354
    ...UNL 05.04  001240+ GEN     50. 00021500 LB0:-00112034
    ...ACD 03.00  001242+ GEN     50. 00042500 LB0:-00067714
    ...BOO 03.10  001246+ GEN     50. 00047600 LB0:-00070422
    ...CON 05.00  001250+ GEN     50. 00135600 LB0:-00072615
    ...ELI 04.03  001252+ GEN     50. 00032600 LB0:-00076524
    ...LOA 05.03  001254+ GEN     50. 00040000 LB0:-00102754
    ...MAG 03.00  001256+ GEN     50. 00037300 LB0:-00103571
    ...PSW 03.02  001260+ GEN     50. 00017500 LB0:-00105651
    YLA	OFL	CPA	CSR=177560	VEC=60	PRI=5
    DAA	OFL	CPA	CSR=177220	VEC=174	PRI=4
    VF0:			OFL	DRIVER
    VF1:			OFL	DRIVER
    CO0:			OFL	DRIVER
    TT0:	YLA0:		OFL	DRIVER
    VT0:			OFL	DRIVER
    RD0:			ONL	DRIVER
    DA0:	DAA0:		OFL	DRIVER
    DA1:	DAA1:		OFL	DRIVER
    DA2:	DAA2:		OFL	DRIVER
    DA3:	DAA3:		OFL	DRIVER
    DA4:	DAA4:		OFL	DRIVER
    DA5:	DAA5:		OFL	DRIVER
    DA6:	DAA6:		OFL	DRIVER
    DA7:	DAA7:		OFL	DRIVER
    DA10:	DAA10:		OFL	DRIVER
    DA11:	DAA11:		OFL	DRIVER
    DA12:	DAA12:		OFL	DRIVER
    DA13:	DAA13:		OFL	DRIVER
    DA14:	DAA14:		OFL	DRIVER
    DA15:	DAA15:		OFL	DRIVER
    DA16:	DAA16:		OFL	DRIVER
    DA17:	DAA17:		OFL	DRIVER
    DA20:	DAA20:		OFL	DRIVER
    DA21:	DAA21:		OFL	DRIVER
    DA22:	DAA22:		OFL	DRIVER
    DA23:	DAA23:		OFL	DRIVER
    DA24:	DAA24:		OFL	DRIVER
    DA25:	DAA25:		OFL	DRIVER
    DA26:	DAA26:		OFL	DRIVER
    DA27:	DAA27:		OFL	DRIVER
    DA30:	DAA30:		OFL	DRIVER
    DA31:	DAA31:		OFL	DRIVER
    DA32:	DAA32:		OFL	DRIVER
    DA33:	DAA33:		OFL	DRIVER
    DA34:	DAA34:		OFL	DRIVER
    DA35:	DAA35:		OFL	DRIVER
    DA36:	DAA36:		OFL	DRIVER
    DA37:	DAA37:		OFL	DRIVER
    NL0:			OFL	DRIVER
    POOL=1200:4480.:04480.:1200
    >SET /UIC=[200,200]
    >;
    >REM MACT0
    >REM PIPT0
    >REM LBRT0
    >REM TKBT0
    >REM VMRT0
    >;
    >; End of SYSGEN
    >;
    >TIME
    23:19:12 16-APR-21
    >;
    >ASN =
    >;
    >@ <EOF>
    >BOO [1,54]
    RSX-11M-PLUS V4.6   BL87

    >

    >TIM 23:55 16-APR-2021
    >SAV /WB/MOU="/ACP=UNIQUE"

    RSX-11M-PLUS V4.6  BL87   512.KW  System:"RSXMPL"
    >RED DA34:=SY:
    >RED DA34:=LB:
    >RED DA34:=SP:
    >MOU DA34:"RSX11MPBL87"/ACP=UNIQUE
    >@DA34:[1,2]STARTUP
    >;                      PLEASE NOTE
    >;
    >;      If you have not yet read the system release notes, please do so
    >;      now before attempting to perform a SYSGEN or to utilize the new
    >;      features of this system.
    >;
    >;
    >* Please enter time and date (HH:MM DD-MMM-YYYY) [S]: