RSX-11M-PLUS V4.6  BL87   2044.KW  System:"Baseline"
>RED DH:=SY:
>RED DH:=LB:
>RED DH:=SP:
>MOU DH0:"RSX11MPBL87"
>@[2,54]BASTART.CMD
>SET /CRASHDEV=MM0:
SET -- Crash device MM000: has been successfully loaded
>;
>* Do you wish to see the Installation Notes? [Y/N]:
>SET /UIC=[200,200]
>;
>;                      PLEASE NOTE
>;
>;      If you have not yet read the system release notes, please do so
>;      now before attempting to perform a SYSGEN or to utilize the new
>;      features of this system.
>;
>;
>;      In order to start the SYSGEN process, type:
>;
>;      >@SYSGEN
>;
>;      When SYSGEN has completed and your generated system is
>;      running, you may wish to edit several supplied prototype
>;      command and text files to suit your system and application:
>;
>;      File                    Purpose
>;      ----                    -------
>;      [0,0]RSX11.SYS          An account/password file
>;                              This file does contain privileged accounts.
>;
>;      [1,2]STARTUP.CMD        (This file) Invoked at bootstrap time to
>;                              control bringing up the system.
>;
>;      [1,2]QMGSTART.CMD       Invoked by STARTUP to start up the Queue
>;                              Manager and spooling system.
>;
>;      [1,2]SHUTUP.CMD         Invoked by SHUTUP when taking down the system
>;                              to perform system dependent shutdown tasks.
>;
>;      [1,2]QMGSTOP.CMD        Invoked by SHUTUP to stop the Queue Manager
>;                              and spooling system.
>;
>;      [1,2]LOGIN.TXT          Displayed on user's terminal when logging in.
>;
>;      [1,2]BATCH.TXT          Displayed at the beginning of each batch log
>;                              file.
>;
>;
>* Please enter time and date (HH:MM DD-MMM-YYYY) [S]: 6-MAY-2021 2:27
>TIME 6-MAY-2021 2:27
>ACS SY:/BLKS=1024.
>CON ONLINE ALL
>ELI /LOG/LIM
>CLI /INIT=DCL/CTRLC/DPR="<15><12>/$ /"
>INS LB:[1,1]RMSRESAB.TSK/RON=YES/PAR=GEN
>INS LB:[1,1]RMSLBL.TSK/RON=YES/PAR=GEN
>INS LB:[1,1]RMSLBM.TSK/RON=YES/PAR=GEN
>INS $QMGCLI
>INS $QMGCLI/TASK=...PRI
>INS $QMGCLI/TASK=...SUB
>QUE /START:QMG
>INS $QMGPRT/TASK=PRT.../SLV=NO
>QUE LP0:/CR/NM
>START/ACCOUNTING
>CON ESTAT LP0:
>QUE LP0:/SP/FL:2/LOWER/FO:0
>QUE BAP0:/BATCH
>QUE LP0:/AS:PRINT
>QUE BAP0:/AS:BATCH
>@ <EOF>
>CON SET SYS $TKPS=50.
>TIM 2:30
>@SYSGEN
>;
>; RSX-11M-PLUS  V4.6  BL87  SYSGEN
>;
>; Copyright (c) 1995-1999 by Mentec Inc., U.S.A.
>;
>SET /DPRO=[RWED,RWED,RWE,R]
>;
>; To exit from the SYSGEN procedure at any time, type CTRL/Z.
>;
>; If you are unsure of the answer to a question for which a de-
>; fault answer exists, use the default answer.
>;
>;
>;
>;===================================================
>;  Choosing SYSGEN Options      06-MAY-21 at 02:30
>;===================================================
>;
>;
>;
>; Every question is preceded by a question number (for example SU010)
>; which you can use to find the explanation of the question in the
>; RSX-11M-PLUS System Generation and Installation Guide.
>;
>; An explanation of every question is also available by pressing
>; the ESC key (or the ALTMODE key) in response to the question.
>;
>; If you are unfamiliar with the SYSGEN procedure, the explanation of
>; each question can be printed automatically before the question.
>;
>* SU010   Do you always want the explanation printed? [Y/N D:N]:
>;
>; SYSGEN always creates saved answer files containing your responses
>; to the SYSGEN questions:
>;
>;    SYSGENSA1.CMD     Setup questions, Executive options
>;    SYSGENSA2.CMD     Peripheral configuration
>;    SYSGENSA3.CMD     Nonprivileged task builds
>;
>; You should perform a PREPGEN first to create saved answer files, and
>; then perform a SYSGEN, specifying those saved answer files as input
>; to the Executive, peripheral, and nonprivileged task build sections.
>;
>* SU020   Do you want to use a saved answer file as input for
>*         the Executive options? [Y/N D:N]:
>;
>* SU040   Do you want to use a saved answer file as input for
>*         the peripheral configuration? [Y/N D:N]:
>;
>* SU060   Do you want to use a saved answer file as input for
>*         the nonprivileged task builds? [Y/N D:N]:
>;
>* SU080   Do you want to do a PREPGEN? [Y/N D:N]:
>;
>* SU090   Enter the name of the disk drive containing your
>*         target system disk [ddnn:] [S R:2-5]: SY
>;
>ASN SY:=IN:
>ASN SY:=OU:
>ASN SY:=LB:
>ASN SY:=WK:
>ASN SY:=TK:
>ASN SY:=BC:
>ASN SY:=LI:
>ASN SY:=OB:
>ASN SY:=EX:
>ASN SY:=MP:
>;
>* SU100   Do you want to run Autoconfigure on the host system
>*         hardware? [Y/N D:N]: Y
>;
>; Running Autoconfigure:
>;
>INS $ACF
>ACF
>INS $ACO
>ACO SHOW
Processor Type:  11/23-PLUS          Memory Size:  2044. Kw
 
Options:
 
        Extended Instruction Set (EIS)
        Extended (22-Bit) Addressing
        Switch Register (SWR)
        Display Register
        Parity Memory
 
Name    Vector     CSR      Unit    Type      Remark
LPA      200      177514
YLA      060      177560
YLB      300      176500
YLC      310      176510
YLD      320      176520
YLE      330      176530
DHA      164      177720
                             0      HD11
                             1      UNKNOWN
                             2      UNKNOWN
                             3      UNKNOWN
                             4      UNKNOWN
                             5      UNKNOWN
                             6      UNKNOWN
                             7      HD11
 
>ACO SYSGEN
>;
>* SU110   Do you want to override the Autoconfigure results? [Y/N D:N]:
>;
>; You can:
>;
>;    o  do a complete SYSGEN
>;
>;    o  continue a previous SYSGEN from where you left off
>;
>;    o  do an individual section of SYSGEN
>;
>;
>* SU120   Do you want to do a complete SYSGEN? [Y/N D:Y]:
>;
>INS [3,54]MAC/TASK=MACT0
>INS [3,54]PIP/TASK=PIPT0
>INS [3,54]LBR/TASK=LBRT0
>INS [3,54]TKB/TASK=TKBT0
>INS [3,54]VMR/TASK=VMRT0
>;
>;
>;
>;======================================================
>;  Choosing Executive Options      06-MAY-21 at 02:30
>;======================================================
>;
>;
>;
>; The answers to the questions in this section are put in the saved
>; answer file [200,200]SYSGENSA1.CMD.
>;
>; Enter a comment for inclusion in the SYSGENSA1 saved answer file.
>; The comment may contain more than one line.  The "V" in the right
>; margin below marks the maximum line length.  When you are done,
>; press RETURN in response to the prompt.
>;                                                                             V
>* Comment [S R:0.-55.]: DVK
>* Comment [S R:0.-55.]:
>;
>* CE020   Do you want the Full-functionality Executive? [Y/N D:Y]:
>;
>* CE120   Do you want support for communications products
>*         (such as DECnet, PSI, and LAT)? [Y/N D:N]: Y
>;
>* CE130   What is the system name? [S R:0-6 D:"RSXMPL"]: KYPEBO
>;
>* CE215   Do you want the default date format to be
>*         ISO 8601:1988 compliant? [Y/N D:N]:
>;
>* CE216   Do you want the default date format to include
>*         a four digit year? [Y/N D:N]:
>;
>* CE264   Do you want IP11 industrial I/O subsystem support? [Y/N D:N]:
>;
>* CE270   Do you want to include XDT? [Y/N D:N]:
>;
>* CE280   Enter the crash notification device CSR
>*         address [O R:160000-177700 D:177564]:
>;
>; Note:  Enter both the device and the logical unit number.
>;        For example, MM0: or DL1:.
>;
>; Note:  Enter XX: if you desire loadable DA:, DH:, DU:, DL:, MU:, MS:
>;        or MM: crash driver support.
>;
>* CE290   On what device and unit do you want crash dumps
>*         to be written? [S R:2-6]: XX:
>;
>* CE300   Enter the initial number of virtual disks to be
>*         included [D R:0.-16. D:2.]:
>;
>* CE315   Support UNIBUS memory occupying UNIBUS map address space? [Y/N D:N]:
>;
>* CE330   Is your system clock programmable (KW11-P)? [Y/N D:N]:
>;
>* CE350   Is your line frequency 50 Hz? [Y/N D:N]: Y
>;
>;
>;
>;=============================================================
>;  Choosing Peripheral Configuration      06-MAY-21 at 02:31
>;=============================================================
>;
>;
>;
>; The answers to the questions in this section are put in the saved
>; answer file [200,200]SYSGENSA2.CMD.
>;
>; Enter a comment for inclusion in the SYSGENSA2 saved answer file.
>; The comment may contain more than one line.  The "V" in the right
>; margin below marks the maximum line length.  When you are done,
>; press RETURN in response to the prompt.
>;                                                                             V
>* Comment [S R:0.-55.]: DVK
>* Comment [S R:0.-55.]:
>;
>;
>;   DH:    controller: HD11
>;
>;                        DH Configuration
>;
>;                      Physical Unit Number
>;
>;      0       1       2       3       4       5       6       7
>;
>; DHA  DH0:    DH1:    DH2:    DH3:    DH4:    DH5:    DH6:    DH7:
>;
>;
>;
>;   VF:    Virtual disk/tape driver
>;
>;
>;
>;   CR:    controllers: CM11, CR11
>;
>* CP4004  How many CM/CR11 card readers do you have? [O D:0]:
>;
>;
>;   LP:    controllers: LA180, LN01, LP11, LS11, LV11
>;          devices:     LA180, LG01, LG02, LN01, LP01, LP02, LP04, LP05,
>;                       LP06,  LP07, LP14, LP25, LP26, LP27, LS11, LV01
>;
>* CP5408  Enter the number of seconds between
>*         line printer-not-ready messages [D R:0.-255. D:15.]: 120
>;
>* CP5480  Enter line printer type for LPA [S R:4-5 D:"LP25"]:
>;
>* CP5484  Does LPA have lowercase characters? [Y/N D:N]:
>;
>;
>;   LA:    controller:  LPA11
>;
>* CP6204  How many LPA11 lab subsystems do you have? [D R:0.-16. D:0.]:
>;
>;
>;   TT:    controllers: DL11, DLV11    controller mnemonic: YL
>;
>* CP6820  Do any of the DL11/DLV11 lines require modem support? [Y/N D:N]:
>;
>* CP6832  Enter terminal type for YLA [S R:4-6 D:"LA120"]: VT52
>;
>* CP6832  Enter terminal type for YLB [S R:4-6 D:"LA120"]: VT52
>;
>* CP6832  Enter terminal type for YLC [S R:4-6 D:"LA120"]: VT52
>;
>* CP6832  Enter terminal type for YLD [S R:4-6 D:"LA120"]: VT52
>;
>* CP6832  Enter terminal type for YLE [S R:4-6 D:"LA120"]: VT52
>;
>;
>;   TT:    controller:  DJ11           controller mnemonic: YJ
>;
>* CP7204  Enter number of DJ11 asynchronous line
>*         multiplexers [D R:0.-16. D:0.]:
>;
>;
>* CP7604  Do you have any intercomputer communication devices? [Y/N D:N]:
>;
>;
>; Enter device mnemonics for any user-supplied drivers.  The driver
>; source files must reside in [11,10] and be named ddDRV.MAC and
>; ddTAB.MAC where dd is the device mnemonic.
>;
>; You may enter the mnemonics on more than one line.  When you have
>; listed all the drivers, press RETURN when asked for the device
>; mnemonic.
>;
>; The device mnemonic must not include a colon.
>;
>* CP9604  Enter device mnemonics for user-supplied drivers [S]:
>;
>;
>; The highest vector among the devices you specified in this SYSGEN
>; is 374(octal).  This is the default response for this question.
>;
>* CP9632  What is the highest interrupt vector
>*         address? [O R:374-774 D:374]:
>;
>;
>;
>;================================================================
>;  Assembling the Executive and Drivers      06-MAY-21 at 02:36
>;================================================================
>;
>;
>;
>; The answers to the questions in this section are put in the saved
>; answer file [200,200]SYSGENSA1.CMD.
>;
>PIP RSXMC3.MAC=RSXMC1.MAC,RSXMC2.MAC
>PIP RSXMC.MAC=RSXMC3.MAC,RSXMC0.MAC
>;
>SET /UIC=[1,24]
>PIP [11,10]/NV=[200,200]RSXMC.MAC
>PIP [11,10]/NV=[200,200]SYSTB.MAC
>PIP [11,24]/NV=[200,200]RSXASM.CMD
>PIP [11,24]/NV=[200,200]DRIVERS.ASM
>;
>;
>* AE010   Do you want assembly listings of the Executive and
>*         drivers? [Y/N D:N]:
>;
>ASN NL:=LS:
>;
>;
>* AE030   Do you wish to pause to edit any files before
>*         assembling? [Y/N D:N]:
>;
>SET /UIC=[11,24]
>;
>PIP *.OBJ;*/DE/NM,*.TTY;*
>;
>TIME
02:36:58 6-MAY-21
>;
>MAC @RSXASM
>;
>TIME
03:53:48 6-MAY-21
>;
>MAC @DRIVERS.ASM
>;
>TIME
04:33:02 6-MAY-21
>;
>PIP RSX11M.OBS=*.OBJ
>PIP TTDRV.OBS=*.TTY
>;
>SET /UIC=[200,200]
>PIP /NV=[11,10]RSXMC.MAC
>;
>SET /UIC=[1,24]
>PIP RSXBLD.CMD/PU/NM
>PIP RSX11M.OLB;*/DE/NM
>PIP [200,200]RSXMC.MAC/PU/NM
>;
>LBR RSX11M/CR:256.::256./-EP=[11,24]RSX11M.OBS
>PIP [11,24]RSX11M.OBS;*,*.OBJ;*/DE
>;
>LBR TTDRV/CR:40.:392.:128.=[11,24]TTDRV.OBS
>PIP [11,24]TTDRV.OBS;*,*.TTY;*/DE
>SET /UIC=[200,200]
>;
>;
>;
>;==============================================================
>;  Building the Executive and Drivers      06-MAY-21 at 04:34
>;==============================================================
>;
>;
>;
>; The answers to the questions in this section are put in the saved
>; answer file [200,200]SYSGENSA1.CMD.
>;
>;
>; Allocate space to be used later for the system image file.
>;
>SET /UIC=[1,54]
>PIP RSX11M.TMP/CO/BL:1026.=NL:
>;
>SET /UIC=[200,200]
>;
>SET /UIC=[1,24]
>SET /UIC=[200,200]
>SET /UIC=[1,54]
>PIP SYSVMR.CMD=[200,200]SYSVMR.CMD,VMRTTY.CMD
>;
>SET /UIC=[200,200]
>;
>* BE030   Do you want to pause to edit any files before
>*         task-building? [Y/N D:N]:
>;
>SET /UIC=[1,24]
>PIP [1,24]/NV/NM=[200,200]RSXBLD.CMD,RSX11M,DSP11M,LDR11M
>PIP [1,24]/NV=[200,200]DIR11M.CMD,DR211M,DIRCOM,DR2COM,DIR
>PIP [1,24]/NV=[200,200]DR311M.CMD,DR411M,DR3COM,DR4COM
>PIP [1,24]/NV=[200,200]VEC11M.CMD,DCM11M,VECCOM
>;
>TIME
04:36:21 6-MAY-21
>;
>TKB @RSXBLD
>;
>TIME
04:54:25 6-MAY-21
>;
>TKB @[200,200]DRIVERS.BLD
>;
>TIME
04:56:49 6-MAY-21
>SET /UIC=[200,200]
>;
>;
>;
>;=========================================================
>;  Building the Privileged Task      06-MAY-21 at 04:56
>;=========================================================
>;
>;
>;
>; The answers to the questions in this section are put in the saved
>; answer file [200,200]SYSGENSA1.CMD.
>;
>;
>* BP040   Do you want the maps of the privileged tasks? [Y/N D:N]: Y
>;
>* BP050   What is to be the map device [ddu:]? [S R:2-5 D:"SY:"]:
>;
>ASN SY:=MP:
>;
>SET /UIC=[1,24]
>;
>TIME
04:57:14 6-MAY-21
>;
>TKB @SAVBLD
>;
>TIME
05:01:28 6-MAY-21
>;
>ASN LB:=OU:
>SET /UIC=[200,200]
>;
>;
>;
>;============================================================
>;  Rebuilding Supplied System Tasks      06-MAY-21 at 05:01
>;============================================================
>;
>;
>;
>; The answers to the questions in this section are put in the saved
>; answer file [200,200]SYSGENSA3.CMD.
>;
>;
>* BN010   Do you want to rebuild any system tasks? [Y/N D:N]:
>;
>;
>;
>;==========================================================
>;  Creating the System Image File      06-MAY-21 at 05:01
>;==========================================================
>;
>;
>SET /UIC=[1,54]
>;
>PIP RSX11M.TMP;*/DE/NM
>;
>PIP RSX11M.SYS/CO/NV/BL:1026.=RSX11M.TSK
>;
>ASN LB:=SY:
>VMR @SYSVMR
VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
SET /TOP=SYSPAR:-*
VMR -- *DIAG*-Loadable driver larger than 4K
LOA TT:/SIZE=16300
VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
SET /TOP=DRVPAR:-*
SECPOL 117734 00120000 00100000  SEC POOL
SYSPAR 117670 00220000 00166100  MAIN
       117624 00220000 00112100  RO COM !DIR11M!
       117440 00332100 00004400  TASK   [...LDR]
       117240 00336500 00033500  TASK   [MCR...]
       117040 00372200 00010500  TASK   [TKTN  ]
       116640 00402700 00003200  TASK   [SHF...]
DRVPAR 116560 00406100 00073500  MAIN
       116514 00406100 00006700  RO COM !TTEXT !
       116430 00415000 00036000  DRIVER (TT:)
       115520 00453000 00000600  DRIVER (DH:)
       115260 00453600 00001300  DRIVER (LP:)
       115050 00455100 00000100  DRIVER (NL:)
       115004 00455200 00017700  DRIVER (VF:)
       114740 00475100 00000300  DRIVER (CO:)
       114674 00475400 00002500  DRIVER (VT:)
       114630 00500100 00001500  DRIVER (RD:)
GEN    114564 00501600 17256200  MAIN
...LDR 12.01  117504  SYSPAR 248. 00004400 LB0:-00215634 FIXED
TKTN   07.01  117104  SYSPAR 248. 00010500 LB0:-00101455 FIXED
F11MSG 15.00  112554  GEN    200. 00006300 LB0:-00067744
MTAACP 17.00  112174  GEN    200. 00016200 LB0:-00074424
SHE... 06.01  111734  GEN    200. 00014500 LB0:-00100073
MCR... 07.00  117304  SYSPAR 160. 00033500 LB0:-00073403 FIXED
F11ACP 07.00  114354  GEN    149. 00011100 LB0:-00066414
ERRLOG 05.03  114024  GEN    148. 00056200 LB0:-00066332
PMT... 02.02  113374  GEN    148. 00007500 LB0:-00075334
COT... 02.04  112674  GEN    145. 00014300 LB0:-00062570
HRC... 05.00  112314  GEN    140. 00042500 LB0:-00054056
PMD... 07.05  112054  GEN    140. 00017600 LB0:-00075304
SYSLOG 04.03  113134  GEN    130. 00024500 LB0:-00100333
SHF... 07.01  116704  SYSPAR 105. 00003200 LB0:-00100112 FIXED
FXR... 03.02  112434  GEN    100. 00003300 LB0:-00067736
BAP0   04.11  114144  GEN     80. 00050300 LB0:-00060247
QMG... 06.04  113254  GEN     75. 00037300 LB0:-00075736
LP0    07.04  113610  GEN     70. 00020300 LB0:-00072721
ACNT   06.04  113014  GEN     50. 00057600 LB0:-00057712
SHUTUP 04.04  111614  GEN     50. 00016500 LB0:-00100117
...RMD 05.00  001236+ GEN    225. 00042000 LB0:-00217703
...DCL 06.01  001212+ GEN    160. 00062500 LB0:-00063074
...DMO 04.02  001214+ GEN    160. 00017300 LB0:-00064047
...MCR 07.00  001230+ GEN    160. 00040300 LB0:-00217375
...MOU 26.06  001232+ GEN    160. 00045600 LB0:-00074333
...CA. 01.00  001266+ GEN    150. 00026100 LB0:-00100362
...INS 16.00  001226+ GEN    100. 00053200 LB0:-00071415
...SAV 11.00  001262+ GEN    100. 00071400 LB0:-00225407
...UFD 07.02  001270+ GEN    100. 00014500 LB0:-00101470
...VCP V04.10 001272+ GEN     90. 00020300 LB0:-00101656
...ACS 04.00  001244+ GEN     70. 00006200 LB0:-00060070
...ACC 05.00  001204+ GEN     65. 00032100 LB0:-00057376
...SHA 06.01  001264+ GEN     65. 00032000 LB0:-00077720
...AT. 10.0   001220+ GEN     64. 00056700 LB0:-00071150
...INI 24.00  001222+ GEN     60. 00037200 LB0:-00071321
...HOM 24.00  001224+ GEN     60. 00037200 LB0:-00071321
...BRO 09.10  001206+ GEN     50. 00041500 LB0:-00060375
...BYE 05.01  001210+ GEN     50. 00021700 LB0:-00060701
...HEL 06.00  001216+ GEN     50. 00031600 LB0:-00070074
...PIP 21.00  001234+ GEN     50. 00036400 LB0:-00075124
...UNL 05.04  001240+ GEN     50. 00021500 LB0:-00101604
...ACD 03.00  001242+ GEN     50. 00042500 LB0:-00057467
...BOO 03.10  001246+ GEN     50. 00050000 LB0:-00053740
...CON 05.00  001250+ GEN     50. 00135600 LB0:-00062366
...ELI 04.03  001252+ GEN     50. 00032600 LB0:-00066275
...LOA 05.03  001254+ GEN     50. 00040000 LB0:-00072524
...MAG 03.00  001256+ GEN     50. 00037300 LB0:-00073341
...PSW 03.02  001260+ GEN     50. 00017500 LB0:-00075421
YLA     OFL     CPA     CSR=177560      VEC=60  PRI=5
YLB     OFL     CPA     CSR=176500      VEC=300 PRI=5
YLC     OFL     CPA     CSR=176510      VEC=310 PRI=5
YLD     OFL     CPA     CSR=176520      VEC=320 PRI=5
YLE     OFL     CPA     CSR=176530      VEC=330 PRI=5
DHA     OFL     CPA     CSR=177720      VEC=164 PRI=5
LPA     OFL     CPA     CSR=177514      VEC=200 PRI=4
VF0:                    OFL     DRIVER
VF1:                    OFL     DRIVER
CO0:                    OFL     DRIVER
TT0:    YLA0:           OFL     DRIVER
TT1:    YLB0:           OFL     DRIVER
TT2:    YLC0:           OFL     DRIVER
TT3:    YLD0:           OFL     DRIVER
TT4:    YLE0:           OFL     DRIVER
VT0:                    OFL     DRIVER
RD0:                    ONL     DRIVER
DH0:    DHA0:           OFL     DRIVER
DH1:    DHA1:           OFL     DRIVER
DH2:    DHA2:           OFL     DRIVER
DH3:    DHA3:           OFL     DRIVER
DH4:    DHA4:           OFL     DRIVER
DH5:    DHA5:           OFL     DRIVER
DH6:    DHA6:           OFL     DRIVER
DH7:    DHA7:           OFL     DRIVER
LP0:    LPA0:           OFL     DRIVER
NL0:                    OFL     DRIVER
POOL=1200:4604.:04604.:1200
>SET /UIC=[200,200]
>;
>REM MACT0
>REM PIPT0
>REM LBRT0
>REM TKBT0
>REM VMRT0
>;
>; End of SYSGEN
>;
>TIME
05:03:29 6-MAY-21
>;
>ASN =
>;
>@ <EOF>
>BOO [1,54]
RSX-11M-PLUS V4.6   BL87
 
 
>
 
>TIM 5:3 6-MAY-2021
>SAV /WB/MOU="/ACP=UNIQUE"
 
 
RSX-11M-PLUS V4.6  BL87   2044.KW  System:"KYPEBO"
>RED DH:=SY:
>RED DH:=LB:
>RED DH:=SP:
>MOU DH0:"RSX11MPBL87"/ACP=UNIQUE
>@DH:[1,2]STARTUP
>;                      PLEASE NOTE
>;
>;      If you have not yet read the system release notes, please do so
>;      now before attempting to perform a SYSGEN or to utilize the new
>;      features of this system.
>;
>;
>* Please enter time and date (HH:MM DD-MMM-YYYY) [S]:
