    RSX-11M-PLUS V4.6  BL87   512.KW  System:"Baseline"
    >RED HD7:=SY:
    >RED HD7:=LB:
    >RED HD7:=SP:
    >MOU HD7:"RSX11MPBL87"
    >@[2,54]BASTART.CMD
    >SET /CRASHDEV=MM0:
    SET -- Crash device MM000: has been successfully loaded
    >;
    >* Do you wish to see the Installation Notes? [Y/N]:
    >SET /UIC=[200,200]
    >;
    >;                      PLEASE NOTE
    >;
    >;      If you have not yet read the system release notes, please do so
    >;      now before attempting to perform a SYSGEN or to utilize the new
    >;      features of this system.
    >;
    >;
    >;      In order to start the SYSGEN process, type:
    >;
    >;      >@SYSGEN
    >;
    >;      When SYSGEN has completed and your generated system is
    >;      running, you may wish to edit several supplied prototype
    >;      command and text files to suit your system and application:
    >;
    >;      File                    Purpose
    >;      ----                    -------
    >;      [0,0]RSX11.SYS          An account/password file
    >;                              This file does contain privileged accounts.
    >;
    >;      [1,2]STARTUP.CMD        (This file) Invoked at bootstrap time to
    >;                              control bringing up the system.
    >;
    >;      [1,2]QMGSTART.CMD       Invoked by STARTUP to start up the Queue
    >;                              Manager and spooling system.
    >;
    >;      [1,2]SHUTUP.CMD         Invoked by SHUTUP when taking down the system
    >;                              to perform system dependent shutdown tasks.
    >;
    >;      [1,2]QMGSTOP.CMD        Invoked by SHUTUP to stop the Queue Manager
    >;                              and spooling system.
    >;
    >;      [1,2]LOGIN.TXT          Displayed on user's terminal when logging in.
    >;
    >;      [1,2]BATCH.TXT          Displayed at the beginning of each batch log
    >;                              file.
    >;
    >;
    >* Please enter time and date (HH:MM DD-MMM-YYYY) [S]: 22:01 27-NOV-2016
    >TIME 22:01 27-NOV-2016
    >ACS SY:/BLKS=1024.
    >CON ONLINE ALL
    >ELI /LOG/LIM
    >CLI /INIT=DCL/CTRLC/DPR="<15><12>/$ /"
    >INS LB:[1,1]RMSRESAB.TSK/RON=YES/PAR=GEN
    >INS LB:[1,1]RMSLBL.TSK/RON=YES/PAR=GEN
    >INS LB:[1,1]RMSLBM.TSK/RON=YES/PAR=GEN
    >INS $QMGCLI
    >INS $QMGCLI/TASK=...PRI
    >INS $QMGCLI/TASK=...SUB
    >QUE /START:QMG
    >INS $QMGPRT/TASK=PRT.../SLV=NO
    >QUE LP0:/CR/NM
    >START/ACCOUNTING
    >CON ESTAT LP0:
    >QUE LP0:/SP/FL:2/LOWER/FO:0
    >QUE BAP0:/BATCH
    >QUE LP0:/AS:PRINT
    >QUE BAP0:/AS:BATCH
    >@ <EOF>
    >@SYSGEN
    >;
    >; RSX-11M-PLUS  V4.6  BL87  SYSGEN
    >;
    >; Copyright (c) 1995-1999 by Mentec Inc., U.S.A.
    >;
    >SET /DPRO=[RWED,RWED,RWE,R]
    >;
    >; To exit from the SYSGEN procedure at any time, type CTRL/Z.
    >;
    >; If you are unsure of the answer to a question for which a de-
    >; fault answer exists, use the default answer.
    >;
    >;
    >;
    >;===================================================
    >;  Choosing SYSGEN Options      27-NOV-16 at 22:01
    >;===================================================
    >;
    >;
    >;
    >; Every question is preceded by a question number (for example SU010)
    >; which you can use to find the explanation of the question in the
    >; RSX-11M-PLUS System Generation and Installation Guide.
    >;
    >; An explanation of every question is also available by pressing
    >; the ESC key (or the ALTMODE key) in response to the question.
    >;
    >; If you are unfamiliar with the SYSGEN procedure, the explanation of
    >; each question can be printed automatically before the question.
    >;
    >* SU010   Do you always want the explanation printed? [Y/N D:N]:
    >;
    >; SYSGEN always creates saved answer files containing your responses
    >; to the SYSGEN questions:
    >;
    >;    SYSGENSA1.CMD     Setup questions, Executive options
    >;    SYSGENSA2.CMD     Peripheral configuration
    >;    SYSGENSA3.CMD     Nonprivileged task builds
    >;
    >; You should perform a PREPGEN first to create saved answer files, and
    >; then perform a SYSGEN, specifying those saved answer files as input
    >; to the Executive, peripheral, and nonprivileged task build sections.
    >;
    >* SU020   Do you want to use a saved answer file as input for
    >*         the Executive options? [Y/N D:N]:
    >;
    >* SU040   Do you want to use a saved answer file as input for
    >*         the peripheral configuration? [Y/N D:N]:
    >;
    >* SU060   Do you want to use a saved answer file as input for
    >*         the nonprivileged task builds? [Y/N D:N]:
    >;
    >* SU080   Do you want to do a PREPGEN? [Y/N D:N]:
    >;
    >* SU090   Enter the name of the disk drive containing your
    >*         target system disk [ddnn:] [S R:2-5]: LB
    >;
    >ASN LB:=IN:
    >ASN LB:=OU:
    >ASN LB:=LB:
    >ASN LB:=WK:
    >ASN LB:=TK:
    >ASN LB:=BC:
    >ASN LB:=LI:
    >ASN LB:=OB:
    >ASN LB:=EX:
    >ASN LB:=MP:
    >;
    >* SU100   Do you want to run Autoconfigure on the host system
    >*         hardware? [Y/N D:N]: Y
    >;
    >; Running Autoconfigure:
    >;
    >INS $ACF
    >ACF
    >INS $ACO
    >ACO SHOW
    Processor Type:  LSI-11/73          Memory Size:  124. Kw

    Options:

            Extended Instruction Set (EIS)
            Parity Memory

    Name    Vector     CSR      Unit    Type      Remark
    DKA      220      177404
                                 0      RK05
    DXA      264      177170
    LPA      200      177514
    MTA      224      172522
    PPA      074      177554
    PRA      070      177550
    YLA      060      177560

    >ACO SYSGEN
    >;
    >* SU110   Do you want to override the Autoconfigure results? [Y/N D:N]: Y
    >;
    >; You can:
    >;
    >;    o  do a complete SYSGEN
    >;
    >;    o  continue a previous SYSGEN from where you left off
    >;
    >;    o  do an individual section of SYSGEN
    >;
    >;
    >* SU120   Do you want to do a complete SYSGEN? [Y/N D:Y]:
    >;
    >INS [3,54]MAC/TASK=MACT0
    >INS [3,54]PIP/TASK=PIPT0
    >INS [3,54]LBR/TASK=LBRT0
    >INS [3,54]TKB/TASK=TKBT0
    >INS [3,54]VMR/TASK=VMRT0
    >;
    >;
    >;
    >;======================================================
    >;  Choosing Executive Options      27-NOV-16 at 22:01
    >;======================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >; Enter a comment for inclusion in the SYSGENSA1 saved answer file.
    >; The comment may contain more than one line.  The "V" in the right
    >; margin below marks the maximum line length.  When you are done,
    >; press RETURN in response to the prompt.
    >;                                                                             V
    >* Comment [S R:0.-55.]:
    >;
    >* CE010   What is your target processor type? [S R:3.-12. D:"LSI-11/73"]: 11/23-PLUS
    >;
    >* CE020   Do you want the Full-functionality Executive? [Y/N D:Y]:
    >;
    >* CE120   Do you want support for communications products
    >*         (such as DECnet, PSI, and LAT)? [Y/N D:N]: Y
    >;
    >* CE130   What is the system name? [S R:0-6 D:"RSXMPL"]: KYPEBO
    >;
    >* CE215   Do you want the default date format to be
    >*         ISO 8601:1988 compliant? [Y/N D:N]:
    >;
    >* CE216   Do you want the default date format to include
    >*         a four digit year? [Y/N D:N]:
    >;
    >* CE264   Do you want IP11 industrial I/O subsystem support? [Y/N D:N]:
    >;
    >* CE270   Do you want to include XDT? [Y/N D:N]: Y
    >;
    >* CE280   Enter the crash notification device CSR
    >*         address [O R:160000-177700 D:177564]:
    >;
    >; Note:  Enter both the device and the logical unit number.
    >;        For example, MM0: or DL1:.
    >;
    >; Note:  Enter XX: if you desire loadable DU:, DL:, MU:, MS: or MM:
    >;        crash driver support.
    >;
    >* CE290   On what device and unit do you want crash dumps
    >*         to be written? [S R:2-6]: XX:
    >;
    >* CE300   Enter the initial number of virtual disks to be
    >*         included [D R:0.-16. D:2.]:
    >;
    >* CE310   Enter memory size (in K words) [D R:256.-2044. D:256.]:
    >;
    >* CE315   Support UNIBUS memory occupying UNIBUS map address space? [Y/N D:N]:
    >;
    >* CE320   Do you want floating point processor support? [Y/N D:N]:
    >;
    >* CE330   Is your system clock programmable (KW11-P)? [Y/N D:N]:
    >;
    >* CE350   Is your line frequency 50 Hz? [Y/N D:N]: Y
    >;
    >;
    >;
    >;=============================================================
    >;  Choosing Peripheral Configuration      27-NOV-16 at 22:02
    >;=============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA2.CMD.
    >;
    >; Enter a comment for inclusion in the SYSGENSA2 saved answer file.
    >; The comment may contain more than one line.  The "V" in the right
    >; margin below marks the maximum line length.  When you are done,
    >; press RETURN in response to the prompt.
    >;                                                                             V
    >* Comment [S R:0.-55.]:
    >;
    >;
    >* CP0604  How many RH controllers do you have? [D R:0.-15. D:0.]:
    >;
    >;
    >;   DK:    controller:  RK11           devices: RK05, RK05F
    >;
    >* CP2204  How many RK11 cartridge disk controllers do you have? [O D:1]: 0
    >;
    >;
    >;   DM:    controllers: RK611, RK711   devices: RK06, RK07
    >;
    >* CP2404  How many RK611/711 disk cartridge controllers do
    >*         you have? [O D:0]:
    >;
    >;
    >;   DL:    controllers: RL11, RLV12    devices: RL01, RL02
    >;
    >* CP2604  How many RL11/RLV11 disk cartridge controllers do
    >*         you have? [O D:0]:
    >;
    >;
    >;   DP:    controller:  RP11           devices: RP02, RPR02, RP03
    >;
    >* CP2804  How many RP11 disk pack controllers do you have? [O D:0]:
    >;
    >;   DU:    controllers: RQZX1, RQDX1, RQDX2, RQDX3,
    >;                       RUX50, RQC25, KDA50, UDA50
    >;
    >;          devices:     RX33, RX50, RD31, RD51, RD52, RD53, RD54,
    >;                       RC25, RA60, RA70, RA71, RA72, RA80, RA81,
    >;                       RA82, RA90, RA92, RZ23L, RZ24L, RZ26x, RZ29B
    >;
    >;   The total of DU and MU controllers cannot be greater than 10.
    >;
    >* CP3004  How many MSCP disk controllers do you have? [D R:0.-10. D:0.]:
    >;
    >;
    >;   MU:    controllers: TK50, TU81, TU81E, TQ81E, RQZX1
    >;
    >* CP3404  How many TMSCP tape controllers do you have? [D R:0.-10. D:0.]:
    >;
    >;   VF:    Virtual disk/tape driver
    >;
    >;
    >;
    >;   CR:    controllers: CM11, CR11
    >;
    >* CP4004  How many CM/CR11 card readers do you have? [O D:0]:
    >;
    >;
    >;   CT:    controller:  TA11           device:  TU60
    >;
    >* CP4204  How many TA11 dual cassettes do you have? [O D:0]:
    >;
    >;
    >;   MS:    controllers: TS11, TU80, TSV05, TK25
    >;
    >* CP4404  How many TS11/TU80/TSV05/TK25
    >*         magtape controllers do you have? [O D:0]:
    >;
    >;
    >;   DT:    controller:  TC11           device:  TU56
    >;
    >* CP4604  How many TC11 DECtape controllers do you have? [O D:0]:
    >;
    >;
    >;   DX:    controller:  RX11           device:  RX01
    >;
    >* CP4804  How many RX11 disk controllers do you have? [O D:1]:
    >;
    >* CP4868  Enter vector address of the next RX11 [O R:60-774 D:264]:
    >;
    >* CP4872  What is its CSR address? [O R:160000-177700 D:177170]:
    >;
    >* CP4876  How many drives does DXA have? [D R:1.-2. D:2.]:
    >;
    >;
    >;   DY:    controller:  RX211, RXV21   device:  RX02
    >;
    >* CP5004  How many RX211/RXV21 disk controllers do you have? [O D:0]:
    >;
    >;
    >;   DD:    controller:  DL11           device:  TU58
    >;
    >* CP5204  How many TU58 controllers do you have? [O D:0]:
    >;
    >;
    >;   LP:    controllers: LA180, LN01, LP11, LS11, LV11
    >;          devices:     LA180, LG01, LG02, LN01, LP01, LP02, LP04, LP05,
    >;                       LP06,  LP07, LP14, LP25, LP26, LP27, LS11, LV01
    >;
    >* CP5404  How many LP/LS/LV/LG/LN/LA180 line printers do you have? [O D:1]:
    >;
    >* CP5408  Enter the number of seconds between
    >*         line printer-not-ready messages [D R:0.-255. D:15.]: 60
    >;
    >* CP5468  Enter vector address of the next line
    >*         printer [O R:60-774 D:200]:
    >;
    >* CP5472  What is its CSR address? [O R:160000-177700 D:177514]:
    >;
    >* CP5480  Enter line printer type for LPA [S R:4-5 D:"LP25"]:
    >;
    >* CP5484  Does LPA have lowercase characters? [Y/N D:N]:
    >;
    >;
    >;   MT:    controllers: TM11, TMA11, TMB11   devices: TE10, TU10, TU10W, TS03
    >;
    >* CP5604  How many TM/TMA/TMB11 magtape controllers do you have? [O D:1]: 0
    >;
    >;
    >;   PP:    controller:  PC11
    >;
    >* CP5804  How many PC11 paper tape reader/punches do you have? [O D:1]:
    >;
    >* CP5868  Enter vector address of the next PC11 [O R:60-774 D:74]: 70
    >;
    >* CP5872  What is its CSR address? [O R:160000-177700 D:177554]: 177550
    >;
    >;
    >;   PR:    controller:  PR11
    >;
    >; Exclude the number of PC11s from your answer to this question.
    >;
    >* CP6004  How many PR11 paper tape readers do you have? [O D:1]: 0
    >;
    >;
    >;   LA:    controller:  LPA11
    >;
    >* CP6204  How many LPA11 lab subsystems do you have? [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:    controllers: DL11, DLV11    controller mnemonic: YL
    >;
    >* CP6804  Enter number of additional DL11/DLV11 line interfaces [O D:0]: 1
    >;
    >* CP6820  Do any of the DL11/DLV11 lines require modem support? [Y/N D:N]:
    >;
    >* CP6832  Enter terminal type for YLA [S R:4-6 D:"LA120"]: VT52
    >;
    >* CP6868  Enter vector address of YLB [O R:300-770]: 360
    >;
    >* CP6872  What is its CSR address? [O R:160000-177700]: 176560
    >;
    >* CP6832  Enter terminal type for YLB [S R:4-6 D:"LA120"]: VT52
    >;
    >;
    >;   TT:    controller:  DH11           controller mnemonic: YH
    >;
    >* CP7004  Enter number of DH11 asynchronous line
    >*         multiplexers [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:                                   controller mnemonic: YV
    >;
    >;      controllers: DHU11, DHV11, CXA16, CXB16, CXY08
    >;
    >;
    >* CP7104  Enter number of DHU11/DHV11/CXA16/CXB16/CXY08 (YV:-type)
    >*         asynchronous line multiplexers [D R:0.-32. D:0.]:
    >;
    >;
    >;   TT:    controller:  DJ11           controller mnemonic: YJ
    >;
    >* CP7204  Enter number of DJ11 asynchronous line
    >*         multiplexers [D R:0.-16. D:0.]:
    >;
    >;
    >;   TT:    controllers: DZ11, DZQ11, DZV11, DFA01    controller mnemonic: YZ
    >;
    >* CP7404  Enter number of DZ11/DZQ11/DZV11/DFA01 asynchronous line
    >*         multiplexers [D R:0.-32. D:0.]:
    >;
    >;
    >* CP7604  Do you have any intercomputer communication devices? [Y/N D:N]:
    >;
    >;
    >; Enter device mnemonics for any user-supplied drivers.  The driver
    >; source files must reside in [11,10] and be named ddDRV.MAC and
    >; ddTAB.MAC where dd is the device mnemonic.
    >;
    >; You may enter the mnemonics on more than one line.  When you have
    >; listed all the drivers, press RETURN when asked for the device
    >; mnemonic.
    >;
    >; The device mnemonic must not include a colon.
    >;
    >* CP9604  Enter device mnemonics for user-supplied drivers [S]:
    >;
    >;
    >; The highest vector among the devices you specified in this SYSGEN
    >; is 374(octal).  This is the default response for this question.
    >;
    >* CP9632  What is the highest interrupt vector
    >*         address? [O R:374-774 D:374]: 474
    >;
    >;
    >;
    >;================================================================
    >;  Assembling the Executive and Drivers      27-NOV-16 at 22:03
    >;================================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >PIP RSXMC3.MAC=RSXMC1.MAC,RSXMC2.MAC
    >PIP RSXMC.MAC=RSXMC3.MAC,RSXMC0.MAC
    >;
    >SET /UIC=[1,24]
    >PIP [11,10]/NV=[200,200]RSXMC.MAC
    >PIP [11,10]/NV=[200,200]SYSTB.MAC
    >PIP [11,24]/NV=[200,200]RSXASM.CMD
    >PIP [11,24]/NV=[200,200]DRIVERS.ASM
    >;
    >;
    >* AE010   Do you want assembly listings of the Executive and
    >*         drivers? [Y/N D:N]:
    >;
    >ASN NL:=LS:
    >;
    >;
    >* AE030   Do you wish to pause to edit any files before
    >*         assembling? [Y/N D:N]:
    >;
    >SET /UIC=[11,24]
    >;
    >PIP *.OBJ;*/DE/NM,*.TTY;*
    >;
    >TIME
    22:03:19 27-NOV-16
    >;
    >MAC @RSXASM
    >;
    >TIME
    22:05:11 27-NOV-16
    >;
    >MAC @DRIVERS.ASM
    >;
    >TIME
    22:06:14 27-NOV-16
    >;
    >PIP RSX11M.OBS=*.OBJ
    >PIP TTDRV.OBS=*.TTY
    >;
    >SET /UIC=[200,200]
    >PIP /NV=[11,10]RSXMC.MAC
    >;
    >SET /UIC=[1,24]
    >PIP RSXBLD.CMD/PU/NM
    >PIP RSX11M.OLB;*/DE/NM
    >PIP [200,200]RSXMC.MAC/PU/NM
    >;
    >LBR RSX11M/CR:256.::256./-EP=[11,24]RSX11M.OBS
    >PIP [11,24]RSX11M.OBS;*,*.OBJ;*/DE
    >;
    >LBR TTDRV/CR:40.:392.:128.=[11,24]TTDRV.OBS
    >PIP [11,24]TTDRV.OBS;*,*.TTY;*/DE
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;==============================================================
    >;  Building the Executive and Drivers      27-NOV-16 at 22:06
    >;==============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >;
    >; Allocate space to be used later for the system image file.
    >;
    >SET /UIC=[1,54]
    >PIP RSX11M.TMP/CO/BL:1026.=NL:
    >;
    >SET /UIC=[200,200]
    >;
    >SET /UIC=[1,24]
    >SET /UIC=[200,200]
    >SET /UIC=[1,54]
    >PIP SYSVMR.CMD=[200,200]SYSVMR.CMD,VMRTTY.CMD
    >;
    >SET /UIC=[200,200]
    >;
    >* BE030   Do you want to pause to edit any files before
    >*         task-building? [Y/N D:N]:
    >;
    >SET /UIC=[1,24]
    >PIP [1,24]/NV/NM=[200,200]RSXBLD.CMD,RSX11M,DSP11M,LDR11M
    >PIP [1,24]/NV=[200,200]DIR11M.CMD,DR211M,DIRCOM,DR2COM,DIR
    >PIP [1,24]/NV=[200,200]DR311M.CMD,DR411M,DR3COM,DR4COM
    >PIP [1,24]/NV=[200,200]VEC11M.CMD,DCM11M,VECCOM
    >;
    >TIME
    22:06:26 27-NOV-16
    >;
    >TKB @RSXBLD
    >;
    >TIME
    22:06:55 27-NOV-16
    >;
    >TKB @[200,200]DRIVERS.BLD
    >;
    >TIME
    22:06:59 27-NOV-16
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;=========================================================
    >;  Building the Privileged Task      27-NOV-16 at 22:06
    >;=========================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA1.CMD.
    >;
    >;
    >* BP040   Do you want the maps of the privileged tasks? [Y/N D:N]: Y
    >;
    >* BP050   What is to be the map device [ddu:]? [S R:2-5 D:"SY:"]:
    >;
    >ASN SY:=MP:
    >;
    >SET /UIC=[1,24]
    >;
    >TIME
    22:07:03 27-NOV-16
    >;
    >TKB @SAVBLD
    >;
    >TIME
    22:07:10 27-NOV-16
    >;
    >ASN LB:=OU:
    >SET /UIC=[200,200]
    >;
    >;
    >;
    >;============================================================
    >;  Rebuilding Supplied System Tasks      27-NOV-16 at 22:07
    >;============================================================
    >;
    >;
    >;
    >; The answers to the questions in this section are put in the saved
    >; answer file [200,200]SYSGENSA3.CMD.
    >;
    >;
    >* BN010   Do you want to rebuild any system tasks? [Y/N D:N]:
    >;
    >;
    >;
    >;==========================================================
    >;  Creating the System Image File      27-NOV-16 at 22:07
    >;==========================================================
    >;
    >;
    >SET /UIC=[1,54]
    >;
    >PIP RSX11M.TMP;*/DE/NM
    >;
    >PIP RSX11M.SYS/CO/NV/BL:1026.=RSX11M.TSK
    >;
    >ASN LB:=SY:
    >VMR @SYSVMR
    VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
    SET /TOP=SYSPAR:-*
    VMR -- *DIAG*-Loadable driver larger than 4K
    LOA TT:/SIZE=16300
    VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
    SET /TOP=DRVPAR:-*
    SECPOL 117734 00120000 00100000  SEC POOL
    SYSPAR 117670 00220000 00166100  MAIN
           117624 00220000 00112100  RO COM !DIR11M!
           117440 00332100 00004400  TASK   [...LDR]
           117240 00336500 00033500  TASK   [MCR...]
           117040 00372200 00010500  TASK   [TKTN  ]
           116640 00402700 00003200  TASK   [SHF...]
    DRVPAR 116560 00406100 00075700  MAIN
           116514 00406100 00006700  RO COM !TTEXT !
           116430 00415000 00036000  DRIVER (TT:)
           116060 00453000 00001700  DRIVER (DX:)
           115620 00454700 00001300  DRIVER (LP:)
           115360 00456200 00000500  DRIVER (PP:)
           115120 00456700 00000400  DRIVER (PR:)
           114710 00457300 00000100  DRIVER (NL:)
           114644 00457400 00017700  DRIVER (VF:)
           114600 00477300 00000300  DRIVER (CO:)
           114534 00477600 00002500  DRIVER (VT:)
           114470 00502300 00001500  DRIVER (RD:)
    GEN    114424 00504000 01274000  MAIN
    ...LDR 12.01  117504  SYSPAR 248. 00004400 LB0:-00166112 FIXED
    TKTN   07.01  117104  SYSPAR 248. 00010500 LB0:-00065277 FIXED
    F11MSG 15.00  112414  GEN    200. 00006300 LB0:-00053566
    MTAACP 17.00  112034  GEN    200. 00016200 LB0:-00060246
    SHE... 06.01  111574  GEN    200. 00014500 LB0:-00063715
    MCR... 07.00  117304  SYSPAR 160. 00033500 LB0:-00057225 FIXED
    F11ACP 07.00  114214  GEN    149. 00011100 LB0:-00052236
    ERRLOG 05.03  113664  GEN    148. 00056200 LB0:-00052154
    PMT... 02.02  113234  GEN    148. 00007500 LB0:-00061156
    COT... 02.04  112534  GEN    145. 00014300 LB0:-00046412
    HRC... 05.00  112154  GEN    140. 00042500 LB0:-00054352
    PMD... 07.05  111714  GEN    140. 00017600 LB0:-00061126
    SYSLOG 04.03  112774  GEN    130. 00024500 LB0:-00064155
    SHF... 07.01  116704  SYSPAR 105. 00003200 LB0:-00063734 FIXED
    FXR... 03.02  112274  GEN    100. 00003300 LB0:-00053560
    BAP0   04.11  114004  GEN     80. 00050300 LB0:-00044071
    QMG... 06.04  113114  GEN     75. 00037300 LB0:-00061560
    LP0    07.04  113450  GEN     70. 00020300 LB0:-00056543
    ACNT   06.04  112654  GEN     50. 00057600 LB0:-00043534
    SHUTUP 04.04  111454  GEN     50. 00016500 LB0:-00063741
    ...RMD 05.00  001236+ GEN    225. 00042000 LB0:-00061643
    ...DCL 06.01  001212+ GEN    160. 00062500 LB0:-00046716
    ...DMO 04.02  001214+ GEN    160. 00017300 LB0:-00047671
    ...MCR 07.00  001230+ GEN    160. 00040300 LB0:-00057263
    ...MOU 26.06  001232+ GEN    160. 00045600 LB0:-00060155
    ...CA. 01.00  001266+ GEN    150. 00026100 LB0:-00064204
    ...INS 16.00  001226+ GEN    100. 00053200 LB0:-00055237
    ...SAV 11.00  001262+ GEN    100. 00071000 LB0:-00171627
    ...UFD 07.02  001270+ GEN    100. 00014500 LB0:-00065312
    ...VCP V04.10 001272+ GEN     90. 00020300 LB0:-00065500
    ...ACS 04.00  001244+ GEN     70. 00006200 LB0:-00043712
    ...ACC 05.00  001204+ GEN     65. 00032100 LB0:-00043220
    ...SHA 06.01  001264+ GEN     65. 00032000 LB0:-00063542
    ...AT. 10.0   001220+ GEN     64. 00056700 LB0:-00054772
    ...INI 24.00  001222+ GEN     60. 00037200 LB0:-00055143
    ...HOM 24.00  001224+ GEN     60. 00037200 LB0:-00055143
    ...BRO 09.10  001206+ GEN     50. 00041500 LB0:-00044217
    ...BYE 05.01  001210+ GEN     50. 00021700 LB0:-00044523
    ...HEL 06.00  001216+ GEN     50. 00031600 LB0:-00053716
    ...PIP 21.00  001234+ GEN     50. 00036400 LB0:-00060746
    ...UNL 05.04  001240+ GEN     50. 00021500 LB0:-00065426
    ...ACD 03.00  001242+ GEN     50. 00042500 LB0:-00043311
    ...BOO 03.10  001246+ GEN     50. 00047400 LB0:-00044017
    ...CON 05.00  001250+ GEN     50. 00135600 LB0:-00046210
    ...ELI 04.03  001252+ GEN     50. 00032600 LB0:-00052117
    ...LOA 05.03  001254+ GEN     50. 00040000 LB0:-00056346
    ...MAG 03.00  001256+ GEN     50. 00037300 LB0:-00057163
    ...PSW 03.02  001260+ GEN     50. 00017500 LB0:-00061243
    YLA     OFL     CPA     CSR=177560      VEC=60  PRI=5
    YLB     OFL     CPA     CSR=176560      VEC=360 PRI=5
    DXA     OFL     CPA     CSR=177170      VEC=264 PRI=5
    LPA     OFL     CPA     CSR=177514      VEC=200 PRI=4
    PPA     OFL     CPA     CSR=177554      VEC=74  PRI=4
    PRA     OFL     CPA     CSR=177550      VEC=70  PRI=4
    VF0:                    OFL     DRIVER
    VF1:                    OFL     DRIVER
    CO0:                    OFL     DRIVER
    TT0:    YLA0:           OFL     DRIVER
    TT1:    YLB0:           OFL     DRIVER
    VT0:                    OFL     DRIVER
    RD0:                    ONL     DRIVER
    DX0:    DXA0:           OFL     DRIVER
    DX1:    DXA1:           OFL     DRIVER
    LP0:    LPA0:           OFL     DRIVER
    PP0:    PPA0:           OFL     DRIVER
    PR0:    PRA0:           OFL     DRIVER
    NL0:                    OFL     DRIVER
    POOL=1200:3428.:03428.:1200
    >SET /UIC=[200,200]
    >;
    >REM MACT0
    >REM PIPT0
    >REM LBRT0
    >REM TKBT0
    >REM VMRT0
    >;
    >; End of SYSGEN
    >;
    >TIME
    22:07:27 27-NOV-16
    >;
    >ASN =
    >;
    >@ <EOF>
    >INS $EDT
    >CHD 1 54
    >EDT SYSVMR.CMD
        1       RSX11M.SYS
    *F "LOA DX:"
    *I
                LOA HD:/VEC
                ^Z
       84       LOA DX:/VEC
    *EX
    HD7:[1,54]A.CMD;2 239 lines
    >PIP RSX11M.SYS/NV/BL:1026.=RSX11M.TSK
    >INS $VMR
    >VMR @SYSVMR
    VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
    SET /TOP=SYSPAR:-*
    VMR -- *DIAG*-Loadable driver larger than 4K
    LOA TT:/SIZE=16300
    VMR -- *DIAG*-Installed tasks or commons may no longer fit in partition
    SET /TOP=DRVPAR:-*
    SECPOL 117734 00120000 00100000  SEC POOL
    SYSPAR 117670 00220000 00166100  MAIN
           117624 00220000 00112100  RO COM !DIR11M!
           117440 00332100 00004400  TASK   [...LDR]
           117240 00336500 00033500  TASK   [MCR...]
           117040 00372200 00010500  TASK   [TKTN  ]
           116640 00402700 00003200  TASK   [SHF...]
    DRVPAR 116560 00406100 00076400  MAIN
           116514 00406100 00006700  RO COM !TTEXT !
           116430 00415000 00036000  DRIVER (TT:)
           116060 00453000 00001700  DRIVER (DX:)
           115210 00454700 00000500  DRIVER (HD:)
           114770 00455400 00001300  DRIVER (LP:)
           114530 00456700 00000500  DRIVER (PP:)
           114270 00457400 00000400  DRIVER (PR:)
           114060 00460000 00000100  DRIVER (NL:)
           114014 00460100 00017700  DRIVER (VF:)
           113750 00500000 00000300  DRIVER (CO:)
           113704 00500300 00002500  DRIVER (VT:)
           113640 00503000 00001500  DRIVER (RD:)
    GEN    113574 00504500 01273300  MAIN
    ...LDR 12.01  117504  SYSPAR 248. 00004400 LB0:-00166112 FIXED
    TKTN   07.01  117104  SYSPAR 248. 00010500 LB0:-00065277 FIXED
    F11MSG 15.00  111564  GEN    200. 00006300 LB0:-00053566
    MTAACP 17.00  111204  GEN    200. 00016200 LB0:-00060246
    SHE... 06.01  110744  GEN    200. 00014500 LB0:-00063715
    MCR... 07.00  117304  SYSPAR 160. 00033500 LB0:-00057225 FIXED
    F11ACP 07.00  113364  GEN    149. 00011100 LB0:-00052236
    ERRLOG 05.03  113034  GEN    148. 00056200 LB0:-00052154
    PMT... 02.02  112404  GEN    148. 00007500 LB0:-00061156
    COT... 02.04  111704  GEN    145. 00014300 LB0:-00046412
    HRC... 05.00  111324  GEN    140. 00042500 LB0:-00054352
    PMD... 07.05  111064  GEN    140. 00017600 LB0:-00061126
    SYSLOG 04.03  112144  GEN    130. 00024500 LB0:-00064155
    SHF... 07.01  116704  SYSPAR 105. 00003200 LB0:-00063734 FIXED
    FXR... 03.02  111444  GEN    100. 00003300 LB0:-00053560
    BAP0   04.11  113154  GEN     80. 00050300 LB0:-00044071
    QMG... 06.04  112264  GEN     75. 00037300 LB0:-00061560
    LP0    07.04  112620  GEN     70. 00020300 LB0:-00056543
    ACNT   06.04  112024  GEN     50. 00057600 LB0:-00043534
    SHUTUP 04.04  110624  GEN     50. 00016500 LB0:-00063741
    ...RMD 05.00  001236+ GEN    225. 00042000 LB0:-00061643
    ...DCL 06.01  001212+ GEN    160. 00062500 LB0:-00046716
    ...DMO 04.02  001214+ GEN    160. 00017300 LB0:-00047671
    ...MCR 07.00  001230+ GEN    160. 00040300 LB0:-00057263
    ...MOU 26.06  001232+ GEN    160. 00045600 LB0:-00060155
    ...CA. 01.00  001266+ GEN    150. 00026100 LB0:-00064204
    ...INS 16.00  001226+ GEN    100. 00053200 LB0:-00055237
    ...SAV 11.00  001262+ GEN    100. 00071000 LB0:-00171627
    ...UFD 07.02  001270+ GEN    100. 00014500 LB0:-00065312
    ...VCP V04.10 001272+ GEN     90. 00020300 LB0:-00065500
    ...ACS 04.00  001244+ GEN     70. 00006200 LB0:-00043712
    ...ACC 05.00  001204+ GEN     65. 00032100 LB0:-00043220
    ...SHA 06.01  001264+ GEN     65. 00032000 LB0:-00063542
    ...AT. 10.0   001220+ GEN     64. 00056700 LB0:-00054772
    ...INI 24.00  001222+ GEN     60. 00037200 LB0:-00055143
    ...HOM 24.00  001224+ GEN     60. 00037200 LB0:-00055143
    ...BRO 09.10  001206+ GEN     50. 00041500 LB0:-00044217
    ...BYE 05.01  001210+ GEN     50. 00021700 LB0:-00044523
    ...HEL 06.00  001216+ GEN     50. 00031600 LB0:-00053716
    ...PIP 21.00  001234+ GEN     50. 00036400 LB0:-00060746
    ...UNL 05.04  001240+ GEN     50. 00021500 LB0:-00065426
    ...ACD 03.00  001242+ GEN     50. 00042500 LB0:-00043311
    ...BOO 03.10  001246+ GEN     50. 00047400 LB0:-00044017
    ...CON 05.00  001250+ GEN     50. 00135600 LB0:-00046210
    ...ELI 04.03  001252+ GEN     50. 00032600 LB0:-00052117
    ...LOA 05.03  001254+ GEN     50. 00040000 LB0:-00056346
    ...MAG 03.00  001256+ GEN     50. 00037300 LB0:-00057163
    ...PSW 03.02  001260+ GEN     50. 00017500 LB0:-00061243
    YLA     OFL     CPA     CSR=177560      VEC=60  PRI=5
    YLB     OFL     CPA     CSR=176560      VEC=360 PRI=5
    DXA     OFL     CPA     CSR=177170      VEC=264 PRI=5
    HDA     OFL     CPA     CSR=177720      VEC=0   PRI=0
    LPA     OFL     CPA     CSR=177514      VEC=200 PRI=4
    PPA     OFL     CPA     CSR=177554      VEC=74  PRI=4
    PRA     OFL     CPA     CSR=177550      VEC=70  PRI=4
    VF0:                    OFL     DRIVER
    VF1:                    OFL     DRIVER
    CO0:                    OFL     DRIVER
    TT0:    YLA0:           OFL     DRIVER
    TT1:    YLB0:           OFL     DRIVER
    VT0:                    OFL     DRIVER
    RD0:                    ONL     DRIVER
    DX0:    DXA0:           OFL     DRIVER
    DX1:    DXA1:           OFL     DRIVER
    HD0:    HDA0:           OFL     DRIVER
    HD1:    HDA1:           OFL     DRIVER
    HD2:    HDA2:           OFL     DRIVER
    HD3:    HDA3:           OFL     DRIVER
    HD4:    HDA4:           OFL     DRIVER
    HD5:    HDA5:           OFL     DRIVER
    HD6:    HDA6:           OFL     DRIVER
    HD7:    HDA7:           OFL     DRIVER
    LP0:    LPA0:           OFL     DRIVER
    PP0:    PPA0:           OFL     DRIVER
    PR0:    PRA0:           OFL     DRIVER
    NL0:                    OFL     DRIVER
    POOL=1200:3224.:03224.:1200
    >BOO [1,54]
    XDT: 87

    XDT>G
      RSX-11M-PLUS V4.6   BL87

    >

    >TIM 22:10 27-NOV-2016
    >SAV /WB

    RSX-11M-PLUS V4.6  BL87   512.KW  System:"KYPEBO"
    >RED HD7:=SY:
    >RED HD7:=LB:
    >RED HD7:=SP:
    >MOU HD7:"RSX11MPBL87"
    >@HD7:[1,2]STARTUP
    >;                      PLEASE NOTE
    >;
    >;      If you have not yet read the system release notes, please do so
    >;      now before attempting to perform a SYSGEN or to utilize the new
    >;      features of this system.
    >;
    >;
    >* Please enter time and date (HH:MM DD-MMM-YYYY) [S]: