                   RSX/IAS SIG Tape Distribution - Spring 1985
                   ===========================================


          This is the RSX/IAS SIG Symposium Tape from the Spring 1985 DECUS
     Symposium at New Orleans.  The tape contains material submitted by the
     user community for the tape at that meeting.  

          The  programs  on this tape are from user submissions.  The DECUS
     staff, the RSX & IAS SIG staffs, and DEC are all in complete ignorance
     of  the  contents of the tapes.  No warranty of any kind is implied in
     the distribution of these tapes.  The programs may or may not be  well
     documented, they may or may not work, they may even crash your system.
     If you have a problem with the  contents  of  the  tape,  contact  the
     author  of  the program.  Do not contact DECUS, DEC, or the RSX or IAS
     SIG's.  

          The  tape  contains  about  1970 files requiring 57,000 blocks of
     disk space.  Since this will fit on a single 2400 foot  tape  only  in
     BRU  at  1600  bpi,  it  is  being  distributed  as such.  To simplify
     distribution and production, the tape is a single BRU  container  file
     followed (for the LUG distribution only) by several extra files.  

          Directory  [300,1] contains the files documenting the contents of
     the tape.  The following files are present:  
     RSX85ATPE.DOC contains an abstract of the contents of the tape by UIC. 
     85AREADME.ALL  contains a concatenated list of all the README files on
        the tape.  
     RSX85ADIR.LIS  contains  a directory of all the files on the tape (BRU
        does not produce nice directories).  This is a brief  listing  with
        UICs and filenames only for space reasons.  
     SUBMIT.DOC contains guidelines for submissions to the RSX/IAS Sig Tape
        collection.  This is MUST  reading  for  everyone  who  desires  to
        submit a program to the SIG tape.  
     BEGIN85A.DOC has a copy of this text.  
     UICSET85A.CMD contains the UFD commands to create all the needed UIC's
        on a device whose name is asked for in the command file.   Edit  it
        to  match your needs before using BRU to extract the tape contents.
        A word of caution:  under at least  some  circumstances,  11M  V4.0
        BRU's  /UFD  switch  creates  directories  even when it doesn't put
        anything in them.  

     If  your  disk  is smaller than an RM03, you will want to exclude some
        files from the copy in order to have a backup set that  fits  on  a
        smaller  disk.   Copy  these off in separate passes.  The directory
        [300,3]  contains  15005  blocks  and  has  the  sig  tape   index.
        Directory  [356,40]  contains  several Kermits and 7421 blocks.  If
        these are omitted, the tape will fit on an RK07.  



                                        Glenn C. Everhart
                                        RSX/IAS SIG Tape Copy Coordinator
                                        RCA A&D Engineering MS 206-1
                                        Rt. 38
                                        Cherry Hill, N.J. 08358
                                        (609)-338-6022
	RSX SIG SPRING 1985 README FILES


++++++++++++++++++++
[240,001]AAAREADME.TXT
+++++++++++++++++++++
This area has a few random things for 8086/8088 under
MSDOS including a FORTH, a FOCAL for Z80 and CP/M,
and some small C sources.


++++++++++++++++++++
[240,002]READ.ME
+++++++++++++++++++++
PC-VT is a VT100/VT102/VT52 emulator for IBM PC and lookalikes.
 - editor
	Enclosed is the latest version of PC-VT and a copy of the
documentation.  I formatted your diskette double sided, 8 sectors per track
(unless it was already formatted) so that either DOS 1.1 or DOS 2.x could
read it.  If you sent me a single sided diskette, I was not able to get all
of the files onto it.  PC-VT runs on the PC, the PCjr, and the PC AT under
DOS 1.1, 2.0, 2.1, and 3.0.

	This  version (7.6) of PC-VT contains both a Hayes compatible dialer
and XMODEM with CRC transfer capability.  It  supports  DOS  2  path  names.
PC-VT  now supports VT52 compatibility mode and ALT-F1 thru ALT-F10 as macro
keys.  

	The program itself is named PC-VT.EXE.  To run it just type PC-VT in
response  to  the DOS prompt.  The documentation file is named PC-VT.DOC and
can be copied to  any  line  printer.   It  does  not  contain  any  special
formatting commands, it is just straight text.  The file PC-VT.SUM is just a
short summary of the capabilities of PC-VT.

	If  any  files  on  your  distribution disk have a "Q" as the second
character of the extension, they must be Unsqueezed with the USQ program.

	The  file PC-VT.CRD is a quick reference card for use with PC-VT.  I
would like to thank Richard C.  Rohrdanz of the Boston Computer Society  for
his help in creating PC-VT.CRD.

	I've also enclosed a set of XMODEM programs for the VAX running VMS.
They  were  written  by  Jim  Belonis of the University of Washington.  They
work.  I'll leave it up to you to upload them to the VAX and  compile  them.
Read  the  file  named  XMODEM.DOC.  These files are combined into a library
file named XMODVMS.LBR.  You  will  need  the  Library  Utility  (LU.EXE  or
LAR.EXE)  to  remove  them  from  the library file.  If they have a Q as the
second letter of the filetype, they are SQueezed.   Use  USQ  to  make  them
ASCII files.

	If  you  could  upload  PC-VT  and the XMODEM programs to your local
RBBS, I would appreciate your help.  You can  upload  PC-VT.EXE,  PC-VT.SUM,
PC-VT.DOC, and the XMODEM files on XMODVMS.LBR.

	One  useful piece of information : The older versions of PC-VT would
not pass CTRL-C on to the host computer because the CTRL-C  was  intercepted
by PC-DOS as a program termination command.  I have modified this version to
have  PC-DOS  ignore  CTRL-C  when reading from the keyboard.  Now CTRL-C is
sent to the host.   To  terminate  PC-VT  you  can  type  CTRL-F8  from  the
communications  display or still use CTRL-C from the SETUP, DIALING or MACRO
displays.  You should have the PC-DOS option BREAK set to OFF or else  PC-VT
will turn it off.

	SCRLOCK,   the   Extended  Batch  Language,  and  BACKSCRL  are  not
compatible with PC-VT.  SCRLOCK will not work well with DOS 2.0 in any case.
A general comment about PC-DOS "appendages": since there is no  way  that  I
can  try  every  patch to PC-DOS with PC-VT, if you are having problems, try
PC-VT with an unpatched DOS to see what happens.  The issue is how long some
of the attached programs run with interrupts turned off.  The comm  line  to
the  host  is  asynchronous.   If  PC-VT  cannot get back to the RS-232 port
before another character comes in, the old character is lost and an  overrun
error  is  generated.   This  type of problem is more apparent at the higher
baud rates but will also show up at 1200 baud.

	I  hope  that  the program is of use to you.  I would appreciate any
comments which you might have regarding the program or its usefulness.  When
you write, please indicate the version number of PC-VT which you are using.

Sincerely,
Mark C. DiVecchio
9067 Hillery Drive
San Diego, CA 92126
619-566-6810


++++++++++++++++++++
[240,003]README.1ST
+++++++++++++++++++++
	This area contains a MSDOS version of DTC for MS fortran-77
V3.13 or later.


++++++++++++++++++++
[300,340]README.TXT
+++++++++++++++++++++
**********************************************************************
This UIC contains XLISP, an object oriented LISP dialect with
extensions. It was written in DECUS C and has been ported to several
systems.

++++++++++++++++++++
[303,100]README.TXT
+++++++++++++++++++++
**********************************************************************
 
THIS UIC([303,100]) CONTAINS XQDRV UTILITY TASKS SOURCE CODE AND THE 
NECESSARY COMMAND FILES TO BUILD THEM. IF THEY ARE MOVED TO ANOTHER
UIC A FEW COMMAND FILES WILL HAVE TO BE EDITED TO CORRECT EMBEDDED
UIC'S.
 
**********************************************************************
 
THIS UIC CONTAINS FILE ACCESS AND DOWN LINE LOAD ROUTINES AS FOLLOWS;
 
LWT	LINE WATCHER TASK(RSX11M)
	PROCESSES CONNECT REQUESTS
		REMOTE FILE ACCESS
		DOWN LINE LOAD REQUESTS
	FLUSHES STALE PACKETS
	GET LOCAL SYSTEM TIME
	SET LOCAL SYSTEM TIME
	ECHO PACKETS FOR TESTING
	SEND/ACCEPT ID PACKETS
	GET ERROR STATISTICS
	GET AND CLEAR ERROR STATISTICS
	GET LINE STATUS
 
NWT	NODE LINE WATCHER TASK(RSX11S)
	FLUSHES STALE PACKETS
	GET LOCAL SYSTEM TIME
	SET LOCAL SYSTEM TIME
	ECHO PACKETS FOR TESTING
	SEND/ACCEPT ID PACKETS
	GET ERROR STATISTICS
	GET AND CLEAR ERROR STATISTICS
	GET LINE STATUS
 
NFC	NETWORK FILE COPY
	ALLOWS OPERATOR INTERACTIVE FILE TRANSFERS
	REMOTE FILE DELETE(NOT IMPLEMENTED YET)
	REMOTE DIRECTORY(NOT IMPLEMENTED YET)
 
RFA	REMOTE FILE ACCESS
	READS/WRITES FILES(BLOCK MODE)
	READS/WRITES FILE(SEQUENTIAL MODE NOT CHECHED OUT YET)
	DELETE FILE(NOT CHECKED OUT YET)
	DIRECTORY(NOT CHECKED OUT YET)
 
DLT	DOWN LINE LOAD TASK
	LOADS SPECIFIED NODE REQUESTED BY THE REMOTE NODE
 
BOOTQNA	PRIMARY LOADER RESIDES IN EPROM IN NODES TO BE DOWN
	LINE LOADED
 
FALODT	ODT/PRIMARY LOADER RESIDES IN EPROM ON FALCON BOARD
	ALLOWS NORMAL ODT FUNCTIONS PLUS ETHERNET DOWN LINE
	LOAD CAPIBILITY.
 
BOOEDT	DOWN LINE LOADER DATA BASE EDITOR TASK
 
PARSX	COMMAND LINE PARSER USED BY NFC


++++++++++++++++++++
[304,001]README.1ST
+++++++++++++++++++++
    Richard Rhoderick,  Systems Engineering Branch
    USEPA Health Effects Research Laboratory
    			/Neurotoxicology Division
    Mail Drop 74B
    Research Triangle Park, NC   27711

    This account contains several utility command files/programs used to
     automate or make transparent normal operations and system maintenence.
     The programs are written primarily in FORTRAN-77.
     No guarantee is made regarding efficiency or suitability for particular
     applications.  Any sugestions or improvements are gladly welcomed at
     the above address.

    Contents of this directory:
	Single stream batch scheduler:
	  BATCH.CMD - assembly, build, help file
	  BATCH.FTN - command interpreter, user front end
	  BQM.CMD - assembly, build file
	  BQM.FTN - Batch Queue Manager
	  CHKLOG.MAC - check terminal logged on condition
	  SPAWNR.CMD - assembly, build file
	  SPAWNR.FTN - batch job executor
	  RUNBATCH.CMD - assembly, build file
	  RUNBATCH.FTN - disable batch jobs during working hours
	Disk maintenence and backup processes:
	  ASSIGN.CMD - set up user disks at boot
	  NIGHTLY.CMD - batch job incremental backup of all user disks
	  AUTOBCKUP.CMD - "
	  AUTOBCKUP.DAT - "
	  INITNB0.CMD -   "
	  BACKUPSYS.CMD - routine duplication of system packs
	  INITDATE.DAT -     "
	Printer processor (QMG) for XEROX 2700 laser printer
	  X2700.CMD - assembly, build file
	  X2700.FTN - Spooled printer processor
	  X2700FONT.CFG - font configuration definitions
	  RECATR.MAC - file attributes
	Catchall task for monitor commands (very simple skeleton program)
	  CATCHALL.CMD - assembly, build file
	  CATCHALL.FTN - monitor command reinterpreter/run uninstalled tasks
	RS/1 public procedures
	  RS1INIT.RPL - set up standard globals, call RS1IND
	  RS1IND.RPL - indirect RS/1 command execution


++++++++++++++++++++
[307,120]README.ALL
+++++++++++++++++++++

	READMEALL.1ST

		This collection was originally submitted in FLX format
		under uic's: [101,2]    [101,5]    [101,6]    [101,7]
		changed to:  [307,122]  [307,125]  [307,126]  [307,127]

		Any reference to the original uic's within the files
		has not been updated.		
						BAYLUG Libr.
						 1-MAR-1985 
*==============================================================================

Abstract:
_________


This submission includes several software packages for use with Applied
Information Systems PL/I.  The Text Collection Management package can be of
general use with a little adaptation for those familiar with DECUS C.  It
allows a program to invoke a KED-style keypad screen word processor that
operates on text in a given arbitrary window on the screen, leaving the
rest of the screen undisturbed.  This allows implementation of free-form
text areas within fixed-format forms managed by FMS.  The interface between
PL/I and DECUS C is of possible interest to system hackers since it allows
PL/I-callable C procedures to be put in a clustered library even though
they take arguments on the stack.  The PL/I FMS interface is implemented
using this mechanism.  For more on the contents of each account, refer to
the respective README files.


Authorization:
______________

Full permission and consent is hereby given to DECUS to reproduce,
distribute, and publish, in whole or in part, in any form and without
restriction, this software and any information relating thereto.  The
undersigned hereby warrants and represents that he has good and sufficient
right, interest, and title in and to this software and the related
information to grant such permission to DECUS.  This material is currently
in the public domain.


				Walter Epp,
				Information Services Department,
				Kaiser Foundation Health Plan
					  415-428-2518

				5825 Telegraph #51
				Oakland, CA 94609

*==============================================================================
 README.1ST [307,122]

TCM: Text Collection Management System

      In many computer applications there is the  need  to  enter  both
 fixed  length  information and variable length descriptive text.  This
 is especially true in medical applications where  certain  information
 can vary from a single phrase to several pages in length.  FMS-11 aids
 a program in the interactive entry and updating of  fixed  fields  but
 does  not  deal  well  with  long  text fields.  This software package
 provides an easy to use mechanism for acquiring free form textual data
 from a CRT that is concurrently being used by FMS.


      This package allows a program to reserve one or more  rectangular
 areas  on the screen for the entry and editing of variable length text
 fields.  Within these windows the user  is  given  full  text  editing
 capability in a manner that is compatible with the user FMS interface.
 The text collection managment system is being implemented in a  manner
 which  gives  flexibility to an RSX-11M based application with a small
 impact on the program's address space.

      This program runs as a separate task under RSX-11M or RSX-11M+. It
is written in DECUS C and callable from either AIS-PL/I (tested) or DECUS
C (untested).  See TCM.DOC for a full description and TCMNOTES.DOC for
the current state of this program.  The idea of this sub-routine package
is to allow any program to use full screen editing or "Windows".


    			Daniel T. Soldahl
    			Medical Methods Research
    			3151 Piedmont Avenue
    			Oakland, Ca.  94611

*==============================
 README.1ST [307,125]

This account contains a clusterable FMS interface for Applied Information
Systems PL/I, using native PL/I variable types (e.g., CHAR, CHAR VARYING).
Written in DECUS C, requires the C-to-PL/I interface included in the
PLIMMR set of utility routines supplied on this tape on a different account.

  	Walter Epp, 5825 Telegraph #51, Oakland CA 94609
*==============================
 README.1ST [307,126]

This account contains utility routines for Applied Information Systems PL/I,
going by the name PLIMMR, from our in-house library.
Includes a C-to-PL/I interface, allowing a PL/I program to call procedures
written in DECUS C, which can in turn call other C or PL/I procedures.
This interface solves the problem of passing arguments on the stack through
a cluster call, for the case of AIS PL/I calling C, in a completely transparent
manner: the object files of PL/I-callable C procedures can either be linked
into a user task or built into a resident library; such a library can be
simultaneously accessed by some users mapping directly as a resident library,
by others accessing it as the first library of a cluster, and by others still
as the middle library of a cluster. The I/O runtimes have also been reconciled,
so you can do I/O both from PL/I using its native I/O statements and from C
using its standard I/O library calls.

  	Walter Epp, 5825 Telegraph #51, Oakland CA 94609
*==============================
 README.1ST [307,127]

This account contains a debugger for Applied Information Systems PL/I.
IT IS SUPPLIED ON A STRICTLY AS-IS BASIS.

  	Walter Epp, 5825 Telegraph #51, Oakland CA 94609


++++++++++++++++++++
[307,122]README.1ST
+++++++++++++++++++++
TCM: Text Collection Management System

      In many computer applications there is the  need  to  enter  both
 fixed  length  information and variable length descriptive text.  This
 is especially true in medical applications where  certain  information
 can vary from a single phrase to several pages in length.  FMS-11 aids
 a program in the interactive entry and updating of  fixed  fields  but
 does  not  deal  well  with  long  text fields.  This software package
 provides an easy to use mechanism for acquiring free form textual data
 from a CRT that is concurrently being used by FMS.


      This package allows a program to reserve one or more  rectangular
 areas  on the screen for the entry and editing of variable length text
 fields.  Within these windows the user  is  given  full  text  editing
 capability in a manner that is compatible with the user FMS interface.
 The text collection managment system is being implemented in a  manner
 which  gives  flexibility to an RSX-11M based application with a small
 impact on the program's address space.

      This program runs as a separate task under RSX-11M or RSX-11M+. It
is written in DECUS C and callable from either AIS-PL/I (tested) or DECUS
C (untested).  See TCM.DOC for a full description and TCMNOTES.DOC for
the current state of this program.  The idea of this sub-routine package
is to allow any program to use full screen editing or "Windows".


    			Daniel T. Soldahl
    			Medical Methods Research
    			3151 Piedmont Avenue
    			Oakland, Ca.  94611


++++++++++++++++++++
[307,125]README.1ST
+++++++++++++++++++++
This account contains a clusterable FMS interface for Applied Information
Systems PL/I, using native PL/I variable types (e.g., CHAR, CHAR VARYING).
Written in DECUS C, requires the C-to-PL/I interface included in the
PLIMMR set of utility routines supplied on this tape on a different account.

  	Walter Epp, 5825 Telegraph #51, Oakland CA 94609


++++++++++++++++++++
[307,126]README.1ST
+++++++++++++++++++++
This account contains utility routines for Applied Information Systems PL/I,
going by the name PLIMMR, from our in-house library.
Includes a C-to-PL/I interface, allowing a PL/I program to call procedures
written in DECUS C, which can in turn call other C or PL/I procedures.
This interface solves the problem of passing arguments on the stack through
a cluster call, for the case of AIS PL/I calling C, in a completely transparent
manner: the object files of PL/I-callable C procedures can either be linked
into a user task or built into a resident library; such a library can be
simultaneously accessed by some users mapping directly as a resident library,
by others accessing it as the first library of a cluster, and by others still
as the middle library of a cluster. The I/O runtimes have also been reconciled,
so you can do I/O both from PL/I using its native I/O statements and from C
using its standard I/O library calls.

  	Walter Epp, 5825 Telegraph #51, Oakland CA 94609  415-428-2518


++++++++++++++++++++
[307,127]README.1ST
+++++++++++++++++++++
This account contains a debugger for Applied Information Systems PL/I.
IT IS SUPPLIED ON A STRICTLY AS-IS BASIS.

  	Walter Epp, 5825 Telegraph #51, Oakland CA 94609


++++++++++++++++++++
[312,314]README.DOC
+++++++++++++++++++++

             This is the First page of B_BASE Instructions.

          This program is a small DATABASE program designed
        to store and retrieve information of a relative simple
        nature. Facilities to manage this information are MENU
        oriented and for the most part self-explanatory. There
        is ENTER DATA, UPDATE DATA (to change or modify), DELETE
        a RECORD (to delete a RECORD), SEARCH (to find a specific
        RECORD), PRINT a REPORT (to the default DIRECTORY or to
        the attached PRINTER), SCREEN REPORT (prints the REPORT
        to the SCREEN), LIST ALL DATA (displays all DATA in the
        file with RECORD and FIELD numbers), SORT (a general purpose
        SORT of the FILE by FIELD name), and EXIT (to quit).

        This program is designed to work on relatively small data
        the maximum number of RECORDS is 1000 with a maximum number of
        FIELDS being 20. This can be increased depending upon available
        disk/diskette storage space. The program was written with the
        begining user in mind, and performs the same on VAX VMS, PDP-11
        RSX-11M, or PRO-350 P/OS.



        The Program produces and works from two (2) files;

                filename.BBS -- A sequential file containing FILE information.
                    &
                filename.BBD -- A VIRTUTAL file containing the actual data.

        The  filename is a filename that you provide.

        The Program CAN also produce a sequential file REPORT;

                filename.DOC -- A REPORT file containing data in the
                                selected REPORT format.


                   If you have any further questions,
                            Please contact:

                              Randy Jordan
                             Black & Veatch
                      Computer Services Department
                            11401 Lamar Ave.
                      Overland Park, Kansas 66211
                             (913) 967-2544


++++++++++++++++++++
[312,315]AAAREADME.TXT
+++++++++++++++++++++
This area contains various utilities of general interest. Any
files of type .LZC have been compressed with LZCOMPRS which
is elsewhere on this tape. These are text files (and code
source) and may be reconstructed without the -B option of
LZDECOMP. The new DDT is of particular interest for RSX and
POS users, as it now can help find out how you got to a weird
place in your code after something has messed the stack up.
The new options should have been there years ago but better late
than never.
The BGL2*.* programs draw very pretty banners on your printer.
The BGL2.FTN is actually for VAX native mode; edit the TT: to
TI: to convert for RSX. It runs WELL on both systems (must be
compiled with /I4 and /NOF77 for both). The BGL2PC.FOR is an
8088 version for MSDOS using Microsoft Fortran (V3.2 or thereabouts)
to compile. We use the banners for birthday parties, or other random
celebrations. Most printable ASCII can be handled.
	gce
Also in this area is a program not by me called FIGEDT which allows
figure editing with text on an ordinary VT100. You can draw lines
or boxes, fill in text, center text, insert text files, and so
on. It works in VMS V3 or V4 and allows speedy creation or edit
of character graphics charts. The .OBJ file is supplied for those
who don't have VMS Pascal; just link/nomap figedt to get the .EXE.



++++++++++++++++++++
[312,315]README.TXT
+++++++++++++++++++++
G. Everhart submissions for Spring 1985

The following are offered for your amusement or use:

1. in [312,366], [312,370], several versions of DTC. These have been
somewhat debugged and new features added. In particular the [312,370]
is an entirely new revision with many enhancements by C. Garman
of RCA MSR. A few features were left out of his version however,
so it does not replace all existing ones. A new version for 8088
has been supplied also. This is a really nifty desktop calendar
that keeps getting nicer as more features are added. The new
version is also MUCH faster than the original one, though it
is designed for Vax only. The 8088 DTC is in [240,3].

2. In [312,315] are a few handy items from various places. These
include a revision of the DDT symbolic (Pdp11) debugger with some
features to permit back tracing where a program came from to
get to an error. It is quite useful on VAX or RSX as a symbolic
image examine/patch utility also. The ATT program (which reads
or alters file attributes in place) and the BIGTPC fast tape
to disk to tape copy utility are supplied. A version of DUMPER.C
(to read TOPS-20 DUMPER tapes on VMS) is supplied. Also the
LISTRS multicolumn lister, and CB.C, another BBS utility to
"beautify" C code.

3. In [312,371] is the latest PDP11, PRO 350, and VAX version
of AnalytiCalc with VAX support for DTR-32 (see DTRIF.DOC
for further info on how it works). DTR-32 is NOT required,
and a version can be built not using it if desired. Some
code speedups and other random novelties have been added
too, including ability to generate very wide output reports
(up to 512 characters, probably wider than YOUR printer).

4. In [312,345] is the lastes VAX spreadsheet that does not
use DTR (actually, on VMS you can pick the one here or the
one in [312,371]. The one here is a bit faster but uses more
memory. The one in [312,371] uses less memory but is a bit
slower. It can however access DTR-32. Try both and compare,
then choose. All documents are here, plus income tax templates,
a management system template for predicting manpower needs with
several jobs, and a Business Expense Report template (to help
you write up expenses for DECUS symposia and the like) with
all the numbers at your fingertips.

5. In [312,320] is a DBMS for RT11 with some necessary hooks to
convert to RSX (including VAX/RSX) or P/OS.

6. In [312,317] is a new squeeze/unsqueeze system that is far
superior to SQ/USQ, works on binary files (at least, on .EXE
files) as well as text, and compiles in DECUS C or VAX11 C
thanks to M. Minow. There are some sources for LAR (a utility
to read CP/M or MSDOS LU libraries or write them) and a
dialect of LOGO, both done for un*x originally and awaiting
conversion to RSX or VMS. LAR is actually pretty close as it
stands and will list directories of libraries now in VMS.


	G. Everhart
	May, 1985


++++++++++++++++++++
[312,317]AAAREADME.TXT
+++++++++++++++++++++
This area contains a few files downloaded from a BBS of interest
to VMS systems. LAR.C and docs are a utility to handle CP/M and
MSDOS LU-formatted "library" files. The program is not quite right
under VAX11C but is pretty close and is presented in case it is
needed badly enough for someone else to fix up first.
 LZ*.* is a super compressor-expander which will compile with either
VAX11C or DECUS C thanks to Martin Minow who deserves all the credit
for it. It generates noticeably smaller compressed files than does
SQ and, if run with the -B flag at runtime, will correctly handle
binary files. I have tested it one some .EXE images and on some
text files; original input was correctly regenerated in both cases.
This compression scheme is said to be compatible with the un*x
"compress" utility. It should be VERY handy for moving files
across networks, especially if they contain repetitive patterns.
The algorithm used Huffman codes strings, not bytes, so can
achieve much better results than byte-oriented methods, and with
considerable speed.
	The subdirectory .LOGO contains a UN*X based subset LOGO
in C. It's also presented in case someone wants to clean it up for
use on VMS in his/her copious spare time (while waiting for V4
compatible layered products that work to arrive?)


++++++++++++++++++++
[312,345]AAAREADME.TXT
+++++++++++++++++++++
	PortaCalc
This file is VAX build notes:
For VAX PortaCalc use the @compilvmx procedure in this
account. For RSX, use the [312,371] account and edit
pccpdpnew.com to make a suitable compile file. Then make
needed libraries and build with PCCNAT.CMD and PCCNAT.ODL.
Inspect PCCNAT.ODL to see what object files to make libraries
out of.
For PRO 350, use PCCPRO.COM or a mod to compile, then build with
PCCNAT.* again as in RSX (do it on the PRO). The PCCMAKI.COM
file in [312,371] is to build the VAX variant of that form of
PortaCalc.
	This version may need your VIRTUALPAGECNT sysgen parameter
to be increased (perhaps to 20000) to link. Do so if you need
to.
	ALWAYS BUILD FROM SOURCE IF POSSIBLE.
	For those with Fortran, the COMPILVMX.COM file builds
these files from source. You can edit the HVKLUGPR5.FTN file
first (compilvmx.com copies it to vklugprm.ftn for inclusion in the
compiles) to set your max sheet sizes if the ones supplied are too
small. The maxima possible then are large enough you are very
unlikely to need to go into sources to edit them.
Look over the READMEs before doing your build please!!!!!!!!!
	The file PortaCalc.rno can become a VAX help library
and be integrated with your system help if desired. The graphics
utility is described separately in PCG.DOC and there is a file
called KEYPAD.DOC in the distribution which describes various files
of PortaCalc commands which implement auxiliary keypad functions.
It should be edited to reflect any system default changes if
these features are to be generally used. Note that if CMDMUN.FOR
is compiled with the /debug qualifier, these files reside on device
DK:, which may be ASSIGN/USER'd to a particular system area prior
to running the local PortaCalc version.
	The PortaCalc.rno file must be passed through Runoff (possibly
DECUS runoff as opposed to DSR) to convert it to a VAX help file
format. It is designed to fit on 2 columns (using the LISTRS program
to reformat it, available in various places in the DECUS library
including 11-SP-6), but can fit on other sizes output with a little
editing. Column size of less than 60 characters may fail in some
places.
	I now have an 8088 version of this program. It sells
for $49.95/copy on IBM PC DSDD disks, and needs 256K RAM.
There's a  $5 s/h charge also, and NJ residents must add
6% sales tax. Order by writing Glenn Everhart, 409 High St.
Mt. Holly NJ 08060 and ask for General Engineering ANALYTICALC-88
giving your name, address, and enclosing payment. I can't handle
credit cards. Specify whether you need the 256K version or the
320K version. The latter is not overlaid and includes logical
naming for cells. The 256K version does not have the cell
naming. Non PCDOS machines may need more memory and if their
screen output calls are not via PCDOS like commands and/or
their ANSI cursor controls are broken, the program may be
unusable. However the techniques I used work on machines like
Tandy 2000 as well as IBM PC and Rainbow so I believe the non IBM
PC flavors will work most times.
		Glenn Everhart
		6/14/1983
Additional note: 8/18/83
	This version of PortaCalc has 2 VAX versions of interest. The
older one uses a random access workfile to hold formulas, and may be
used where the workfile provides insurance against crashes or other
faults. Since this is a burden on some sites with tight disk quotas,
a second version, here called PortaCalc-VM, is provided for VAX only.
It is built by running the COMPILVMX.COM procedure (possibly after edits
to HVKLUGPRM.FTN) and it uses a memory array to hold formulas. The
WRKFIL.F4 source of the routine that handles this array is pretty
crude and could easily be adapted to keep better track of which
array elements are in use, but it works reliably. In this version,
the S command allows resetting title and default format specification,
but does not modify the data. The ZA command clears data out of the
array (virtually; actually, it only zeroes the bitmap), and the
X and XD commands are identical. The VM version of PortaCalc does
not ask any questions about workfile names (since there are none).
	Since VMS will treat the big array as demand-zero pages,
it normally will hit only those you use, so a large sheet is
not a major liability. If it won't link on your system, you may need
to increase the VIRTUALPAGCNT (I think) parameter; the default
of 8192 is too small for some versions. Boost to 20,000 or so
while doing your links. We leave ours at 60,000.
	PDP11 users will find a PortaCalc that uses VERY
much smaller workfiles in the [312,371] area on RSX SIG tapes.
No total build file exists for RSX at my site (though a file to
build in compat mode on VMS is supplied, with working ODL), but
it should be pretty clear what to do from the compat mode file
that IS supplied. The current version supports a 10,000 cell
array on PDP11 with NO special bells & whistles like I/D space
or virtual arrays. If you can use virtual arrays or I/D space
you should be able to reduce the complexity of the overlay structure
and substantially speed the program up. Use PCCNAT.CMD and .ODL
for build in [312,371] and modify PCCPDP.COM to compile everything
for RSX. For POS use PCCPRON.COM as your compile guide; minor edits
are all you should need.


++++++++++++++++++++
[312,345]AAAREADME.V4
+++++++++++++++++++++
VMS V4.X Considerations

To run PortaCalc (AnalytiCalc) under VMS V4, you need to ensure the
terminal you're using is set to NOT have command line editing
during the run, so that arrow keys will go to the program rather
than being intercepted by the terminal driver. Just use the DCL
command to set terminal/noline to allow things to work correctly.
This is all the change that should be needed.


++++++++++++++++++++
[312,347]AAAREADME.TXT
+++++++++++++++++++++
This area contains CPMRSX which will allow one to read/write CP/M
format 8" floppies on RSX (or VMS). It also contains sources for a
CP/M emulator (needs an 8" disk cp/m system to use) from the DECUS
Australia 1982 tape. Given a CP/M system and these utilities you
may be able to build yourself a complete CP/M emulator and run
8080 software on a VAX. Anyone who wants to clean the emulator up
and make it easier to move or who wants to add Z80 opcodes is
invited to do so. The original Australian readme follows:

This is distributed on the basis of people who use it return their improvements.

We would like Z80 emulation.

CPM8080.MAR is really a general emulator. INs and OUTs trap to subroutines
that have to be supplied. For CPM IN is used to do all the CBIOS functions.

To use it first get a CPM license from Digital Research. Add in the VBIOS
provided. Copy the floppy to a RMS disk file using the FLOPPY program.
Now give that as DISK A when you start up the CPM program.

The CPM program itself contains no proprietary software - it is not much
use without a CPM disk!


++++++++++++++++++++
[312,350]README.
+++++++++++++++++++++
Unix Logo Interpreter
	Lincoln-Sudbury Regional High School

-----
This is release 3 of Unix Logo.  Release 1 was the one on the first 1982
Usenix tape.  Release 2 was sent by me (BH) directly to only a few sites.
This release is much like release 2 in capabilities and syntax, but has
been rearranged internally somewhat to make the process of installation
on a new system a bit easier.  One major new feature in release 3 is the
pause facility, which allows interactive debugging in the local context
of an error.  More on this below.

I would like to thank Don Martin and his students at the College of Marin,
who have found huge numbers of obscure bugs in Logo and therefore helped
make this release much more reliable than it would otherwise have been.

If you have questions about this Logo, there are two places to write for help.
On the east coast, try
	Computer Department
	Lincoln-Sudbury Regional High School
	390 Lincoln Road
	Sudbury, MA  01776
On the west coast, try
	Brian Harvey
	2456 Hilgard Av #406
	Berkeley, CA  94709


++++++++++++++++++++
[312,366]README.1ST
+++++++++++++++++++++

			DTC  -  The Desk Top Calender

		       		Mitch  Wyle

		      	       December 1982

		 	Version 1:  REVISED BY GCE



	The  idea here  is to automate an appointment calender.  Most
	appointment  calenders  give  only  one of Month-At-A-Glance, 
	Week-At-A-Glance, or  Day-At-A-Glance.   DTC is an attempt to 
	give all of these functions in a paperless, fast, menu-driven 
	format.

	This release has had considerable work done to it to make it a
	more general tool. See the addendum for the extras.

	Among the features I would like to see added:


		-	Year-At-A-Glance in 132 column mode with
			two rows of six months each

		-	Menu option(s) to print out appointments,
			in day, week, month format

		-	Support for non VT-100 terminals
			(general cursor positioning calls)


	DTC  is  one  of a number of Paperless Office programs I have
	been developing  for  two years.  Other  related programs are
	an on-line telephone directory, an electronic mail system, an
	automatic "While You Were Out"  message  taker  which  spawns
	mail directives, Memo and Form letter templates and programs,
	and software tools for writers in a business environment.

	Mitchell F. Wyle

	Revision 1: Glenn C. Everhart

	I have added a few extras to the program to make it more
	usable and fix a few small bugs. The following has been
	done:

	* Date bugs in displaying weeks at the beginnings of months
	are fixed.
	* The E in Evening now is a pseudo time and gets displayed as
	17:00 on the weekly summary. You can enter evening appointments
	using the D command with E for time. (EV works OK too.)
	* Most commands are accepted in lower case or upper case.
	* Commands T (Today), R (Reminder), and C (Calendar) correspond
	to Day, Week, and Month exactly but cause DTC to exit after
	they are executed. This permits them to be used from MCR
	with instant exit, thus to be placed into login.cmd files for
	an "auto reminder" service.
	* Time ranges may be input (so long as it is done with no format
	errors) in the form hh:mm>h2:m2 (e.g. 09:00>15:30) which will
	replicate the appointment part of the line into DTC.DAT
	over the indicated range.
	* Purge of old appointments (clear out appointments from before
	a given date, defaulting to today)
	* Reverse display of week/month times permitting FREE times to
	be found and displayed rather than occupied ones (potentially
	for a group of people)
	* A second level of data files, permitting an appointment file
	to contain pointers (1 level deep) to other files which can be
	searched as well as the first
	* Multiple appointment files, changeable on command (permitting
	"private" appointment calendars)
	* Scheduling of appointments in multiple files (useful for setting
	up meetings or maintaining multiple files)
	* Lookup for free times of length n * 30 minutes (where n is any
	number in the range 1 to 18) over a week period; display of
	times is made in Week format. Valid start times for meetings of
	given lengths are shown.

	New commands:

P [mmddyy]	- Removes all appointments from current calendar file
		whose date is BEFORE the date specified. If no date
		is specified, today's is assumed.
N(command)	(for example
	NW [mmddyy] )
		- Displays FREE time instead of scheduled time in week or
		month formats. Not deemed useful for Day format, so left
		out there.
F filename	- Closes current calendar file (defaults to DTC.DAT
		initially) and opens filename instead
S [mmddyy hh:mm[>hh:mm]] appointment/meeting
		- Schedules appointment /meeting at the given time.
		If current calendar file contains pointers to other files
		(see below; year=99 and appointment part has 'filename='
		in it) then each of those gets a notice of the appointment
		or meeting added to it as well as the current calendar.
		Otherwise only the current calendar file is updated in the
		D format.
L [mmddyy] nn	- Locate a period of nn half-hours in the week containing
		mmddyy. Displays the free time in week format. Used to
		schedule meetings. nn must be 01 thru 18 and is clamped
		to this range

POINTERS in CALENDAR FILES
	The calendar file format is sequential records of the format:

YYMMDDTTTappointment text of 60 characters length

in which every record has this form, and the time TTT is in the range
(for correct files) of
080 through 170 (for 08:00 through 17:00). The third digit is always
either 3 or 0 as well, since DTC only schedules half hour periods.
	Indirection is accomplished by editing your calendar file
(with any editor) or just entering an "appointment" for year 99 (by which
time somebody should have hacked some more on this to fix it up not
to mess up real appointments). The text of the "appointment" should
be just filespec=, with the = sign as the terminator of the file spec.
This will lead to the file you specified being opened and treated as
if it existed inside your own calendar file (except you need to use
the S function rather than the D function to enter appointments in
it as well as your own.)

CAVEATS:
	DTC is a bit touchy about illegal inputs. Be sure you input
the mmddyy in the format given (i.e. July 4, 1983 is entered as
just "070483", NOT as "7/4/83" or "7483" or anything else. If
DTC seems to generate weird displays, edit DTC.DAT (or whatever
else is your calendar file) and remove or edit lines in which the
date or time are in illegal format.

	To use DTC, you need to create an empty DTC.DAT file
first (and also any other calendar files you expect to need.)
The simplest way to do this in RSX is to use the command

PIP DTC.DAT=NL:

and in VMS

MCR PIP DTC.DAT=NL:

but any method will do, including using an editor to set it up. Don't
be alarmed about occasional open file errors; most have been fixed
but just re-run DTC if any still show up; they don't corrupt your
calendar file. I haven't seen any for awhile, so don't think many
(if any) remain, but I could have missed a spot where a redundant
close is needed. You may fix if need be.


++++++++++++++++++++
[312,370]AAAREADME.TXT
+++++++++++++++++++++
This area has a newer DTC from C. Garman of RCA MSR. Compile
with DTCI4.COM and link with DTCLK.COM. Try it; it has many
features not present in the older one.
	In particular meeting scheduling and instant queries of
your schedule are much easier with this than with older versions.
Also the display is much faster and more readable.


++++++++++++++++++++
[312,371]README.1ST
+++++++++++++++++++++
        This area contains code for a PortaCalc
version which will operate in very small environments by
using bitmaps, etc., for storage. The WRKFIL and WRKSHT
routines are called whenever the work file was accessed
or VBLS, FVLD, or TYPE are called.
        Note that to gain space, the multiple precision
integers are reduced to 20 characters' length from 100.
NOTE: THERE IS ONE DIFFERENCE IN PROGRAM USE SYNTAX BETWEEN
THIS VERSION AND OTHER PORTACALC VERSIONS:
The command R (recalculate) in this version recalculates the
sheet, but does NOT force recalculation of constants. The command
RF recalculates and DOES FORCE recalculation of constants (and the
command RR is a synonym for RF). RF can be read as "recalculate, force".
In the OTHER versions, R forces recalculation of constants, and RAF
recalculates everything except constants. Note that RAF in this
version works as it does in others; bare R however has changed.
Otherwise this version has the capabilities of the full VAX
versions, except the *U XQTCM function is not available (and will
not be until a larger machine that permits major mods to the overlay
structure is available.)

	THIS PROGRAM IS NOW THE PREFERRED PORTACALC FOR PDP11 MACHINES
AND FOR FURTHER DEVELOPMENT. The command files ending in "NAT" were
set up to build a PDP11 .TSK image for RSX under VMS with the RSX TKB
task. For RSX, edit PCCPDP.COM into a .CMD file (take out $ signs
and be sure device defaults etc. are OK) and verify that the FCS11M.ODL
reflects your F77 installation (or fix it up with the F4P flavor if
using F4P); then build. The task WILL FIT on a PDP11 if F77 is used.
If you use F4P, be SURE the FCS11M.ODL reflects the F4P OTS so addresses
won't overflow. The capacity is around 16,000 cells on RSX (edit
PVKLUGPRM.FOR to change how they are assigned in rows and cols). If you
have the ability to use virtual arrays and/or I/D space, or FCSFSL
(you M+ jocks know what that is), DO SO and reduce the complexity of
the overlay structure. It probably won't fit flat, but every simplification
speeds up the program. You can also increase the in memory array sizes
with I/D space or FCSFSL (supervisor mode FCS) if your machine allows.
Again, the parameter file controls this.

RSX BUILD:
 Use PCCPDP.COM as a compile template for PDP11 RSX, or PCCPRON.COM
for PRO 350. Then link using PCCNAT.CMD (and pccnat.odl). This assumes
the F77 compiler is installed as ...F4P. Note that FCS11M.ODL needs
to be adjusted to YOUR version of the F77 compiler. A couple minor
changes to the OPEN statements will be needed for old F4P but otherwise
all should run OK. The compiler will complain about the differences if
you have F4P; that'll show you what to alter. PCCPDPOLD.COM is a somewhat
older PDP11 build file. Tweak the stack size and/or the sheet size in
pvklugprm.for to shrink if needed. Be sure to build against the FCS flavor
Fortran library and that your SYSLIB does NOT have the ANSI magtape
support routines included for size reasons.
	If you run RSX11M+ and can use I/D space and supervisor mode,
edit the ODL file to flatten it somewhat and also include the line
SUPLIB=FCSFSL:SV in your taskbuild and throw away the FCS overlays.
That'll gain you a lot of space. You need to link with the /ID qualifier
then and BE SURE your F77 compiler has the necessary patch (done in
linking the F77 image). The patch is something like GBLPAT=FORTRAN:DSPACE:1
and DEC leaves it out because their debugger won't handle I/D space.
Use DDT which is free and WILL handle I/D space and put the patch in,
and forget F77-debug, which does little or nothing more than DDT does
anyhow, and has the abovementioned restriction (and takes more space
in your task to debug it than DDT). DDT is available as DECUS #11-SP-6
or in the 11-SP-47 distribution.

VAX USERS:
	The PCCMAKIV.COM file builds a fairly respectable VAX version
of this program which uses less virtual address space than the "standard"
one. It does use memory arrays instead of files, but uses formula memory
more efficiently. I have begun putting the hooks for a Datatrieve
interface into it, which is not fully defined yet. However, the idea
will be that a command of the form DTR command will be stripped of
the "DTR" and passed to Datatrieve (so you can ready domains and
the like), and some functions of syntactic form *U DBxxxx will
generate calls (from inside any cell) to return values or text
from Datatrieve. This will allow you to avoid the present method
of creating sequential files (possibly from DTR) and then using
the *Q class commands to extract formulas or values from them;
you'll be able to grab the formulas direct. These functions will
be isolated into a set of separate routines to make it easier to
replace the DTR interface with one of your choice should you
so desire. We need it at my site, so I expect to get it done
sometime in the next 6 months or so; depends on timing of other
things at the office... (as usual). I want to retain the ability to
expand the number of cells greatly, so I will update this version
rather than another. The "standard" VAX version uses much more space
because it uses 128 bytes per formula entry accessed. This will
quickly run out of room (even on a VAX) if the number of cells
increases by an order of magnitude or two. The version here will not
so easily run out, since it does not require memory for every cell.
Nevertheless, the parameters set up by default here (i.e., unless
you edit BVKLUGPR5.FOR) allocate memory for 4 formula nibbles
(12 characters each) per cell. 8 bytes per cell for values are
also used, but this will not cause trouble on a VAX even with much
larger sheets, and the bitmaps will cause no trouble either. You can
run out of space on this version, but only if you have an average of over 48
characters in every cell addressable. This is unlikely except in the most
extreme cases. If it happens, edit BVKLUGPR5.FOR and increase some
of the parameters to get more room. LPDM and LPDMF are the ones to
raise.
	THE PCCMAKIVD.COM file for VAX users has all the above features
PLUS a DTR 32 interface. See DTRIF.DOC for the DTR calls. Only this
version of VAX AnalytiCalc has a DTR interface. A small speedup in
calculations has been added since the 84B SIG tapes also for both
the PDP11 and VAX versions. This is done by keeping track of whether
any D#col#row cell forms have been used. If not, some time can be
saved (and now is) by not looking for each cell's display coordinate
during recalculation.
	If anyone out there is using this program, I appreciate hearing
about it. Usually I hear about troubles, but appreciate hearing that it
was used for something. I'd also like to encourage anyone who develops
templates to this spreadsheet to submit them to the VAX and RSX SIG
tapes so they can be shared by others. I get very little feedback
from DECUS about who (if anyone) is ordering the Library version of
this program, and very little from users. If you use it, let me know.
Thanks. By the way, please note the "announce.mnt" file in the main
documentation directory announcing my (extremely cheap but not free)
IBM PC or general MSDOS version of PortaCalc, called AnalytiCalc. It
is descended from this version too.
		Glenn Everhart
		409 High St.
		Mt. Holly NJ 08060

	This code works on VAX and runs in either native or
compatibility mode. It has been tried on RSX and
looked OK (the build files may be deduced from the VAX compat
mode ones here) but was better tested on VMS. It IS designed
with ALL the capabilities of the VAX version except the
execution of commands from inside cells of forms like CA, CR,
etc. etc. and may be interesting for that reason.
It provides the largest PDP11 spreadsheet of any PortaCalc version
(around 10,000 cells fit; more may be possible) and should be
useful for that reason.
	Please send any versions you bring up as working back to
me in source, regardless of what machine they run on. In return
I may get you my latest mods and bug fixes.
			Glenn Everhart
			409 High St
			Mt. Holly, NJ 08060

	Note that some displays
will appear to zero various displayed numbers. An extra V (View)
command will draw the display correctly if this happens. The CR
command is known to do this.
	The memory storage is small and backs up to disk files
during operation. The sizes are asked for at startup, and if they
overflow, (i.e., a PAGE fills), a message is given on screen. If
the sizes (in K bytes) for the files are given NEGATIVE, then a
different packing algorithm is used which requires more page
swaps, but may allow less dense use of the page file and permit
the same size disk files to handle more active cells. The trade-off
is speed.
	The sizes of memory areas are compiler parameters. The
file present is fairly conservative but may be made smaller
still. LVBF should be at least 50, and LFM at least 32, for
things to make sense.
	The files are NOT opened or used if the memory storage
sizes on file are less than the in-memory storage provided.
Entering a size of 1 will ensure only memory is used. Entering
a 0 will pick a default file size.
	This is the first version of PortaCalc which plays the
same dirty trick on you as commercial spread sheets. That is,
you have a fairly huge matrix, but can't fill in all of it
without overflow. However, by specifying a large enough file
for variables and for formulae, you can always get things
to fit.
	The Best things in life are free!
		PORTACALC
	(alias AnalytiCalc)


++++++++++++++++++++
[312,374]README.1ST
+++++++++++++++++++++
This area is a contribution by Larry Finger of
2801 Upton St. NW
Washington, DC 20008

This area contains PortaCalc input files to allow you to do your
US Federal Income Tax in Portacalc. The rate tables are for the
1984 tax year and need to be edited for the 1985 rates now that
we have rate indexing.


++++++++++++++++++++
[312,375]README.1ST
+++++++++++++++++++++
PortaCalc object files for VMS
CAVEAT:
If you can possibly recompile from source on VAX, DO SO.
Only use these if you have no Fortran to compile with.
	The general technique for making an .exe is
LIBR/EXTR=*/OUT=name.OBJ name.OLB
LINK/NOMAP name

Ignore error warnings.
PCCVM is for VT100 with AVO (works on normal ones too)
PCCCS is colorscan 10 (Datamedia) terminal.
PCCX is VT100 with AVO but is the PCCPC flavor of
portacalc for VAX.
PCGRAF is the graphics package.


++++++++++++++++++++
[312,376]README.1ST
+++++++++++++++++++++
	Keypad Macros for AnalytiCalc

This area contains files for the auxiliary keypad
of AnalytiCalc (PortaCalc). They should be moved to
an area globally assigned as DK: (a single directory
small virtual disk in RSX or a directory in VMS).
	They are written short and small and are NOT
commented since comments would slow them down. Do not
attempt to learn PortaCalc command language from them.
The KEYPAD.DOC file contains information on the
% construct herein, and the PortaCalc manual has further
information about how to write command files. Please don't
let these be the first command files you read. Do however
use them if desired. Once they are moved, you may want
to rename KEYPADCS.PIC to KEYPAD.PIC to support terminals
with advanced video and/or color. If you are using a VT52,
leave KEYPAD.PIC alone. These files will work with either
PortaCalc-VM (build from COMPILVMX.COM and similar
files on VAX), or PortaCalc-PC (build with PCCMAK.COM
on VAX or modify PCCPDP.COM to build for PDP11; it's in
another directory.)
	The other set of keypad files is in the main
directory and does not use a "gold key" style keypad
interaction. These do, and attempt to put the text
"Gold 1" at the upper right part of the screen when
the GOLD key (PF1) is pressed. Other keypad commands
turn this off, but note that the "gold" condition is
cleared by cursor keys or the PF2 key without erasing
this text, so treat the text with a grain of salt.


++++++++++++++++++++
[321,001]README.1ST
+++++++++++++++++++++
;	James A.McGlinchey
;	Software Engineering Consultant
;	Post Office Box 451
;	Warrington, PA 18976
;	(215) 348-7261
;
;
;	Spring 1985 DECUS RSX SIG Tape Submission:
;
;
;		[321,1]SUPERMAC - Structured Programming 
;				 Macros for MACRO-11
;
;		[321,2] - Skeleton Device Drivers for
;			  RSX-11M, RSX-11M-PLUS
;


++++++++++++++++++++
[321,002]README.1ST
+++++++++++++++++++++
;	James A.McGlinchey
;	Software Engineering Consultant
;	Post Office Box 451
;	Warrington, PA 18976
;	(215) 348-7261
;
;
;	Spring 1985 DECUS RSX SIG Tape Submission:
;
;
;		[321,1]SUPERMAC - Structured Programming 
;				 Macros for MACRO-11
;
;		[321,2] - Skeleton Device Drivers for
;			  RSX-11M, RSX-11M-PLUS
;


++++++++++++++++++++
[321,003]README.1ST
+++++++++++++++++++++
 
			TAR(Tape Archive & Retrieval)
 
	This directory contains all files necessary to build TAR, an RSX
utility to manipulate UNIX TAR floppy volumes, either in normal UNIX for-
mat or in Tektronix TNIX(8560) format. For further information on the capa-
bilities of this utility, consult TAR.DOC in this directory.
 
	This software is and remains the property of SSG and no rights or
privileges other than those stated herein are granted to the user.
 
	This software is being contributed to the DECUS RSX/SIG free of charge
and warranty. The user, in accepting this software, understands that it is
delivered "as is". SSG accepts no responsibility for its performance.
 
	SSG grants to the DECUS RSX/SIG and to the user a license to use and
modify this software subject to the conditions listed below. The user, in ac-
cepting this software, agrees to the conditions listed below.
 
				Conditions
 
  1) The user may use and/or modify this software at his own risk.
 
  2) The user may redistribute this software at his discretion provided
     that it is redistributed under the same terms and conditions under
     which it was obtained, i.e., free of charge and warranty, and provided
     that the SSG copyright notice is included in all such redistributions
     as well as an indication that the source is the DECUS RSX/SIG.
 
 
	TAR has been implemented in the SSG version of SUPERMAC, SCAT-11.
Since no attempt has been made by SSG to ensure compatability between SCAT-11
and SUPERMAC, this program may not assemble with the versions of SUPERMAC
available through the RSX/SIG. For this reason, a pre-assembled library
of modules has been included, TAR.OLB. Also supplied is an RSX-11M v3.2
task image of TAR along with documentation and command files. If you care
to assemble the sources, change all references to SCAT11 in the sources
to the appropriate SUPERMAC invocation, SMACIT.
 
 
 
  SSG (Art Gaughan)
  Box #1595
  North Wales, PA  19454
  USA
  (215) 699-9658


	Release 2

	This version of TAR has been modified so that:

1. It will assemble and run correctly with the supplied version of
	SUPERMAC, and
2. It works with RX50 drives that are mounted foreign (e.g., by
	the supplied UTIL program).

	It is useful for communicating with VENIX or ULTRIX systems
using RX50 media since they typically do not have magtape.

	A sample command sequence to use the utility might be
something like the following (comments after the ";" characters
are not typed, only narrative):

INSTALL UTIL
INSTALL TAR		;INSTALL the two utilities

; physically place your blank RX50 in DZ1:

.UTIL FOR DZ1:		;mount the DZ: unit foreign
.TAR DZ1:/INIT		;initialize it as a UNIX volume

.TAR DZ1:=file1.typ	;copy file1.typ onto it
.TAR DZ1:=FILE2.TYP	;copy file2.typ onto it too

.TAR DZ1:/LIST		;list the floppy directory to see it's there.

; to go the other way omit the /INIT and use a command like:

.TAR =DZ1:file1.typ

;to get the file to RSX from TAR format.
modified by Glenn C. Everhart	3/26/1985


++++++++++++++++++++
[332,012]AAAREADME.TXT
+++++++++++++++++++++
     BONNER LAB RUNOFF                                                  Page 1
     

                                      AUTHOR:
                                      -------
                                   John Clement
                                Bonner Nuclear Lab
                                  Rice University
                                     Box 1892
                                 Houston Tx, 77251
                                  (713) 527-4018


                                     ABSTRACT

                              Bonner Lab Runoff (RNO)

     Bonner  Lab Runoff is a text formatter which when used with your favorite
     editor makes a complete word processor.  Its syntax is almost a  complete
     emulation of DSR (Digital Standard Runoff) and it is very compatible with
     previous versions of Runoff.  The document and help file for this version
     can  also be used for DSR.  The intent of this program is to support com-
     plete scientific word processing to produce publication  quality  output.
     It  has been used to produce thesis, progress reports, and scientific pa-
     pers here at Rice University.  

     This version allows complete control of any special printer available via
     user definable escape sequences.  In addition  a  macro  facility  allows
     text  or  sequences  of commands to be abbreviated to a single label.  If
     the printer has the correct features then variable  spacing,subscripting,
     superscripting, and equation formatting are possible.  By properly defin-
     ing escape sequences the user may support different printers in  a  tran-
     sparent  fashion.   In  other  words  the  same  input text will print in
     identical fashion on different printers with different control codes  and
     escape sequences.  

     Table of contents, indexing and sub-indexing are all supported.  Multiple
     table of contents or multiple indexing may be constructed from the avail-
     able  commands.   A  variety  of LAYOUT and STYLE commands may completely
     change the look of the pages.  Table layout is simplified by right justi-
     fied  and 'decimal' justified tabs.  Permanent margins which apply to the
     page headers are available.  These simplify the  setting  of  header  and
     text margins.  

     All  special  characters  are  redefinable.  The user may define new com-
     mands, and text macros.  By defining commands you can  make  it  resemble
     other  text  formatters,  or  other  verstions of RUNOFF.  You may define
     numeric symbols facilitate constructing lists of arbitrary items.   These
     allow page and section references.  A 2 pass option allows forward refer-
     ences to symbols defined later in the text.  

     This  runs  under VMS, RSX, IAS, RT11, TSX, and probably RSTS.  It should
     run on a PRO with no modifacations.  RNO occupies a minimum of 30  to  37
     kbytes depending on the operating system.  

                                   Distribution

     This  distribution  contains all files necessary for building RNO for any
     supported operating systems.  Nearly All file names are 6  characters  or
     less  to  acommodate all operating systems.  Once you have built the exe-
     cutable image, you can use it to generate documentation  and  help  files
     for  your  operating system.  Several files are included to document this
     version.  Instructions for building the  program  are  in  the  BUILD.DOC
     file.   Bugs that have been fixed are in RNOBUG.DOC.  The latest enhance-
     ments are in CHANGE.DOC.  The VMS distribution contains RNO.EXE, but  all
     other  users  must build RNO.  The full document (RUNOFF.DOC) is not dis-
     tributed on small (floppy) kits, but it is included with mag tape kits.  


++++++++++++++++++++
[350,050]README.1ST
+++++++++++++++++++++
[350,50] Submission from B. Z. Lederman

How Fast is your CPU? A set of programs which will measure
CPU instruction execution speed, with test results for the
PDP-11/70, PDP-11/84 and PRO-350, and a description of how
the tests work. Also, a preliminary version of a speed test
for the VAX.

Sort-11 V3.0: a set of articles on how it compares with V2.0,
and instructions on how to get it to run faster by building
it linked to RMS resident libraries, non-overlayed, and/or
I-and-D space, with test results.

Error Log Reports: how to get RPT to run considerably faster
by building it non-overlayed and I-and-D space. Also a version
which is overlayed but faster than the DEC supplied version
for people whose systems don't have I-and-D space.

SPM-11: two programs to make it easier to read the data from
SPM. One reads all collected records and translates them into
english (has been on a previous SIG tape), the other translates
overlay read requests. Includes a module which makes it easy
to use Abort ASTs in Fortran.

DCL as a Catch-all for MCR: a copy of the Multi-tasker article on
how to get this to work. It is a really nifty combination, giving
you the best of MCR and DCL at the same time.

Plus a couple of simple programs: one lets you input an FCS error
number and translates it into english using the message file that
comes with RSX. The other reads .STB files and lists the symbols
defined there.

See [350,50]README.2ND for further descriptions of what each file
in this account is for.

B. Z. Lederman
2572 E. 22nd St.
Brooklyn, N.Y. 11235


++++++++++++++++++++
[351,070]AAAREADME.1ST
+++++++++++++++++++++

	Project Software & Development, Inc.
	14 Story St.
	Cambridge, Ma. 02138
	617-661-1444

	Program:	VTL
	Author:		Robin Miller
	Date:		Fall 1984

     Description:

	This program is used to list file(s) on a VT100 family  terminal.
     The  file(s)  are  displayed  one screen at a time for easy viewing.
     Various commands can be entered to change listing parameters  or  to
     position  to a particular portion of the file.  Many of the commands
     are the same as the Digital editor EDT.   Commands  can  be  entered
     either by using keys on the VT100 keypad, or by entering commands to
     the prompt at the bottom of the screen.  Some of the major  features
     of the program are outlined below:

       o  CTRL/C detection for aborting searches, etc.
       o  Delete the file being displayed.
       o  Display a ruler along the top of the file.
       o  Display the next file or next the directory.
       o  Display record numbers along the left margin.
       o  Display the file header of file being displayed.
       o  Print the file being displayed.
       o  Search (forward only) for a specified string.
       o  Shift the display window left or right.
       o  Split screen mode to display two files.
       o  Teco compatible see-all mode.
       o  Write portions of the file being displayed.

     The maximum record size that can be  displayed  is  512  characters.
     All  commands  have a repetition count of one.  Relative and indexed
     files are not supported.

     The  special  wildcard  characters "* and %" can be used with VTL on
     RSX-11M using FCS for I/O instead of RMS. Previously these were only
     valid  on VMS since a native image was being called to lookup files.

     [ File "VTL.MEM" contains full documentation for this program. ]


++++++++++++++++++++
[351,072]AAAREADME.1ST
+++++++++++++++++++++

       			       Free software BY
			     Northern Telecom Inc.

     This  software  is  furnished for free and may be used and  copied as
     desired. This software or  any  other copies  thereof may be provided
     or  otherwise  made  available  to any other person.  No title to and
     ownership of  the  software  is  hereby transferred or allowed. 

     The information in this software is subject to change  without notice
     and should not be construed as a commitment by NORTHERN TELECOM INC.

     NORTHERN TELECOM assumes no responsibility for the use or reliability  
     of this software on any equipment whatsoever.

	Northern Telecom Inc.
	Network Support Systems Division
	P.O. Box 649, Airport Road
	Concord, New Hampshire 03301
	(603) 224-6511 X2024

	Program:	DIRectory
	Author:		Robin Miller
	Date:		Spring 1985

Description:

   The  DIRECTORY command lists the files contained in a directory.  When
   you use certain qualifiers with the command, additional information is
   displayed,  along  with  the  names  of  the files.  The output of the
   DIRECTORY  command  depends on certain formatting qualifiers and their
   defaults.  These  qualifiers  are:  /COLUMNS,  /DATE,  /FULL,  /OWNER,
   /PROTECTION, and /SIZE.

   In  studying the qualifiers and the capabilities they offer, watch for
   qualifiers that override other qualifiers. For example, if you specify
   the  /FULL  format,  the  system cannot display all the information in
   more  than  one column.  Thus, if you specify both /COLUMNS and /FULL,
   the number of columns you requested is ignored.

   Format:	DIRECTORY [file-spec[,...]]

   Additional information available:

   ALL         BEFORE      BRIEF       COLUMN      CONTROL     CREATED
   DATE        DETACH      EXPIRED     FID         FILEID      FORMAT
   FORMFEED    FULL        GRANDTOTAL  HEADING     HELP        MODIFIED
   OUTPUT      OWNER       PARAMETERS  PRINTER     PROTECTION  REWIND
   REVISED     QUALIFIERS  SINCE       SIZE        SPOOL       STARTUP
   TODAY       TOTAL       TRAILING    VERSION

	*****************************************************
	* Refer to the help file (DIR.HLP) for descriptions *
	* and examples of the above qualifiers.             *
	*****************************************************


++++++++++++++++++++
[352,004]README.1ST
+++++++++++++++++++++
 
[352,4]README.1ST - New Orleans - Spring 1985 - Files submitted by:
 
			SRD Working Group
			Bob Turkelson
			NASA/Goddard Space Flight Center
			Mail Code 614
			Greenbelt, MD  20771
			301-344-5660
			FTS 344-5660
 
 
This UIC contains the files for building SRD V6.6.
 
The modifications made by the SRD Working Group since V6.5 are:
 
  o  Modified the sort algorithm for greatly improved performance.
	(Thanks to Jim DeMange and Tony Gandy of Systeme Corporation,
	Orlando, FL.)  The improvement will be noticed most when
	listing large directories.  Using RSX-11M-PLUS accounting,
	we found that to generate a brief sorted listing of a
	directory containing about 1300 files, the CPU time went
	from 1992 units with V6.5 to 804 with V6.6.  (The time
	for PIP /BR unsorted listing was 1646.  SRD issued 91 QIO's
	while PIP issued 1707.)

  o  Turned off /HD (command line display) when a listing file is
	not specified.  There is no need to display the command
	line when listing files on TI:.

  o  Corrected a problem where an output filename spec with embedded
	blanks resulted in a "Directory not found" error message.
	This problem was introduced with the V6.4 modification to
	display the original command line, and was fixed by moving
	the new code to a different location.

  o  Rewrote most of SRDTST, making the logic easier to follow,
	while fixing a bug which ignored /WI when a '*' was given
	in the match template (e.g. AB*D failed to match ABCDE).
	The original code worked at the time it was written, when
	wildcards were not allowed in file specifications on command
	lines, but broke when RSX-11M V4.0 and RSX-11M-PLUS V2.0
	permitted embedded wildcards.  However this bug was noticed
	only recently.

  o  Modified the help and command files.  For P/OS and Micro/RSX
	systems, SRD is now built non-overlayed by default.


The *.C66 files are correction files which have already been applied to
the V6.5 source files.  They are provided here for reference purposes
only.  The *.MAC files are those for V6.6.

SRD.TSK is a task built with the default switches shown in SRDDEF.HLP;1.
It was built for RSX-11M V4.0/V4.1 with dynamic checkpoint allocation.

SRDMOD.DOC describes the past changes to this version of SRD.

SRDREF. is the text for a two-page SRD Reference Guide showing the
available switches.  Please send us any ideas you have for improving
its organization and content.  We will be updating it for each new
version.  HELP SRD GUIDE will display an on-line version of SRDREF.

EXAMPLE.GEN shows an example of generating this version of SRD.
 
Procedure:	@SRD		!  Asks configuration questions and
				!    builds SRD

		Copy SRD.HLP and SRDDEF.HLP to [1,2] and refer to SRD.HLP
		in [1,2]MCR.HLP.
		HELP SRD NOTES will display various things you should know.
		HELP SRD NEW will show users a list of recent new switches.


The changes to the selection/listing overlay segment and the root
segment result in a decrease of 140. words (when built without FCSRES).
The largest directory section which can be handled at one time remains
at approximately 110 blocks.  Each block contains up to 32 file entries.

The SRD Working Group plans to make additional modifications for future
SIG tapes.  Command and help file improvements are planned as well as
program changes.  A number of changes on our wish-list are currently
being implemented for the next version.
 
We would appreciate hearing from those who have made changes or plan to
make changes to this version or other versions, so we can continue to
improve this useful utility.  Many thanks to those who have written.
 
[352,4]README.1ST - END



++++++++++++++++++++
[356,010]README.1ST
+++++++++++++++++++++
Akron, Ohio
May 1985

Notes on a submission to the RSX SIG tape for Spring 1985 DECUS
Symposium at New Orleans, Louisiana.


*********************************************************************
IMPORTANT: The files in this save set are designed to properly modify
RSX11M V4.1 Update D patched distribution kits.
*********************************************************************

The files in this SIG tape submission allow a system manager to make
a number of useful modifications to an RSX11M system at the time it
is built.

The set of changes made by the files HEXMOD.CMD and HEXMOD.COR install
a hexadecimal numeric processing facility into RSX11M that parallels
the current capability to process octal numbers in command lines.
The HEXMOD.DOC file describes the changes in more detail, and provides
instructions on how and when to apply the changes.

The changes made by the files EXEDRVMOD.CMD, EXEDRVMOD.COR, SYSGENMOD.CMD
and SYSGENMOD.COR apply a set of changes to RSX11M sources and SYSGEN
command files to make all DEC supplied device drivers into loadable
drivers with LOADABLE DATA BASES!  (Something RSX11M+ has standard!)
The SYSGENMOD.DOC file describes the changes in more detail, and
provides instructions on how and when to apply the changes.

The DECUSMODS.CMD file is the main driver file for applying both sets
of changes described above.

In addition, the XEDRVMOD.CMD and XEDRVMOD.COR files apply a
critical patch to the DEUNA device driver released with RSX11M
V4.1 Update D.
The file DEUNASPR.DOC completely describes the problem, its solution
and the documentation change that must also be made to make DEUNA
Ethernet controller diagnostic functions perform properly when
no data transfer is to be performed with the diagnostic function.
The file is the body of an SPR submitted to DEC in late April 1985
describing and correcting the problem.

To use the modification file set on each type of distribution kit, follow
the directions below that pertain to your system.

For Big Disc Distribution kit:

To use the modification kit on the Big Disc Distribution, restore the
modification file set to the RSXM35 volume on the system drive after
applying RSX11M V4.1 Update D.
Then invoke the DECUSMODS.CMD command procedure.
When the procedure is finished, the modification file set can be deleted.

For RK06/RK07 Distribution kit:

To use the modification kit on the RK06/RK07 Distribution, after applying
RSX11M V4.1 Update D restore the modification file set to the RSXM35
volume on the system drive.
Then invoke the DECUSMODS.CMD command procedure.
When the procedure is finished, the modification file set can be deleted.

For RL02 Distribution kit:

To use the modification kit on the RL02 Distribution, after applying
RSX11M V4.1 Update D restore the modification file set to the RSXM35
volume on the system drive.
Then load the second volume of the distribution kit, EXCSRC, on DL1:,
mount the volume with MOU DL1:EXCSRC and invoke the DECUSMODS.CMD
command procedure.
When the procedure is finished, the modification file set can be deleted.


Good luck,

Carl T. Mickelson
Goodyear Aerospace Corporation
1210 Massillon Road D470/G3
Akron, Ohio 44315
(216) 796-2388


++++++++++++++++++++
[356,011]README.1ST
+++++++++++++++++++++
Akron, Ohio
May 1985

Notes on a submission to the RSX SIG tape for Spring 1985 DECUS
Symposium at New Orleans, Louisiana.


*********************************************************************
IMPORTANT: The files in this save set are designed to properly modify
RSX11M V4.1 Update E patched distribution kits.
*********************************************************************

The files in this SIG tape submission allow a system manager to make
a number of useful modifications to an RSX11M system at the time it
is built.

The set of changes made by the files HEXMOD.CMD and HEXMOD.COR install
a hexadecimal numeric processing facility into RSX11M that parallels
the current capability to process octal numbers in command lines.
The HEXMOD.DOC file describes the changes in more detail, and provides
instructions on how and when to apply the changes.

The changes made by the files EXEDRVMOD.CMD, EXEDRVMOD.COR, SYSGENMOD.CMD
and SYSGENMOD.COR apply a set of changes to RSX11M sources and SYSGEN
command files to make all DEC supplied device drivers into loadable
drivers with LOADABLE DATA BASES!  (Something RSX11M+ has standard!)
The SYSGENMOD.DOC file describes the changes in more detail, and
provides instructions on how and when to apply the changes.

The DECUSMODS.CMD file is the main driver file for applying both sets
of changes described above.

In addition, the XEDRVMOD.CMD and XEDRVMOD.COR files apply a
critical patch to the DEUNA device driver released with RSX11M
V4.1 Update D.
The error was NOT repaired with Update E, and is still required.
The file DEUNASPR.DOC completely describes the problem, its solution
and the documentation change that must also be made to make DEUNA
Ethernet controller diagnostic functions perform properly when
no data transfer is to be performed with the diagnostic function.
The file is the body of an SPR submitted to DEC in late April 1985
describing and correcting the problem.

To use the modification file set on each type of distribution kit, follow
the directions below that pertain to your system.

For Big Disc Distribution kit:

To use the modification kit on the Big Disc Distribution, restore the
modification file set to the RSXM35 volume on the system drive after
applying RSX11M V4.1 Update E.
Then invoke the DECUSMODS.CMD command procedure.
When the procedure is finished, the modification file set can be deleted.

For RK06/RK07 Distribution kit:

To use the modification kit on the RK06/RK07 Distribution, after applying
RSX11M V4.1 Update E restore the modification file set to the RSXM35
volume on the system drive.
Then invoke the DECUSMODS.CMD command procedure.
When the procedure is finished, the modification file set can be deleted.

For RL02 Distribution kit:

To use the modification kit on the RL02 Distribution, after applying
RSX11M V4.1 Update E restore the modification file set to the RSXM35
volume on the system drive.
Then load the second volume of the distribution kit, EXCSRC, on DL1:,
mount the volume with MOU DL1:EXCSRC.
Finally, load the new Update E RL01/RL02 volume, PRVBLD, on DL2:,
mount the volume with MOU DL2:PRVBLD, and invoke the DECUSMODS.CMD
command procedure.
When the procedure is finished, the modification file set can be deleted.


Good luck,

Carl T. Mickelson
Goodyear Aerospace Corporation
1210 Massillon Road D470/G3
Akron, Ohio 44315
(216) 796-2388


++++++++++++++++++++
[356,012]README.1ST
+++++++++++++++++++++
Akron, Ohio
May 1985

Notes on a submission to the RSX SIG tape for Spring 1985 DECUS
Symposium at New Orleans, Louisiana.


*********************************************************************
IMPORTANT: The files in this save set can be used with any version of
RSX11M from V3.2 thru V4.1.
*********************************************************************

The files supplied here represent a FORTRAN callable RSX11M command line
interface package, together with some examples of how to use the
facilities provided by the programs.

The files CSINTF.MAC and CSINTR.MAC are two versions of the basic command
line interface.  The principle difference between the two versions is that
CSINTF uses an internal command line buffer, that cannot be accessed by the
user program other than to process commands.  The CSINTR version uses an
external command line buffer, and allows the user program to process the
command in conjunction with the RSX11M CSI facility.

The files CSINTFDEF.MAC and .MLB are macro definitions and a macro library
that are used by the interface routines.

The rest of the files contained here are samples of how to set up switch
tables and the other data bases needed between the user program and
the command line interface.

Full documentation on the use of these interface routines will be published
in a forth-coming Multi-Tasker article, as soon as the article is completed.
Full examples will be provided in that article to illustrate how a user
program can use this interface package to create applications that look just
like DEC provided utilities.

Good luck,

Carl T. Mickelson
Goodyear Aerospace Corporation
1210 Massillon Road D470/G3
Akron, Ohio 44315
(216) 796-2388


++++++++++++++++++++
[370,112]README.1ST
+++++++++++++++++++++
	REUTERS, LTD	RSX CONTRIBUTION SPRING '85

The following five files are contained on this tape:


LABEL.MAC

	This task accepts command lines in either of two forms:

		LAB dd:		or	LAB ddn:

	A file called LABEL.CMD;1 is created in your current UIC;  if you then
	include the command "@LABEL" in an indirect command file, the global
	string symbol "$LABEL" will be defined as the volume label of the
	specified disk.

	NOTE that the command "LAB ddnn:" won't work.  This should be an easy
	fix.


MAKLABEL.CMD

	This command file creates two files, LABELASM.CMD and LABELBLD.CMD, 
	and then invokes them to build the LABEL task.  Note that LABEL 
	installs as ...LAB.


WHERE.CMD

	Some of our systems consist of two 11/70s, linked by DECnet as live
	and backup.  The two systems are nearly identical, and I often forget
	which system I'm on or which system I've remoted to.  Put this in
	[3,54] on your RSX-11M+ system, and anyone who types @WHERE will know
	where they are.  If accounting is turned off, or if you've logged in
	before accounting is turned on, much of the usual information isn't 
	available.


MAIN.CMD
INDEX.CMD

	I'm not claiming wonderful things for these, but they're the best I 
	could do in the middle of the night when I discovered how poorly the
	modules in [1,2]INDSYS.CLB worked on my system (RSX-11M+ V2.1E).

	Seems the <filspc> parameter gets clobbered somehow when .INDEX is
	chained to from .MAIN. if your UIC isn't the same as the one the
	library file is in.  This causes .INDEX to fail miserably.

	Use the following two command lines to fix your copy of INDSYS.CLB:

		LBR [1,2]INDSYS.CLB=[uic]MAIN.CMD/RP:.MAIN.
		LBR [1,2]INDSYS.CLB=[uic]INDEX.CMD/RP:.INDEX



	*****> SOME TIMELY WARNINGS/INFORMATION/ETC <*****

	Our systems are PDP-11/70s, running RSX-11M+ V2.1E.  All of our users
are privileged, so if you're non-privileged you may have some surprises.  I
don't expect this to be the case, but I simply don't know.  Additionally, there
is no way for me to know if any of this will work on anything but the above
system configuration.

	These files are supplied to DECUS for use, free of charge, by anyone
who wants them.  There are no guarantees of anything concerning this stuff.
If you have any problems, feel free to contact me at the address which follows.
I can't promise to fix it, but I can certainly try!

	Gus Altobello
	Reuters, Ltd
	90 Davids Dr
	Hauppauge, NY  11788


++++++++++++++++++++
[370,230]README.1ST
+++++++++++++++++++++
         TEM - Terminal EMulator for RSX -- Version:  85.008      PAGE 1 
 
         Author: T. R. Wyant III, E. I. DuPont de Nemours, Richmond, VA. 
 
         Operating System:  RSX11M+ V2.0 forward, RSX-11M V4.0 forward. 
 
         Language:  MACRO-11 
 
         Memory Required:  14KW 
 
         Other Hardware Required:  Dial-out Modem 
 
         Keywords:  RSX-11;  Communications;  Terminal Emulator 
 
         Abstract:  TEM provides "dumb" terminal emulation over  a  full 
         duplex TT:  line.  It allows the user to "become" a terminal on 
         a remote system, and to do ASCII file transfer between systems. 
         TEM  has  been  used  to  communicate  with RSX, VMS, RSTS, and 
         TOPS-20 systems, as well as non-DEC equipment.  It requires  no 
         software  on  the  remote  system  (and  therefore has no error 
         checking).   
 
              In addition to the basic functionality, TEM can  automati- 
         cally  issue  canned  commands to smart modems at the beginning 
         and end of a session.  The user can also select from  the  fol- 
         lowing features: 
             * Local Echo 
             * Automatic linefeed on carriage return 
             * Translation of inbound control characters to ASCII abbre- 
                 viations  
             * Passthru of control/s, control/q, control/o and control/x 
                 to the remote system 
             * User selectable attention and end-of-file characters. 
             * Redefinition of any desired input character to any other. 
             * Specifiable delay and prompt character for file transfer. 
             * Parity generation and checking. 
 
              TEM requires at least RSX-11M+ V2.0 or RSX-11M  V4.0  with 
         the  full-duplex TT:  driver, get/set multiple characteristics, 
         and unsolicited input AST's.  An attempt has been made to  con- 
         ditionalize it for RSX-11M V3.2, but I have no way to check it. 
         TEM can be initiated from a terminal on the TT:,  HT:,  or  VT: 
         driver, though there are restrictions on its use from a virtual 
         terminal.  It can communicate with any device on the TT:,  HT:, 
         or NL:  driver. 


++++++++++++++++++++
[370,231]README.1ST
+++++++++++++++++++++
	This directory contains several tasks and command files that I
	have found useful. These come with the standard DECUS grarantee
	(ie - if it doesn't work or crashes your system, tough). The
	phrase "Will run under" means I have tried it under these
	operating systems, and had no problems. The phrase "Should run
	under" means I have not tried it, but know of no reason why it
	needs to be modified to work under these operating systems.

	A couple of bugs in the Spring '84 version have been fixed in
	this release - see below for details.

				T. R. Wyant
				Central Virginia LUG
				E. I. DuPont de Nemours & co
				TFD - P.O. Box 27001
				Richmond, Virginia 23261


	TIZ - Task Image Zapper
	    Source Language   - Fortran-77
	    Will run under    - RSX-11M V3.2, RSX-11M+ V1.0, 2.0, and
					2.1
	    Should run under  - RSX-11M, at least back to V3.0 and
				forward to V4.1
	    Function          - Provide formatted dump of task image
				label blocks, showing name, partition,
				priority, creation date, LUN assign-
				ments, and so on. Most of the items
				dumped can be modified. This grew out of
				a task written to deal with the M+ V2.0
				task builder's incorrect common area
				access assignment (since patched).
	    Modified          - 16-Mar-84 to correctly determine where
				number of LUNs is stored, and to add
				support for TKB IDENT keyword.
			      - Summer 84 so /IP sets the right bit and
				doesn't crash your system, and to allow
				you to change the name of the resident
				library (or common) your task is mapped
				to.

	CALC - Calculator and radix converter.
	    Source Language   - "@" processor.
	    Will run under    - RSX-11M+ V2.0
	    Should run under  - RSX-11M V4.0
	    Function          - Do integer calculations in octal or
				decimal, and radix conversion to or from
				ASCII (word), RAD-50, or any radix from
				2 thru 16. User can create numeric
				symbols on the fly to store results for
				later use. Note that the calculations
				string is interpreted in "@" fashion
				(left to right), rather than in
				algebraic fashion (* and / before + and
				-). Also, trapping errors in the
				calculation string requires servicing
	CALC - Calculator and radix converter (continued).

	    Function (cont'd)	Type 2 errors with an ONERR directive,
				ignoring the manual's contention that
				you can't continue after a Type 2 error.
				Wierd things may happen in this case,
				though it has worked okay, so far.
	    Modified:	      -	To add the ability to compute an "n" bit
				checksum on the input.

	BRU - BRU command line builder.
	    Source Language   - "@" processor.
	    Will run under    - RSX-11M V3.2, RSX-11M+ V1.0, 2.0 and 2.1
	    Should run under  - RSX-11M V4.0 and V4.1
	    Function          - Construct the required mount commands
				and BRU command line to do most of our
				BRU runs. Can be invoked interactively
				(@BRU), or with parameter passing (@BRU
				IN: OU: or @BRU OU:=IN:). Validates
				input and output devices, mounts all
				unmounted media foreign (under M+ only),
				and selects BRU switches depending on
				whether the input and output media are
				disk or tape, and whether mounted
				FILES-11 or foreign. All media mounted
				by this command file will be dismounted
				when it exits.

				Under and RSX-11M+ V1.0 only, media
				should be either mounted FILES-11 or
				unmounted; unmounted devices should not
				be set public. Under the other 3
				operating systems, this doesn't matter.

				This command file will apply the /DEN
				switch for MF:, MM:, MS:, and MT: out-
				put, using the highest density avail-
				able. No density is assumed for input.
				This should be readily modifiable to
				meet individual site needs.

				This command file will also (under M+
				V2.0 and M V4.0) compute initial and
				maximum index file sizes for disk-to-
				disk transfers between different-sized
				disks. In all tested cases, these ap-
				proximate the INI defaults.

	Modified              - 16-Mar-84 to correct initialization for
				multi-header index files.
			      - Add the following switches:
					/PR to control preservation of
						file IDs.
					/IM to (partly) support image
						disks.
					/EX to support file exclusion.
				Add elapsed time calculations
				Add ability to CON the output device
					ONLINE if needed (M+).


++++++++++++++++++++
[370,360]README.1ST
+++++++++++++++++++++


	This UIC contains the I/D space version of APL-11. It must be

	ran on a RSX-11M-PLUS V2.1 System supporting Supervisor Mode

	Libraries and I/D Space Tasks. Included along with the task

	image are the Macro Modules modified, the Build Command File,

	and Overlay Descriptor File. The complete source kit for APL-11

	can be ordered from the DECUS Library (Order No. 11-SP-25).

	See the file APLID.DOC for further information. Installation

	instructions to maximize workspace size are as follows:



			MCR> INS APL/INC=64240



	This gave us a workspace size of 53,548 bytes.


++++++++++++++++++++
[370,361]README.1ST
+++++++++++++++++++++




			    COMPOSE ABSTRACT



	The COMPOSE program permits you to design and automatically

	generate custom character sets for the VT200 family of

	terminals. The output of COMPOSE consists of two files;

	a FORTRAN direct access file that contains the character

	definitions in binary form and a text file that can be

	"TYPED" at an appropriately configured VT200 terminal to

	actually create the custom character set. An example set

	of files used to generate the APL character set is included.
