PDP-10 Emulators

Last Updated: 23NOV01

This page attempts to show the differences between the various functional PDP-10 emulators.

Charateristc | Emulator
TS10 | SIMH | KLH10 | KX10
CPU | KS10 | KS10 | KS10 | KL10B | KS10?
Memory | 512KW | 512KW | 512KW | 4MW | ?
Microcode | ? | ? | ITS v.262, DEC v.130 | v.442 | ?
OS Support | TOPS-10 7.03, TOPS- 10 7.04 | TOPS-10 7.03, TOPS- 10 7.04, TOPS-20 4.1, ITS | TOPS-10 7.04, TOPS-20 4.1, ITS | TOPS-10 7.04, TOPS-20 7.0 | TOPS-20
Drives | ? | RP04, RP05, RP06, RP07, RM03, RM05, RM80 | RP06, RP07 | RP06, RP07 | RP06, RP07
Tape | ? | TU45 | TU45, TU77 | TU45, TU77 | TU45
Terminals | DZ11 | DZ11 | not supported | not supported | ?
Printer | ? | LP20 | not supported | not supported | ?
Network | not supported | not supported | IMP interface (ITS only) | NI20 | ?