1000#JUST ON
1040#PAGE 66,58,7
1060#PNUM 251
1080#SPACE 1
 1090#title Secretary Addendums
1095\
'1100<ADDENDUM 9.5/9.6 (JULY 15, 1980)
1110 
J11201) Control-D now works like it does in North Star BASIC.  To get the
L1130   second occurrance of a character, enter control-d and the character
I1140   a second time.  You do not have to enter the character itself to
&1150   fill in the first occurrance.
1160 
N11702) The @ character can be used as a valid input character.  It no longer
21180   will be accepted as an editing character.
1190 
L12003) BOOT has been changed to always jump to E800.  This is because both
G1210   new single and double density boards have the prom at E800 and
F1220   only the very old single density boards use the prom at E900.
1230 
K12404) The question about memory size has been deleted from the configure
G1250   procedure.  Instead the program will determine the memory size
K1260   itself.  This is done by writing zeroes throughout memory and then
N1270   reading them back.  When it does not get a zero back, it assumes that
L1280   is the top of memory.  If this top does not fall on a page boundry,
J1290   the message "MEMORY ERROR AT XXXX" will be printed warning you of
K1300   a possible memory problem.  If you want to force the top of memory
J1310   to be something other than the true top, change the top-of-memory
1320   variable at 2D41H.
1330 
I13405) The word PAGE has been eliminated from the first line during the
B1350   PRINT command.  Page numbers will still appear as before.
1360 
H13706) When you edit a line using the EDIT command, a right arrow will
J1380   appear on the line ahead of the edited line.  The purpose of this
F1390   is to indicate that what comes next is the edited line and to
J1400   shift the line over one character to line up with any lines above
/1410   it that you may want to pattern after.
1420 
M14307) Bugs in BSAVE/BLOAD, comment lines, and NSAVE have been checked out.
K1440   Since many double density users are also using quad density, NSAVE
H1450   does not check for room on a disk.  This is because a file that
K1460   would not fit on a double density disk would fit on a quad density
K1470   disk by writing on the second side.  Someone with a double density
M1480   disk, however, may get a disk error trying to write to a nonexistant
K1490   track in the last file on the disk.  This is not a bug, but rather
H1500   a lack of intelligence by the program.  If you get a disk error
G1510   trying to NSAVE the last file on a disk, simply put in another
H1520   disk with more space.  Also remember that the file size created
L1530   during NSAVE is four blocks larger than the size displayed with the
D1540   FREE command.  The line number bug in BSAVE has been fixed.
1550 
+15608) The data area now begins at 6100H.
1570 
I15809) The default system, prior to using CONFIGURE, is now set for 24K
I1590   of memory starting at 2000H, a 24 line CRT, a 78 character input
F1600   line, continuous forms printer, and line wrap around enabled.
1610 
G162010) When using the insert feature in EDIT, the line length may go
A1630   beyond the screen length to a maximum of 138 characters.
