NOTE:	THERE ARE TWO VERSIONS OF TECO PRESENT IN [300,10].  VERSION 20
	IS SUPPLIED IN SOURCE AND OBJECT FORM FOR RSX11D/IAS SYSTEMS, AND
	FOR RSX11M SYSTEMS IF IT (MODULES 'TECO' AND 'TECOIO') IS RE-
	ASSEMBLED.
 
	FOR RSX11M SYSTEMS, OBJECTS ARE PROVIDED FOR VERSION 22.  THESE
	ARE STORED IN THE LIBRARY 'TEC11MV22.OLB'.
 
	IF YOU ARE GOING TO CREATE TECO IN A UIC OTHER THAN [300,10], DO
	NOT FORGET TO CHANGE THE FILE SPECIFICATIONS IN THE COMMAND FILES.
 
 **FLASH**
 
	TECO VERSION 25 HAS BEEN ADDED FOR RSX11D/IAS USERS (17-FEB-77). THIS
	IS STILL A FAIRLY EXPERIMENTAL VERSION, AS IT WAS EXTENSIVELY MODIFIED
	TO RUN UNDER RSX-11D/IAS.  IT GENERATE A NUMBER OF WARNING MESSAGES
	WHEN BEING TASKBUILT, BUT THESE ARE MERELY DIAGNOSTICS (THE ODL STILL
	REQUIRES CLEANING UP).  THERE ARE NO KNOWN ERRORS IN THIS VERSION,
	AND IT APPEARS TO BE A VERY SOPHISTICATED TECO (SUPPORT FOR WILDCARD
	OPERATIONS, AUTOMATIC MACRO INITIALIZATION, ETC.)
 
	THERE IS A DESCRIPTION FILE WHICH LISTS SOME OF THE ENHANCEMENTS
	UNDER THE NAME 'TECOV25.TXT'.  NOTE THAT A NUMBER OF THE OPTIONS
	USE FEATURES OF THE RSX11M TT HANDLER, AND ARE NOT SUPPORTED BY
	THE RSX11D/IAS TT HANDLER (NOT EVEN THE NEW ONE WITH RSX11D V6.2
	OR IAS V2).  ALSO, THE DYNAMIC MEMORY SUPPORT ('GET MAIN') IS
	NOT SUPPORTED.
