			*** VUE ***

******************
**** WARNING *****
******************

This ONLY works on VT-100's


VUE is a modified version of TECO V28 which provides screen editing
capability without TECO macros. Most of us who have tried to use 
VT52.TEC or VTEDIT.TEC for keypad/screen editing on RSX-11M systems
have found that it only takes a few users to bring the system to it's
knees. For this reason, at Gould NavCom Systems we have implemented
A variation of TECO, called VUE, which supports a "window" while
the user enters normal TECO command strings at the bottom of the screen.

I have supplied only the TECO I/O modules which were modified, along
with instructions for assembling and building VUE, given the DECUS
11-333 tape and a mapped system task image. The build instructions are
VUEBLD.INF. There is a manual which I prepared for use at Gould as a
supplement to the TECO manual which documents the changes and operating
instructions.

NOTE: If you accidently scroll the screen, type 1 which forces a total
      refresh. This is documented in the manual.

******************
**** WARNING *****
******************

This ONLY works on VT-100's


Submitted by:
		Bob Denny
		Gould NavCom Systems Div.
		4323 N. Arden Dr.
		El Monte,Ca. 91731
		(213) 442-0123 Ext. 587/535
