 The DYL utility is used to load a bootable task image onto a floppy  in
 either RX01 or RX02 format.  The loader will write the bootstrap  block
 for an RX01 in single density format or an RX02 in dual density format.
 It will not, however, write for an RX02 in single  density  format.  If
 the target diskette is not at  the  user-specified  density,  DYL  will
 format the floppy to the proper density before loading.  The syntax  of
 the DYL utility is:

 DYL DYn:/Density=Taskimage[/-WB]

 Where:
  DYn: is either DY0: or DY1:
  /Density is /SGL for RX01 or /DBL for RX02 format
  /-WB is an optional switch to disable writing the Boot Block.

 In order to taskbuild a program for use with the DYL program, use the 
 following format:

 >TKB
 TKB>TASK/-MM/-HD,MAP=OBJECT
 TKB>/
 ENTER OPTIONS:
 TKB>STACK=0
 TKB>PAR=LSIPAR:stadd:size   ! Stadd is the start address in octal
 TKB>//


