
	Virtual Disk Package with error logging

	1.	Read VDXGEN.CMD and perform the edits required to [11,10]
		RSXMC.MAC.

	2.	Say ">@VDXGEN" and interact with the command file.

	3.	Copy VD.TSK, VD.STB, AVD.TSK and DVD.TSK to your system
		UIC (usually [1,54]).

	4. 	Load the VD driver.

	5.	Read VD.HLP, AVD.HLP and DVD.HLP.

	6.	Edit DCL.HLP and MCR.HLP to add the VD, AVD and DVD topics.
		It is a good idea to add a synonym for VD of "VIRTUAL_DISKS".

	7.	Edit the supplied HELP files for the number of VD units
		you chose to support at VDXGEN time.  The files are set
		up for 8 units (VD0: through VD7:).

	** In addition, if your system supports error logging:

	8.	Compile DISPATCH.CNF and DSP9M1.CNF, using the
		supplied command files. Insert/replace into
		LB:[1,6]ERRLOG.ULB.

			>INS $CFL
			>INS $LBR/INC=20000
			>@DISPATCH
			>@DSP9M1

		NOTE: DISPATCH MUST BE COMPILED FIRST, AS DSP9M1
		      REQUIRES DISPATCH.SYM TO COMPILE PROPERLY.

	9.	ERRLOG will log VD driver loads and unloads, AVD's
		and DVD's, mounts and dismounts.  Take a look at the
		FULL format report on an AVD, you'll see that it
		records the creation size and placement control
		if they are used on the AVD.

	NOTE:	See the file SPCCTL.MAC for the new "type 9" packet
		subpacket formats.

