
		Updated Loadable XDT for RSX-11M V4.0
		======= ======== === === ======= ====

	This version has a few minor fixes, and really was tested with
	a virgin EXDBT.MAC off the BL32 kit.  The BE:xxxxxx message now
	also goes to the selected terminal, rather than the 777560/60
	terminal.  Also, single step and multiple breaks work properly,
	thanks to Ralph pointing me in the right direction while chasing
	that one.

	If it wasn't for Loadable XDT's APR 6 "blind spot", it would be
	operationally indistinguishable from the resident one.

