 AFTER PROGRAM
	PROGRAM TO CONNECT TO A RUNNING TASK
	THEN SPAWN A COMMAND LINE OR LINES TO MCR
 
  COMMAND SYNTAX:
	>AFTer tsknam command line
		or
	>AFT tsknam&cmdline1&cmdline2&...
		or
	>AFT &cmdline1&cmdlin2&...
	WHERE:
		tsknam  - is the installed name of task to wait for
		&  - indicates that AFT must wait for MCR spawned task to exit
		&  - also separates multiple commands to MCR
  NOTE:
	If any task exits with an error code > 1 then AFT will exit with
	that status.
 
  OUTPUT:
	ON ERROR SPAWN EPRINT TASK
	EXIT STATUS - 4 IF ERROR
			ELSE EXIT STATUS OF TASK OR MCR
