*********************************************************************
*                                                                   *
* README.XMT            XMITR PROGRAM                               *
*                                                                   *
* ORIGINAL AUTHOR    Michael D. Lampi                               *
*                    McDonnell Douglas Corporation                  *
*                                                                   *
* CONTRIBUTOR        Glenn EVerhart                                 *
*                    Jeff Hamilton                                  *
*********************************************************************

XMTBLD.CMD		Command file to assemble & task build XMT
                        @XMTBLD  (or @XMTBLD LIST)
			(to modify a module, edit it, delete obj and
			@XMTBLD again; only not found obj are remade)
ABREAK.FTN
ASCII8.FTN
BREAK.FTN
CLSFIL.FTN
COPYMD.FTN
CTLCHR.FTN
CTLSUB.FTN
DELAY.FTN
DIAL.FTN
ECHO.FTN
ENQUE.FTN
FORMAT.FTN
HELP.FTN
INPFIL.FTN
OPNGET.FTN
OPNPUT.FTN
OUTFIL.FTN
PROMPT.FTN
READST.FTN
REDEF.FTN
SETUP.FTN
STATUS.FTN
STOPIT.FTN
XMITR.FTN
GETSQ.MAC		(Just as written in the FORTRAN-IV User's Guide)
ICNT.MAC

	The following MACRO-11 subroutines may have to be tailored
	to correspond to your respective systems.

ITTOUR.MAC
TTYOUT.MAC
TWAIT.MAC

	For a bit more background, this program was originally designed
	to run in an RT-11 environment using DL-11W's for communication.
	It was then transported over to RSX-11M 3.1 using DZ-11's and
	212 modems. No loss of information was found at speeds of 300
	baud when talking with ANY system, but PDP-11/70's were able
	to out-talk our poor 11/34 at 1200 baud and cause us to lose
	information, but usually only when XMT was checkpointed for
	extended lenghts of time. Under RSX-11M v3.2 a few features
	were added to the ITTOUR.MAC and INPTT1.MAC subroutines to make
	use of a few v3.2 TT: driver features, such as full-duplex
	and 8-bit characters. This program has been successful in
	receiving and transmitting at rates up to 4800 baud on an
	11/34 system (under v3.1) with no data loss. Under v3.2
	there should be no loss of data at any speed.

	(JLH) Made flags permenant feature to reduce CPU overhread.
	(JLH) Added auto-dial of HAYES SMARTMODEM 300 (1200?)
	(JLH) Added ability to insert LFs for those systems which
	do not supply them.  
	(JLH) Restructored status reports.
	(JLH) Used for data transfers across DZ at 9600 to tek 8560
	and HP1000 with no data loss.
	(JLH) Redesigned build file.
