 
 DLY PROGRAM
	PROGRAM TO DELAY THEN SPAWN A COMMAND TO MCR
 
  COMMAND SYNTAX:
 
	>DLY nnnU,command
	>DLY nnnU
	>DLY nnnU command
 
	WHERE:
		nnn - is a deciamal number
		U - is the delay units (H,M,S,T) default is S
		    Hours,Minuts,Seconds,Ticks
		command - is optional command to mcr
