**********************************************************************
 
THIS UIC([100,3]) CONTAINS XQDRV UTILITY TASKS SOURCE CODE AND THE 
NECESSARY COMMAND FILES TO BUILD THEM. IF THEY ARE MOVED TO ANOTHER
UIC A FEW COMMAND FILES WILL HAVE TO BE EDITED TO CORRECT EMBEDDED
UIC'S.
 
**********************************************************************
 
THIS UIC CONTAINS FILE ACCESS AND DOWN LINE LOAD ROUTINES AS FOLLOWS;
 
LWT	LINE WATCHER TASK(RSX11M)
	PROCESSES CONNECT REQUESTS
		REMOTE FILE ACCESS
		DOWN LINE LOAD REQUESTS
	FLUSHES STALE PACKETS
	GET LOCAL SYSTEM TIME
	SET LOCAL SYSTEM TIME
	ECHO PACKETS FOR TESTING
	SEND/ACCEPT ID PACKETS
	GET ERROR STATISTICS
	GET AND CLEAR ERROR STATISTICS
	GET LINE STATUS
 
NWT	NODE LINE WATCHER TASK(RSX11S)
	FLUSHES STALE PACKETS
	GET LOCAL SYSTEM TIME
	SET LOCAL SYSTEM TIME
	ECHO PACKETS FOR TESTING
	SEND/ACCEPT ID PACKETS
	GET ERROR STATISTICS
	GET AND CLEAR ERROR STATISTICS
	GET LINE STATUS
 
NFC	NETWORK FILE COPY
	ALLOWS OPERATOR INTERACTIVE FILE TRANSFERS
	REMOTE FILE DELETE(NOT IMPLEMENTED YET)
	REMOTE DIRECTORY(NOT IMPLEMENTED YET)
 
RFA	REMOTE FILE ACCESS
	READS/WRITES FILES(BLOCK MODE)
	READS/WRITES FILE(SEQUENTIAL MODE NOT CHECHED OUT YET)
	DELETE FILE(NOT CHECKED OUT YET)
	DIRECTORY(NOT CHECKED OUT YET)
 
DLT	DOWN LINE LOAD TASK
	LOADS SPECIFIED NODE REQUESTED BY THE REMOTE NODE
 
BOOTQNA	PRIMARY LOADER RESIDES IN EPROM IN NODES TO BE DOWN
	LINE LOADED
 
FALODT	ODT/PRIMARY LOADER RESIDES IN EPROM ON FALCON BOARD
	ALLOWS NORMAL ODT FUNCTIONS PLUS ETHERNET DOWN LINE
	LOAD CAPIBILITY.
 
BOOEDT	DOWN LINE LOADER DATA BASE EDITOR TASK
 
PARSX	COMMAND LINE PARSER USED BY NFC
