

	The following utilities are provided by:

	Eddy Fey 
	Utah Power and Light
	Room 125-51
	P.O. Box 899
	Salt Lake City, Utah 84110
	801-535-2795

	2591 E. Grand View Drive
	Sandy, Utah 84092
	801-942-3185

	1.0	Task-to-task Communications and Flying Install Subsystem.

		1.1 RUNNER and INSREM
		    Set of programs used to send parameters to a task,
		    install the task, activate it and remove it upon exit.
		    This is a complete 'flying install' subsystem and will
		    work for permanently installed tasks as well (see RUNNER.DOC).

		1.2 SNDPRM and RCVPRM
		    Interface to RUNNER and INSREM for sending and receiving
		    parameters.

		1.3 VXDRV and VXUTIL
		    This is yet another re-write of the VSDRV by Osudar.
		    It provides mulitple units each capable of having 16kb 
		    of pool space. This will only work on RSX11M+ with I/D.

		1.4 PIPE
		    Interface to VXDRV QIO's for sending, receiving, creating
		    queues.

		1.5 SNDTST and RCVTST
		    Test programs for demonstration.

	2.0	CMB
		Compare binary. Compares two fixed length binary files for
		equality. Can be used for task images, data files, etc.

	3.0	WATCHER
		Nifty patch for finding executive space memory clobbers.

	4.0	IODUMP
		Dumps buffers in hex-ascii byte or word format.

	5.0	BUGMSG
		Prints debug messages only if lun 4 is not assigned to the NL:
		device (i.e. TT: or HT:).

	6.0	SYSMSG
		Prints messages on the system terminal device (ST0:).

	7.0	CDUMP
		Searches a binary CDA file for a given pattern.

