[273,54]	Telex (5-hole Baudot code) routines.

		A client uses these to prepare telexes with a
		PDP-11 then punch a telex tape. Ditto to read
		telex tapes into a computer. Our reader/punch
		is a TTY-33 with tape reader punch. We use a
		paper clip to narrow the reader/punch for 5-hole
		tape, since 33's are built for 8-hole tape.

TLR.C		Read a baudot tape.

TLP.C		Punch a baudot tape.

TLX.CMD		Set up a terminal for this

SHUTDOWN.CMD	Demo what mantra to feed RSX to let these programs work.
		This is what you say AFTER using telex programs.
		It tries to turn ASR33 back to a VDU terminal.

SHUTUP.CMD	Demo what mantra to feed RSX to let these programs work.
		This is what you say BEFORE using telex programs.
		It makes TT: driver happy.
