
		Caterpillar Inc. Submissions [370,210]

		Submitted by:	Rick Webster
				Caterpillar Inc.
				Factory Integration Div.
				Mail Stop AD235
				600 W. Washington St. 
				East Peoria, Il. 61630

				309-675-9662

VTL - Virtual Terminal Logger (Not to be confused with Robin Miller's
      VTL, Video Terminal List from previous tapes)

	VTL  is  a utility to allow a virtual terminal to be accessed
	from  an actual physical terminal. Any output directed to the
	virtual  terminal  will  be  displayed  on  the  user's  TI:.
	Optionally, the data can be logged to a file at the same time,
	creating an exact log of all the data that appears on the
	screen during the interactive terminal session. 

	Note that this is for RSX11M+ only and has been tested on
	both V2.1 and V3.0.

	Files:	VTL.MAC		Source code
		VTLON.MAC	Program to re-attach to VTL after
				a detach from VTL
		VTL.RNO		User's Guide
		VTLBLD.CMD	Build command file

BYEBRK - Task to implement automatic disconnect from Micom port
	 on user log out.

	BYEBRK and companion task CSRFND can be used to send a
	BREAK to a port when a user logs out. This will cause
	an automatic disconnect on a properly configured Micom
	port selector.

	This has been tested on RSX11M+ V2.1 and V3.0 and although
	not tested, it should also work on RSX11M V4.0 and beyond.

	Files:	BYEBRK.MAC	Source to BYEBRK
		CSRFND.MAC	Source to CSRFND
		BYEBRKBLD.CMD	Command file to build BYEBRK
				and CSRFND
		SYSLOGOUT.CMD	Sample system log out command file
				to implement BYEBRK
		BYEBRK.RNO	User's Guide

