This UIC contains the files required to manufacture a Read-only ACP for
ODS-2 file structures. The sources are made from the V3.0 RSX-11M+ kit.

To build the ACP;
	Place the original SYSGEN sources on a volume.
	Copy  the files in this UIC to a new directory at [13,14] on that 
volume.

	Execute @slipper. This makes the new macro sources in this uic from the
sources in [13,10].

	Execute @doall. The UIC of [13,24], [13,34], [1,54] are required on the
volume. The RSXMC.MAC is required in LB:[11,10] and the EXEMC.MLB are required 
on LB:[1,1]. If you link in the debugger, the debugger will start at the first 
call to the ACP. i.e. 'Mount du:/ove/show' will produce the first break. Just do 
a go and the ACP is off and running. The ACP is not overlaid so the address are  
correct for a debug set-up.

	If you make a change to the sources, a command file called onefile
will reassemble it for you.

	In [350,125] I have added a directory routine to use a modified PIP.
With this PIP you can do directorys and copy files. The full file directory 
string has to be used. You must call out the full file string for it to work 
correctly. PIP clobbers the default directory string for partial file strings.

	Any Questions?

		Dan L. Eisner
		Perkin-Elmer Corporation
		7421 Orangewood Avenue
		Garden Grove, California
